# CUpti_ActivityUnifiedMemoryCounter Struct Reference
[CUPTI Activity API]

The activity record for Unified Memory counters (deprecated in CUDA 7.0). More...

## Data Fields
CUpti_ActivityUnifiedMemoryCounterKind | counterKind
uint32_t | deviceId
CUpti_ActivityKind | kind
uint32_t | pad
uint32_t | processId
CUpti_ActivityUnifiedMemoryCounterScope | scope
uint64_t | timestamp
uint64_t | value

## Detailed Description

This activity record represents a Unified Memory counter (CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER).

## Field Documentation

CUpti_ActivityUnifiedMemoryCounterKind CUpti_ActivityUnifiedMemoryCounter::counterKind

The Unified Memory counter kind. See CUpti_ActivityUnifiedMemoryCounterKind

uint32_t CUpti_ActivityUnifiedMemoryCounter::deviceId

The ID of the device involved in the memory transfer operation. It is not relevant if the scope of the counter is global (all devices).

CUpti_ActivityKind CUpti_ActivityUnifiedMemoryCounter::kind

The activity record kind, must be CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER

uint32_t CUpti_ActivityUnifiedMemoryCounter::pad

Undefined. Reserved for internal use.

uint32_t CUpti_ActivityUnifiedMemoryCounter::processId

The ID of the process to which this record belongs to. In case of global scope, processId is undefined.

CUpti_ActivityUnifiedMemoryCounterScope CUpti_ActivityUnifiedMemoryCounter::scope

Scope of the Unified Memory counter. See CUpti_ActivityUnifiedMemoryCounterScope

uint64_t CUpti_ActivityUnifiedMemoryCounter::timestamp

The timestamp when this sample was retrieved, in ns. A value of 0 indicates that timestamp information could not be collected

uint64_t CUpti_ActivityUnifiedMemoryCounter::value

Value of the counter