-->
CUPTI (PDF) - v11.7 (older) - Last updated May 03, 2022 - Send Feedback -

## 5. Modules

Here is a list of all modules:

- CUPTI Result Codes
- CUPTI Version
- CUPTI Activity API
- CUPTI Callback API
- CUPTI Event API
- CUPTI Metric API
- CUPTI Profiling API
- CUPTI Checkpoint API
- CUPTI PC Sampling API
- CUPTI PC Sampling Utility API

### 5.1. CUPTI Result Codes

Error and result codes returned by CUPTI functions.

#### Enumerations

enum CUptiResult
  CUPTI result codes.

#### Functions

CUptiResult cuptiGetResultString ( CUptiResult result, const char** str )
  Get the descriptive string for a CUptiResult.

#### Enumerations

enum CUptiResult

  Error and result codes returned by CUPTI functions.

  ###### Values

  CUPTI_SUCCESS = 0
    No error.
  CUPTI_ERROR_INVALID_PARAMETER = 1
    One or more of the parameters is invalid.
  CUPTI_ERROR_INVALID_DEVICE = 2
    The device does not correspond to a valid CUDA device.
  CUPTI_ERROR_INVALID_CONTEXT = 3
    The context is NULL or not valid.
  CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID = 4
    The event domain id is invalid.
  CUPTI_ERROR_INVALID_EVENT_ID = 5
    The event id is invalid.
  CUPTI_ERROR_INVALID_EVENT_NAME = 6
    The event name is invalid.
  CUPTI_ERROR_INVALID_OPERATION = 7
    The current operation cannot be performed due to dependency on other factors.
  CUPTI_ERROR_OUT_OF_MEMORY = 8
    Unable to allocate enough memory to perform the requested operation.
  CUPTI_ERROR_HARDWARE = 9
    An error occurred on the performance monitoring hardware.
  CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT = 10
    The output buffer size is not sufficient to return all requested data.
  CUPTI_ERROR_API_NOT_IMPLEMENTED = 11
    API is not implemented.
  CUPTI_ERROR_MAX_LIMIT_REACHED = 12
    The maximum limit is reached.
  CUPTI_ERROR_NOT_READY = 13
    The object is not yet ready to perform the requested operation.
  CUPTI_ERROR_NOT_COMPATIBLE = 14
    The current operation is not compatible with the current state of the object
  CUPTI_ERROR_NOT_INITIALIZED = 15
    CUPTI is unable to initialize its connection to the CUDA driver.
  CUPTI_ERROR_INVALID_METRIC_ID = 16
    The metric id is invalid.
  CUPTI_ERROR_INVALID_METRIC_NAME = 17
    The metric name is invalid.
  CUPTI_ERROR_QUEUE_EMPTY = 18
    The queue is empty.
  CUPTI_ERROR_INVALID_HANDLE = 19
    Invalid handle (internal?).
  CUPTI_ERROR_INVALID_STREAM = 20
    Invalid stream.
  CUPTI_ERROR_INVALID_KIND = 21
    Invalid kind.
  CUPTI_ERROR_INVALID_EVENT_VALUE = 22
    Invalid event value.
  CUPTI_ERROR_DISABLED = 23
    CUPTI is disabled due to conflicts with other enabled profilers
  CUPTI_ERROR_INVALID_MODULE = 24
    Invalid module.
  CUPTI_ERROR_INVALID_METRIC_VALUE = 25
    Invalid metric value.
  CUPTI_ERROR_HARDWARE_BUSY = 26
    The performance monitoring hardware is in use by other client.
  CUPTI_ERROR_NOT_SUPPORTED = 27
    The attempted operation is not supported on the current system or device.
  CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED = 28
    Unified memory profiling is not supported on the system. Potential reason could be unsupported OS or architecture.
  CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_DEVICE = 29
    Unified memory profiling is not supported on the device
  CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_NON_P2P_DEVICES = 30
    Unified memory profiling is not supported on a multi-GPU configuration without P2P support between any pair of devices
  CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_WITH_MPS = 31
    Unified memory profiling is not supported under the Multi-Process Service (MPS) environment. CUDA 7.5 removes this restriction.
  CUPTI_ERROR_CDP_TRACING_NOT_SUPPORTED = 32
    In CUDA 9.0, devices with compute capability 7.0 don't support CDP tracing
  CUPTI_ERROR_VIRTUALIZED_DEVICE_NOT_SUPPORTED = 33
    Profiling on virtualized GPU is not supported.
  CUPTI_ERROR_CUDA_COMPILER_NOT_COMPATIBLE = 34
    Profiling results might be incorrect for CUDA applications compiled with nvcc version older than 9.0 for devices with compute capability 6.0 and 6.1. Profiling session will continue and CUPTI will notify it using this error code. User is advised to recompile the application code with nvcc version 9.0 or later. Ignore this warning if code is already compiled with the recommended nvcc version.
  CUPTI_ERROR_INSUFFICIENT_PRIVILEGES = 35
    User doesn't have sufficient privileges which are required to start the profiling session. One possible reason for this may be that the NVIDIA driver or your system administrator may have restricted access to the NVIDIA GPU performance counters. To learn how to resolve this issue and find more information, please visit https://developer.nvidia.com/CUPTI_ERROR_INSUFFICIENT_PRIVILEGES
  CUPTI_ERROR_OLD_PROFILER_API_INITIALIZED = 36
    Legacy CUPTI Profiling API i.e. event API from the header cupti_events.h and metric API from the header cupti_metrics.h are not compatible with the Profiling API in the header cupti_profiler_target.h and Perfworks metrics API in the headers nvperf_host.h and nvperf_target.h.
  CUPTI_ERROR_OPENACC_UNDEFINED_ROUTINE = 37
    Missing definition of the OpenACC API routine in the linked OpenACC library.One possible reason is that OpenACC library is linked statically in the user application, which might not have the definition of all the OpenACC API routines needed for the OpenACC profiling, as compiler might ignore definitions for the functions not used in the application. This issue can be mitigated by linking the OpenACC library dynamically.
  CUPTI_ERROR_LEGACY_PROFILER_NOT_SUPPORTED = 38
    Legacy CUPTI Profiling API i.e. event API from the header cupti_events.h and metric API from the header cupti_metrics.h are not supported on devices with compute capability 7.5 and higher (i.e. Turing and later GPU architectures). These API will be deprecated in a future CUDA release. These are replaced by Profiling API in the header cupti_profiler_target.h and Perfworks metrics API in the headers nvperf_host.h and nvperf_target.h.
  CUPTI_ERROR_MULTIPLE_SUBSCRIBERS_NOT_SUPPORTED = 39
    CUPTI doesn't allow multiple callback subscribers. Only a single subscriber can be registered at a time. Same error code is used when application is launched using NVIDIA tools like nvprof, Visual Profiler, Nsight Systems, Nsight Compute, cuda-gdb and cuda-memcheck.
  CUPTI_ERROR_VIRTUALIZED_DEVICE_INSUFFICIENT_PRIVILEGES = 40
    Profiling on virtualized GPU is not allowed by hypervisor.
  CUPTI_ERROR_CONFIDENTIAL_COMPUTING_NOT_SUPPORTED = 41
    Profiling and tracing are not allowed when confidential computing mode is enabled.
  CUPTI_ERROR_CMP_DEVICE_NOT_SUPPORTED = 42
    CUPTI does not support NVIDIA Crypto Mining Processors (CMP). For more information, please visit https://developer.nvidia.com/ERR_NVCMPGPU
  CUPTI_ERROR_UNKNOWN = 999
    An unknown internal error has occurred.
  CUPTI_ERROR_FORCE_INT = 0x7fffffff

#### Functions

CUptiResult cuptiGetResultString ( CUptiResult result, const char** str )
  Get the descriptive string for a CUptiResult.

  ###### Parameters

  `result`
    The result to get the string for
  `str`
    Returns the string

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_INVALID_PARAMETER

    if `str` is NULL or `result` is not a valid CUptiResult

  ###### Description

  Return the descriptive string for a CUptiResult in `*str`.

  Note:

  Thread-safety: this function is thread safe.

### 5.2. CUPTI Version

Function and macro to determine the CUPTI version.

#### Defines

#define CUPTI_API_VERSION 17
  The API version for this implementation of CUPTI.

#### Functions

CUptiResult cuptiGetVersion ( uint32_t* version )
  Get the CUPTI API version.

#### Defines

#define CUPTI_API_VERSION 17

  The API version for this implementation of CUPTI. This define along with cuptiGetVersion can be used to dynamically detect if the version of CUPTI compiled against matches the version of the loaded CUPTI library.

  v1 : CUDAToolsSDK 4.0 v2 : CUDAToolsSDK 4.1 v3 : CUDA Toolkit 5.0 v4 : CUDA Toolkit 5.5 v5 : CUDA Toolkit 6.0 v6 : CUDA Toolkit 6.5 v7 : CUDA Toolkit 6.5(with sm_52 support) v8 : CUDA Toolkit 7.0 v9 : CUDA Toolkit 8.0 v10 : CUDA Toolkit 9.0 v11 : CUDA Toolkit 9.1 v12 : CUDA Toolkit 10.0, 10.1 and 10.2 v13 : CUDA Toolkit 11.0 v14 : CUDA Toolkit 11.1 v15 : CUDA Toolkit 11.2, 11.3 and 11.4 v16 : CUDA Toolkit 11.5 v17 : CUDA Toolkit 11.6

#### Functions

CUptiResult cuptiGetVersion ( uint32_t* version )
  Get the CUPTI API version.

  ###### Parameters

  `version`
    Returns the version

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_INVALID_PARAMETER

    if `version` is NULL

  ###### Description

  Return the API version in `*version`.

  See also:

  CUPTI_API_VERSION

### 5.3. CUPTI Activity API

Functions, types, and enums that implement the CUPTI Activity API.

#### Classes

struct
CUpti_Activity
  The base activity record.
struct
CUpti_ActivityAPI
  The activity record for a driver or runtime API invocation.
struct
CUpti_ActivityAutoBoostState
  Device auto boost state structure.
struct
CUpti_ActivityBranch
  The activity record for source level result branch. (deprecated).
struct
CUpti_ActivityBranch2
  The activity record for source level result branch.
struct
CUpti_ActivityCdpKernel
  The activity record for CDP (CUDA Dynamic Parallelism) kernel.
struct
CUpti_ActivityContext
  The activity record for a context.
struct
CUpti_ActivityCudaEvent
  The activity record for CUDA event.
struct
CUpti_ActivityDevice
  The activity record for a device. (deprecated).
struct
CUpti_ActivityDevice2
  The activity record for a device. (deprecated).
struct
CUpti_ActivityDevice3
  The activity record for a device. (CUDA 7.0 onwards).
struct
CUpti_ActivityDevice4
  The activity record for a device. (CUDA 11.6 onwards).
struct
CUpti_ActivityDeviceAttribute
  The activity record for a device attribute.
struct
CUpti_ActivityEnvironment
  The activity record for CUPTI environmental data.
struct
CUpti_ActivityEvent
  The activity record for a CUPTI event.
struct
CUpti_ActivityEventInstance
  The activity record for a CUPTI event with instance information.
struct
CUpti_ActivityExternalCorrelation
  The activity record for correlation with external records.
struct
CUpti_ActivityFunction
  The activity record for global/device functions.
struct
CUpti_ActivityGlobalAccess
  The activity record for source-level global access. (deprecated).
struct
CUpti_ActivityGlobalAccess2
  The activity record for source-level global access. (deprecated in CUDA 9.0).
struct
CUpti_ActivityGlobalAccess3
  The activity record for source-level global access.
struct
CUpti_ActivityGraphTrace
  The activity record for trace of graph execution.
struct
CUpti_ActivityInstantaneousEvent
  The activity record for an instantaneous CUPTI event.
struct
CUpti_ActivityInstantaneousEventInstance
  The activity record for an instantaneous CUPTI event with event domain instance information.
struct
CUpti_ActivityInstantaneousMetric
  The activity record for an instantaneous CUPTI metric.
struct
CUpti_ActivityInstantaneousMetricInstance
  The instantaneous activity record for a CUPTI metric with instance information.
struct
CUpti_ActivityInstructionCorrelation
  The activity record for source-level sass/source line-by-line correlation.
struct
CUpti_ActivityInstructionExecution
  The activity record for source-level instruction execution.
struct
CUpti_ActivityKernel
  The activity record for kernel. (deprecated).
struct
CUpti_ActivityKernel2
  The activity record for kernel. (deprecated).
struct
CUpti_ActivityKernel3
  The activity record for a kernel (CUDA 6.5(with sm_52 support) onwards). (deprecated in CUDA 9.0).
struct
CUpti_ActivityKernel4
  The activity record for a kernel (CUDA 9.0(with sm_70 support) onwards). (deprecated in CUDA 11.0).
struct
CUpti_ActivityKernel5
  The activity record for a kernel (CUDA 11.0(with sm_80 support) onwards). (deprecated in CUDA 11.2) This activity record represents a kernel execution (CUPTI_ACTIVITY_KIND_KERNEL and CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL) but is no longer generated by CUPTI. Kernel activities are now reported using the CUpti_ActivityKernel7 activity record.
struct
CUpti_ActivityKernel6
  The activity record for kernel. (deprecated in CUDA 11.6).
struct
CUpti_ActivityKernel7
  The activity record for kernel.
struct
CUpti_ActivityMarker
  The activity record providing a marker which is an instantaneous point in time. (deprecated in CUDA 8.0).
struct
CUpti_ActivityMarker2
  The activity record providing a marker which is an instantaneous point in time.
struct
CUpti_ActivityMarkerData
  The activity record providing detailed information for a marker.
struct
CUpti_ActivityMemcpy
  The activity record for memory copies. (deprecated).
struct
CUpti_ActivityMemcpy3
  The activity record for memory copies. (deprecated in CUDA 11.1).
struct
CUpti_ActivityMemcpy4
  The activity record for memory copies. (deprecated in CUDA 11.6).
struct
CUpti_ActivityMemcpy5
  The activity record for memory copies.
struct
CUpti_ActivityMemcpyPtoP
  The activity record for peer-to-peer memory copies.
struct
CUpti_ActivityMemcpyPtoP2
  The activity record for peer-to-peer memory copies. (deprecated in CUDA 11.1).
struct
CUpti_ActivityMemcpyPtoP3
  The activity record for peer-to-peer memory copies. (deprecated in CUDA 11.6).
struct
CUpti_ActivityMemcpyPtoP4
  The activity record for peer-to-peer memory copies.
struct
CUpti_ActivityMemory
  The activity record for memory.
struct
CUpti_ActivityMemory2
  The activity record for memory.
struct
CUpti_ActivityMemory3
  The activity record for memory.
struct
CUpti_ActivityMemoryPool
  The activity record for memory pool.
struct
CUpti_ActivityMemoryPool2
  The activity record for memory pool.
struct
CUpti_ActivityMemset
  The activity record for memset. (deprecated).
struct
CUpti_ActivityMemset2
  The activity record for memset. (deprecated in CUDA 11.1).
struct
CUpti_ActivityMemset3
  The activity record for memset. (deprecated in CUDA 11.6).
struct
CUpti_ActivityMemset4
  The activity record for memset.
struct
CUpti_ActivityMetric
  The activity record for a CUPTI metric.
struct
CUpti_ActivityMetricInstance
  The activity record for a CUPTI metric with instance information.
struct
CUpti_ActivityModule
  The activity record for a CUDA module.
struct
CUpti_ActivityName
  The activity record providing a name.
struct
CUpti_ActivityNvLink
  NVLink information. (deprecated in CUDA 9.0).
struct
CUpti_ActivityNvLink2
  NVLink information. (deprecated in CUDA 10.0).
struct
CUpti_ActivityNvLink3
  NVLink information.
struct
CUpti_ActivityNvLink4
  NVLink information.
union
CUpti_ActivityObjectKindId
  Identifiers for object kinds as specified by CUpti_ActivityObjectKind.
struct
CUpti_ActivityOpenAcc
  The base activity record for OpenAcc records.
struct
CUpti_ActivityOpenAccData
  The activity record for OpenACC data.
struct
CUpti_ActivityOpenAccLaunch
  The activity record for OpenACC launch.
struct
CUpti_ActivityOpenAccOther
  The activity record for OpenACC other.
struct
CUpti_ActivityOpenMp
  The base activity record for OpenMp records.
struct
CUpti_ActivityOverhead
  The activity record for CUPTI and driver overheads.
struct
CUpti_ActivityPCSampling
  The activity record for PC sampling. (deprecated in CUDA 8.0).
struct
CUpti_ActivityPCSampling2
  The activity record for PC sampling. (deprecated in CUDA 9.0).
struct
CUpti_ActivityPCSampling3
  The activity record for PC sampling.
struct
CUpti_ActivityPCSamplingConfig
  PC sampling configuration structure.
struct
CUpti_ActivityPCSamplingRecordInfo
  The activity record for record status for PC sampling.
struct
CUpti_ActivityPcie
  PCI devices information required to construct topology.
struct
CUpti_ActivityPreemption
  The activity record for a preemption of a CDP kernel.
struct
CUpti_ActivitySharedAccess
  The activity record for source-level shared access.
struct
CUpti_ActivitySourceLocator
  The activity record for source locator.
struct
CUpti_ActivityStream
  The activity record for CUDA stream.
struct
CUpti_ActivitySynchronization
  The activity record for synchronization management.
struct
CUpti_ActivityUnifiedMemoryCounter
  The activity record for Unified Memory counters (deprecated in CUDA 7.0).
struct
CUpti_ActivityUnifiedMemoryCounter2
  The activity record for Unified Memory counters (CUDA 7.0 and beyond).
struct
CUpti_ActivityUnifiedMemoryCounterConfig
  Unified Memory counters configuration structure.

#### Defines

#define CUPTI_AUTO_BOOST_INVALID_CLIENT_PID 0
#define CUPTI_CORRELATION_ID_UNKNOWN 0
#define CUPTI_FUNCTION_INDEX_ID_INVALID 0
#define CUPTI_GRID_ID_UNKNOWN 0LL
#define CUPTI_MAX_NVLINK_PORTS 32
#define CUPTI_NVLINK_INVALID_PORT -1
#define CUPTI_SOURCE_LOCATOR_ID_UNKNOWN 0
#define CUPTI_SYNCHRONIZATION_INVALID_VALUE -1
#define CUPTI_TIMESTAMP_UNKNOWN 0LL

#### Typedefs

typedef void ( *CUpti_BuffersCallbackCompleteFunc )( CUcontext context, uint32_t streamId, uint8_t* buffer, size_t size, size_t validSize )
  Function type for callback used by CUPTI to return a buffer of activity records.
typedef void ( *CUpti_BuffersCallbackRequestFunc )( uint8_t* *buffer, size_t* size, size_t* maxNumRecords )
  Function type for callback used by CUPTI to request an empty buffer for storing activity records.
typedef uint64_t( ( *CUpti_TimestampCallbackFunc )( )
  Function type for callback used by CUPTI to request a timestamp to be used in activity records.

#### Enumerations

enum CUpti_ActivityAttribute
  Activity attributes.
enum CUpti_ActivityComputeApiKind
  The kind of a compute API.
enum CUpti_ActivityEnvironmentKind
  The kind of environment data. Used to indicate what type of data is being reported by an environment activity record.
enum CUpti_ActivityFlag
  Flags associated with activity records.
enum CUpti_ActivityInstructionClass
  SASS instruction classification.
enum CUpti_ActivityKind
  The kinds of activity records.
enum CUpti_ActivityLaunchType
  The type of the CUDA kernel launch.
enum CUpti_ActivityMemcpyKind
  The kind of a memory copy, indicating the source and destination targets of the copy.
enum CUpti_ActivityMemoryKind
  The kinds of memory accessed by a memory operation/copy.
enum CUpti_ActivityMemoryOperationType
  Memory operation types.
enum CUpti_ActivityMemoryPoolOperationType
  Memory pool operation types.
enum CUpti_ActivityMemoryPoolType
  Memory pool types.
enum CUpti_ActivityObjectKind
  The kinds of activity objects.
enum CUpti_ActivityOverheadKind
  The kinds of activity overhead.
enum CUpti_ActivityPCSamplingPeriod
  Sampling period for PC sampling method.
enum CUpti_ActivityPCSamplingStallReason
  The stall reason for PC sampling activity.
enum CUpti_ActivityPartitionedGlobalCacheConfig
  Partitioned global caching option.
enum CUpti_ActivityPreemptionKind
  The kind of a preemption activity.
enum CUpti_ActivityStreamFlag
  stream type.
enum CUpti_ActivitySynchronizationType
  Synchronization type.
enum CUpti_ActivityThreadIdType
  Thread-Id types.
enum CUpti_ActivityUnifiedMemoryAccessType
  Memory access type for unified memory page faults.
enum CUpti_ActivityUnifiedMemoryCounterKind
  Kind of the Unified Memory counter.
enum CUpti_ActivityUnifiedMemoryCounterScope
  Scope of the unified memory counter (deprecated in CUDA 7.0).
enum CUpti_ActivityUnifiedMemoryMigrationCause
  Migration cause of the Unified Memory counter.
enum CUpti_ActivityUnifiedMemoryRemoteMapCause
  Remote memory map cause of the Unified Memory counter.
enum CUpti_DevType
  The device type for device connected to NVLink.
enum CUpti_DeviceVirtualizationMode
enum CUpti_EnvironmentClocksThrottleReason
  Reasons for clock throttling.
enum CUpti_ExternalCorrelationKind
  The kind of external APIs supported for correlation.
enum CUpti_FuncShmemLimitConfig
  The shared memory limit per block config for a kernel This should be used to set 'cudaOccFuncShmemConfig' field in occupancy calculator API.
enum CUpti_LinkFlag
  Link flags.
enum CUpti_OpenAccConstructKind
  The OpenAcc parent construct kind for OpenAcc activity records.
enum CUpti_OpenAccEventKind
  The OpenAcc event kind for OpenAcc activity records.
enum CUpti_PcieDeviceType
enum CUpti_PcieGen
  PCIE Generation.

#### Functions

CUptiResult cuptiActivityConfigurePCSampling ( CUcontext ctx, CUpti_ActivityPCSamplingConfig* config )
  Set PC sampling configuration.
CUptiResult cuptiActivityConfigureUnifiedMemoryCounter ( CUpti_ActivityUnifiedMemoryCounterConfig* config, uint32_t count )
  Set Unified Memory Counter configuration.
CUptiResult cuptiActivityDisable ( CUpti_ActivityKind kind )
  Disable collection of a specific kind of activity record.
CUptiResult cuptiActivityDisableContext ( CUcontext context, CUpti_ActivityKind kind )
  Disable collection of a specific kind of activity record for a context.
CUptiResult cuptiActivityEnable ( CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record.
CUptiResult cuptiActivityEnableAndDump ( CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record. For certain activity kinds it dumps existing records.
CUptiResult cuptiActivityEnableContext ( CUcontext context, CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record for a context.
CUptiResult cuptiActivityEnableLatencyTimestamps ( uint8_t enable )
  Controls the collection of queued and submitted timestamps for kernels.
CUptiResult cuptiActivityEnableLaunchAttributes ( uint8_t enable )
  Controls the collection of launch attributes for kernels.
CUptiResult cuptiActivityFlush ( CUcontext context, uint32_t streamId, uint32_t flag )
  Wait for all activity records to be delivered via the completion callback.
CUptiResult cuptiActivityFlushAll ( uint32_t flag )
  Request to deliver activity records via the buffer completion callback.
CUptiResult cuptiActivityFlushPeriod ( uint32_t time )
  Sets the flush period for the worker thread.
CUptiResult cuptiActivityGetAttribute ( CUpti_ActivityAttribute attr, size_t* valueSize, void* value )
  Read an activity API attribute.
CUptiResult cuptiActivityGetNextRecord ( uint8_t* buffer, size_t validBufferSizeBytes, CUpti_Activity** record )
  Iterate over the activity records in a buffer.
CUptiResult cuptiActivityGetNumDroppedRecords ( CUcontext context, uint32_t streamId, size_t* dropped )
  Get the number of activity records that were dropped of insufficient buffer space.
CUptiResult cuptiActivityPopExternalCorrelationId ( CUpti_ExternalCorrelationKind kind, uint64_t* lastId )
  Pop an external correlation id for the calling thread.
CUptiResult cuptiActivityPushExternalCorrelationId ( CUpti_ExternalCorrelationKind kind, uint64_t id )
  Push an external correlation id for the calling thread.
CUptiResult cuptiActivityRegisterCallbacks ( CUpti_BuffersCallbackRequestFunc funcBufferRequested, CUpti_BuffersCallbackCompleteFunc funcBufferCompleted )
  Registers callback functions with CUPTI for activity buffer handling.
CUptiResult cuptiActivityRegisterTimestampCallback ( CUpti_TimestampCallbackFunc funcTimestamp )
  Registers callback function with CUPTI for providing timestamp.
CUptiResult cuptiActivitySetAttribute ( CUpti_ActivityAttribute attr, size_t* valueSize, void* value )
  Write an activity API attribute.
CUptiResult cuptiComputeCapabilitySupported ( int major, int minor, int* support )
  Check support for a compute capability.
CUptiResult cuptiDeviceSupported ( CUdevice dev, int* support )
  Check support for a compute device.
CUptiResult cuptiDeviceVirtualizationMode ( CUdevice dev, CUpti_DeviceVirtualizationMode* mode )
  Query the virtualization mode of the device.
CUptiResult cuptiFinalize ( void )
  Detach CUPTI from the running process.
CUptiResult cuptiGetAutoBoostState ( CUcontext context, CUpti_ActivityAutoBoostState* state )
  Get auto boost state.
CUptiResult cuptiGetContextId ( CUcontext context, uint32_t* contextId )
  Get the ID of a context.
CUptiResult cuptiGetDeviceId ( CUcontext context, uint32_t* deviceId )
  Get the ID of a device.
CUptiResult cuptiGetGraphId ( CUgraph graph, uint32_t* pId )
  Get the unique ID of graph.
CUptiResult cuptiGetGraphNodeId ( CUgraphNode node, uint64_t* nodeId )
  Get the unique ID of a graph node.
CUptiResult cuptiGetLastError ( void )
  Returns the last error from a cupti call or callback.
CUptiResult cuptiGetStreamId ( CUcontext context, CUstream stream, uint32_t* streamId )
  Get the ID of a stream.
CUptiResult cuptiGetStreamIdEx ( CUcontext context, CUstream stream, uint8_t perThreadStream, uint32_t* streamId )
  Get the ID of a stream.
CUptiResult cuptiGetThreadIdType ( CUpti_ActivityThreadIdType* type )
  Get the thread-id type.
CUptiResult cuptiGetTimestamp ( uint64_t* timestamp )
  Get the CUPTI timestamp.
CUptiResult cuptiSetThreadIdType ( CUpti_ActivityThreadIdType type )
  Set the thread-id type.

#### Defines

#define CUPTI_AUTO_BOOST_INVALID_CLIENT_PID 0

  An invalid/unknown process id.

#define CUPTI_CORRELATION_ID_UNKNOWN 0

  An invalid/unknown correlation ID. A correlation ID of this value indicates that there is no correlation for the activity record.

#define CUPTI_FUNCTION_INDEX_ID_INVALID 0

  An invalid function index ID.

#define CUPTI_GRID_ID_UNKNOWN 0LL

  An invalid/unknown grid ID.

#define CUPTI_MAX_NVLINK_PORTS 32

  Maximum NVLink port numbers.

#define CUPTI_NVLINK_INVALID_PORT -1

  Invalid/unknown NVLink port number.

#define CUPTI_SOURCE_LOCATOR_ID_UNKNOWN 0

  The source-locator ID that indicates an unknown source location. There is not an actual CUpti_ActivitySourceLocator object corresponding to this value.

#define CUPTI_SYNCHRONIZATION_INVALID_VALUE -1

  An invalid/unknown value.

#define CUPTI_TIMESTAMP_UNKNOWN 0LL

  An invalid/unknown timestamp for a start, end, queued, submitted, or completed time.

#### Typedefs

void ( *CUpti_BuffersCallbackCompleteFunc )( CUcontext context, uint32_t streamId, uint8_t* buffer, size_t size, size_t validSize )

  Function type for callback used by CUPTI to return a buffer of activity records. This callback function returns to the CUPTI client a buffer containing activity records. The buffer contains `validSize` bytes of activity records which should be read using cuptiActivityGetNextRecord. The number of dropped records can be read using cuptiActivityGetNumDroppedRecords. After this call CUPTI relinquished ownership of the buffer and will not use it anymore. The client may return the buffer to CUPTI using the CUpti_BuffersCallbackRequestFunc callback. Note: CUDA 6.0 onwards, all buffers returned by this callback are global buffers i.e. there is no context/stream specific buffer. User needs to parse the global buffer to extract the context/stream specific activity records.

###### Parameters

`context`
  The context this buffer is associated with. If NULL, the buffer is associated with the global activities. This field is deprecated as of CUDA 6.0 and will always be NULL.
`uint32_t streamId`
`buffer`
  The activity record buffer.
`size_t size`
`size_t validSize`

void ( *CUpti_BuffersCallbackRequestFunc )( uint8_t* *buffer, size_t* size, size_t* maxNumRecords )

  Function type for callback used by CUPTI to request an empty buffer for storing activity records. This callback function signals the CUPTI client that an activity buffer is needed by CUPTI. The activity buffer is used by CUPTI to store activity records. The callback function can decline the request by setting `*buffer` to NULL. In this case CUPTI may drop activity records.

###### Parameters

`*buffer`
`size`
  Returns the size of the returned buffer.
`maxNumRecords`
  Returns the maximum number of records that should be placed in the buffer. If 0 then the buffer is filled with as many records as possible. If > 0 the buffer is filled with at most that many records before it is returned.

uint64_t( ( *CUpti_TimestampCallbackFunc )( )

  Function type for callback used by CUPTI to request a timestamp to be used in activity records. This callback function signals the CUPTI client that a timestamp needs to be returned. This timestamp would be treated as normalized timestamp to be used for various purposes in CUPTI. For example to store start and end timestamps reported in the CUPTI activity records. The returned timestamp must be in nanoseconds.

  See also:

  cuptiActivityRegisterTimestampCallback

#### Enumerations

enum CUpti_ActivityAttribute

  These attributes are used to control the behavior of the activity API.

  ###### Values

  CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE = 0
    The device memory size (in bytes) reserved for storing profiling data for concurrent kernels (activity kind CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL), memcopies and memsets for each buffer on a context. The value is a size_t.There is a limit on how many device buffers can be allocated per context. User can query and set this limit using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT. CUPTI doesn't pre-allocate all the buffers, it pre-allocates only those many buffers as set by the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE. When all of the data in a buffer is consumed, it is added in the reuse pool, and CUPTI picks a buffer from this pool when a new buffer is needed. Thus memory footprint does not scale with the kernel count. Applications with the high density of kernels, memcopies and memsets might result in having CUPTI to allocate more device buffers. CUPTI allocates another buffer only when it runs out of the buffers in the reuse pool.Since buffer allocation happens in the main application thread, this might result in stalls in the critical path. CUPTI pre-allocates 3 buffers of the same size to mitigate this issue. User can query and set the pre-allocation limit using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE.Having larger buffer size leaves less device memory for the application. Having smaller buffer size increases the risk of dropping timestamps for records if too many kernels or memcopies or memsets are launched at one time.This value only applies to new buffer allocations. Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.The default value is 3200000 (~3MB) which can accommodate profiling data up to 100,000 kernels, memcopies and memsets combined.Note: Starting with the CUDA 11.2 release, CUPTI allocates profiling buffer in the pinned host memory by default as this might help in improving the performance of the tracing run. Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_MEM_ALLOCATION_TYPE_HOST_PINNED for more details. Size of the memory and maximum number of pools are still controlled by the attributes CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE and CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT.Note: The actual amount of device memory per buffer reserved by CUPTI might be larger.
  CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE_CDP = 1
    The device memory size (in bytes) reserved for storing profiling data for CDP operations for each buffer on a context. The value is a size_t.Having larger buffer size means less flush operations but consumes more device memory. This value only applies to new allocations.Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.The default value is 8388608 (8MB).Note: The actual amount of device memory per context reserved by CUPTI might be larger.
  CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMIT = 2
    The maximum number of device memory buffers per context. The value is a size_t.For an application with high rate of kernel launches, memcopies and memsets having a bigger pool limit helps in timestamp collection for all these activties at the expense of a larger memory footprint. Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE for more details.Setting this value will not modify the number of memory buffers currently stored.Set this value before initializing CUDA to ensure the limit is not exceeded.The default value is 250.
  CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE = 3
    The profiling semaphore pool size reserved for storing profiling data for serialized kernels tracing (activity kind CUPTI_ACTIVITY_KIND_KERNEL) for each context. The value is a size_t.There is a limit on how many semaphore pools can be allocated per context. User can query and set this limit using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMIT. CUPTI doesn't pre-allocate all the semaphore pools, it pre-allocates only those many semaphore pools as set by the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE. When all of the data in a semaphore pool is consumed, it is added in the reuse pool, and CUPTI picks a semaphore pool from the reuse pool when a new semaphore pool is needed. Thus memory footprint does not scale with the kernel count. Applications with the high density of kernels might result in having CUPTI to allocate more semaphore pools. CUPTI allocates another semaphore pool only when it runs out of the semaphore pools in the reuse pool.Since semaphore pool allocation happens in the main application thread, this might result in stalls in the critical path. CUPTI pre-allocates 3 semaphore pools of the same size to mitigate this issue. User can query and set the pre-allocation limit using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE.Having larger semaphore pool size leaves less device memory for the application. Having smaller semaphore pool size increases the risk of dropping timestamps for kernel records if too many kernels are issued/launched at one time.This value only applies to new semaphore pool allocations. Set this value before initializing CUDA or before creating a context to ensure it is considered for the following allocations.The default value is 25000 which can accommodate profiling data for upto 25,000 kernels.
  CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMIT = 4
    The maximum number of profiling semaphore pools per context. The value is a size_t.For an application with high rate of kernel launches, having a bigger pool limit helps in timestamp collection for all the kernels, at the expense of a larger device memory footprint. Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE for more details.Set this value before initializing CUDA to ensure the limit is not exceeded.The default value is 250.
  CUPTI_ACTIVITY_ATTR_ZEROED_OUT_ACTIVITY_BUFFER = 5
    The flag to indicate whether user should provide activity buffer of zero value. The value is a uint8_t.If the value of this attribute is non-zero, user should provide a zero value buffer in the CUpti_BuffersCallbackRequestFunc. If the user does not provide a zero value buffer after setting this to non-zero, the activity buffer may contain some uninitialized values when CUPTI returns it in CUpti_BuffersCallbackCompleteFuncIf the value of this attribute is zero, CUPTI will initialize the user buffer received in the CUpti_BuffersCallbackRequestFunc to zero before filling it. If the user sets this to zero, a few stalls may appear in critical path because CUPTI will zero out the buffer in the main thread. Set this value before returning from CUpti_BuffersCallbackRequestFunc to ensure it is considered for all the subsequent user buffers.The default value is 0.
  CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE = 6
    Number of device buffers to pre-allocate for a context during the initialization phase. The value is a size_t.Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE for details.This value must be less than the maximum number of device buffers set using the attribute CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_POOL_LIMITSet this value before initializing CUDA or before creating a context to ensure it is considered by the CUPTI.The default value is set to 3 to ping pong between these buffers (if possible).
  CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_PRE_ALLOCATE_VALUE = 7
    Number of profiling semaphore pools to pre-allocate for a context during the initialization phase. The value is a size_t.Refer to the description of the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_SIZE for details.This value must be less than the maximum number of profiling semaphore pools set using the attribute CUPTI_ACTIVITY_ATTR_PROFILING_SEMAPHORE_POOL_LIMITSet this value before initializing CUDA or before creating a context to ensure it is considered by the CUPTI.The default value is set to 3 to ping pong between these pools (if possible).
  CUPTI_ACTIVITY_ATTR_MEM_ALLOCATION_TYPE_HOST_PINNED = 8
    Allocate page-locked (pinned) host memory for storing profiling data for concurrent kernels, memcopies and memsets for each buffer on a context. The value is a uint8_t.Starting with the CUDA 11.2 release, CUPTI allocates profiling buffer in the pinned host memory by default as this might help in improving the performance of the tracing run. Allocating excessive amounts of pinned memory may degrade system performance, since it reduces the amount of memory available to the system for paging. For this reason user might want to change the location from pinned host memory to device memory by setting value of this attribute to 0.The default value is 1.
  CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_FORCE_INT = 0x7fffffff
enum CUpti_ActivityComputeApiKind

  ###### Values

  CUPTI_ACTIVITY_COMPUTE_API_UNKNOWN = 0
    The compute API is not known.
  CUPTI_ACTIVITY_COMPUTE_API_CUDA = 1
    The compute APIs are for CUDA.
  CUPTI_ACTIVITY_COMPUTE_API_CUDA_MPS = 2
    The compute APIs are for CUDA running in MPS (Multi-Process Service) environment.
  CUPTI_ACTIVITY_COMPUTE_API_FORCE_INT = 0x7fffffff
enum CUpti_ActivityEnvironmentKind

  ###### Values

  CUPTI_ACTIVITY_ENVIRONMENT_UNKNOWN = 0
    Unknown data.
  CUPTI_ACTIVITY_ENVIRONMENT_SPEED = 1
    The environment data is related to speed.
  CUPTI_ACTIVITY_ENVIRONMENT_TEMPERATURE = 2
    The environment data is related to temperature.
  CUPTI_ACTIVITY_ENVIRONMENT_POWER = 3
    The environment data is related to power.
  CUPTI_ACTIVITY_ENVIRONMENT_COOLING = 4
    The environment data is related to cooling.
  CUPTI_ACTIVITY_ENVIRONMENT_COUNT
  CUPTI_ACTIVITY_ENVIRONMENT_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityFlag

  Activity record flags. Flags can be combined by bitwise OR to associated multiple flags with an activity record. Each flag is specific to a certain activity kind, as noted below.

  ###### Values

  CUPTI_ACTIVITY_FLAG_NONE = 0
    Indicates the activity record has no flags.
  CUPTI_ACTIVITY_FLAG_DEVICE_CONCURRENT_KERNELS = 1<<0
    Indicates the activity represents a device that supports concurrent kernel execution. Valid for CUPTI_ACTIVITY_KIND_DEVICE.
  CUPTI_ACTIVITY_FLAG_DEVICE_ATTRIBUTE_CUDEVICE = 1<<0
    Indicates if the activity represents a CUdevice_attribute value or a CUpti_DeviceAttribute value. Valid for CUPTI_ACTIVITY_KIND_DEVICE_ATTRIBUTE.
  CUPTI_ACTIVITY_FLAG_MEMCPY_ASYNC = 1<<0
    Indicates the activity represents an asynchronous memcpy operation. Valid for CUPTI_ACTIVITY_KIND_MEMCPY.
  CUPTI_ACTIVITY_FLAG_MARKER_INSTANTANEOUS = 1<<0
    Indicates the activity represents an instantaneous marker. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_START = 1<<1
    Indicates the activity represents a region start marker. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_END = 1<<2
    Indicates the activity represents a region end marker. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE = 1<<3
    Indicates the activity represents an attempt to acquire a user defined synchronization object. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE_SUCCESS = 1<<4
    Indicates the activity represents success in acquiring the user defined synchronization object. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_SYNC_ACQUIRE_FAILED = 1<<5
    Indicates the activity represents failure in acquiring the user defined synchronization object. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_SYNC_RELEASE = 1<<6
    Indicates the activity represents releasing a reservation on user defined synchronization object. Valid for CUPTI_ACTIVITY_KIND_MARKER.
  CUPTI_ACTIVITY_FLAG_MARKER_COLOR_NONE = 1<<0
    Indicates the activity represents a marker that does not specify a color. Valid for CUPTI_ACTIVITY_KIND_MARKER_DATA.
  CUPTI_ACTIVITY_FLAG_MARKER_COLOR_ARGB = 1<<1
    Indicates the activity represents a marker that specifies a color in alpha-red-green-blue format. Valid for CUPTI_ACTIVITY_KIND_MARKER_DATA.
  CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_SIZE_MASK = 0xFF<<0
    The number of bytes requested by each thread Valid for CUpti_ActivityGlobalAccess3.
  CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_LOAD = 1<<8
    If bit in this flag is set, the access was load, else it is a store access. Valid for CUpti_ActivityGlobalAccess3.
  CUPTI_ACTIVITY_FLAG_GLOBAL_ACCESS_KIND_CACHED = 1<<9
    If this bit in flag is set, the load access was cached else it is uncached. Valid for CUpti_ActivityGlobalAccess3.
  CUPTI_ACTIVITY_FLAG_METRIC_OVERFLOWED = 1<<0
    If this bit in flag is set, the metric value overflowed. Valid for CUpti_ActivityMetric and CUpti_ActivityMetricInstance.
  CUPTI_ACTIVITY_FLAG_METRIC_VALUE_INVALID = 1<<1
    If this bit in flag is set, the metric value couldn't be calculated. This occurs when a value(s) required to calculate the metric is missing. Valid for CUpti_ActivityMetric and CUpti_ActivityMetricInstance.
  CUPTI_ACTIVITY_FLAG_INSTRUCTION_VALUE_INVALID = 1<<0
    If this bit in flag is set, the source level metric value couldn't be calculated. This occurs when a value(s) required to calculate the source level metric cannot be evaluated. Valid for CUpti_ActivityInstructionExecution.
  CUPTI_ACTIVITY_FLAG_INSTRUCTION_CLASS_MASK = 0xFF<<1
    The mask for the instruction class, CUpti_ActivityInstructionClass Valid for CUpti_ActivityInstructionExecution and CUpti_ActivityInstructionCorrelation
  CUPTI_ACTIVITY_FLAG_FLUSH_FORCED = 1<<0
    When calling cuptiActivityFlushAll, this flag can be set to force CUPTI to flush all records in the buffer, whether finished or not
  CUPTI_ACTIVITY_FLAG_SHARED_ACCESS_KIND_SIZE_MASK = 0xFF<<0
    The number of bytes requested by each thread Valid for CUpti_ActivitySharedAccess.
  CUPTI_ACTIVITY_FLAG_SHARED_ACCESS_KIND_LOAD = 1<<8
    If bit in this flag is set, the access was load, else it is a store access. Valid for CUpti_ActivitySharedAccess.
  CUPTI_ACTIVITY_FLAG_MEMSET_ASYNC = 1<<0
    Indicates the activity represents an asynchronous memset operation. Valid for CUPTI_ACTIVITY_KIND_MEMSET.
  CUPTI_ACTIVITY_FLAG_THRASHING_IN_CPU = 1<<0
    Indicates the activity represents thrashing in CPU. Valid for counter of kind CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THRASHING in CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER
  CUPTI_ACTIVITY_FLAG_THROTTLING_IN_CPU = 1<<0
    Indicates the activity represents page throttling in CPU. Valid for counter of kind CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THROTTLING in CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER
  CUPTI_ACTIVITY_FLAG_FORCE_INT = 0x7fffffff
enum CUpti_ActivityInstructionClass

  The sass instruction are broadly divided into different class. Each enum represents a classification.

  ###### Values

  CUPTI_ACTIVITY_INSTRUCTION_CLASS_UNKNOWN = 0
    The instruction class is not known.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_32 = 1
    Represents a 32 bit floating point operation.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_64 = 2
    Represents a 64 bit floating point operation.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_INTEGER = 3
    Represents an integer operation.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_BIT_CONVERSION = 4
    Represents a bit conversion operation.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_CONTROL_FLOW = 5
    Represents a control flow instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_GLOBAL = 6
    Represents a global load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_SHARED = 7
    Represents a shared load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_LOCAL = 8
    Represents a local load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_GENERIC = 9
    Represents a generic load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_SURFACE = 10
    Represents a surface load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_CONSTANT = 11
    Represents a constant load instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_TEXTURE = 12
    Represents a texture load-store instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_GLOBAL_ATOMIC = 13
    Represents a global atomic instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_SHARED_ATOMIC = 14
    Represents a shared atomic instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_SURFACE_ATOMIC = 15
    Represents a surface atomic instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_INTER_THREAD_COMMUNICATION = 16
    Represents a inter-thread communication instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_BARRIER = 17
    Represents a barrier instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_MISCELLANEOUS = 18
    Represents some miscellaneous instructions which do not fit in the above classification.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_FP_16 = 19
    Represents a 16 bit floating point operation.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_UNIFORM = 20
    Represents uniform instruction.
  CUPTI_ACTIVITY_INSTRUCTION_CLASS_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityKind

  Each activity record kind represents information about a GPU or an activity occurring on a CPU or GPU. Each kind is associated with a activity record structure that holds the information associated with the kind.

  See also:

  CUpti_Activity

  CUpti_ActivityAPI

  CUpti_ActivityContext

  CUpti_ActivityDevice

  CUpti_ActivityDevice2

  CUpti_ActivityDevice3

  CUpti_ActivityDevice4

  CUpti_ActivityDeviceAttribute

  CUpti_ActivityEvent

  CUpti_ActivityEventInstance

  CUpti_ActivityKernel

  CUpti_ActivityKernel2

  CUpti_ActivityKernel3

  CUpti_ActivityKernel4

  CUpti_ActivityKernel5

  CUpti_ActivityKernel6

  CUpti_ActivityKernel7

  CUpti_ActivityCdpKernel

  CUpti_ActivityPreemption

  CUpti_ActivityMemcpy

  CUpti_ActivityMemcpy3

  CUpti_ActivityMemcpy4

  CUpti_ActivityMemcpy5

  CUpti_ActivityMemcpyPtoP

  CUpti_ActivityMemcpyPtoP2

  CUpti_ActivityMemcpyPtoP3

  CUpti_ActivityMemcpyPtoP4

  CUpti_ActivityMemset

  CUpti_ActivityMemset2

  CUpti_ActivityMemset3

  CUpti_ActivityMemset4

  CUpti_ActivityMetric

  CUpti_ActivityMetricInstance

  CUpti_ActivityName

  CUpti_ActivityMarker

  CUpti_ActivityMarker2

  CUpti_ActivityMarkerData

  CUpti_ActivitySourceLocator

  CUpti_ActivityGlobalAccess

  CUpti_ActivityGlobalAccess2

  CUpti_ActivityGlobalAccess3

  CUpti_ActivityBranch

  CUpti_ActivityBranch2

  CUpti_ActivityOverhead

  CUpti_ActivityEnvironment

  CUpti_ActivityInstructionExecution

  CUpti_ActivityUnifiedMemoryCounter

  CUpti_ActivityFunction

  CUpti_ActivityModule

  CUpti_ActivitySharedAccess

  CUpti_ActivityPCSampling

  CUpti_ActivityPCSampling2

  CUpti_ActivityPCSampling3

  CUpti_ActivityPCSamplingRecordInfo

  CUpti_ActivityCudaEvent

  CUpti_ActivityStream

  CUpti_ActivitySynchronization

  CUpti_ActivityInstructionCorrelation

  CUpti_ActivityExternalCorrelation

  CUpti_ActivityUnifiedMemoryCounter2

  CUpti_ActivityOpenAccData

  CUpti_ActivityOpenAccLaunch

  CUpti_ActivityOpenAccOther

  CUpti_ActivityOpenMp

  CUpti_ActivityNvLink

  CUpti_ActivityNvLink2

  CUpti_ActivityNvLink3

  CUpti_ActivityNvLink4

  CUpti_ActivityMemory

  CUpti_ActivityPcie

  ###### Values

  CUPTI_ACTIVITY_KIND_INVALID = 0
    The activity record is invalid.
  CUPTI_ACTIVITY_KIND_MEMCPY = 1
    A host<->host, host<->device, or device<->device memory copy. The corresponding activity record structure is CUpti_ActivityMemcpy5.
  CUPTI_ACTIVITY_KIND_MEMSET = 2
    A memory set executing on the GPU. The corresponding activity record structure is CUpti_ActivityMemset4.
  CUPTI_ACTIVITY_KIND_KERNEL = 3
    A kernel executing on the GPU. This activity kind may significantly change the overall performance characteristics of the application because all kernel executions are serialized on the GPU. Other activity kind for kernel CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL doesn't break kernel concurrency. The corresponding activity record structure is CUpti_ActivityKernel7.
  CUPTI_ACTIVITY_KIND_DRIVER = 4
    A CUDA driver API function execution. The corresponding activity record structure is CUpti_ActivityAPI.
  CUPTI_ACTIVITY_KIND_RUNTIME = 5
    A CUDA runtime API function execution. The corresponding activity record structure is CUpti_ActivityAPI.
  CUPTI_ACTIVITY_KIND_EVENT = 6
    An event value. The corresponding activity record structure is CUpti_ActivityEvent.
  CUPTI_ACTIVITY_KIND_METRIC = 7
    A metric value. The corresponding activity record structure is CUpti_ActivityMetric.
  CUPTI_ACTIVITY_KIND_DEVICE = 8
    Information about a device. The corresponding activity record structure is CUpti_ActivityDevice4.
  CUPTI_ACTIVITY_KIND_CONTEXT = 9
    Information about a context. The corresponding activity record structure is CUpti_ActivityContext.
  CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL = 10
    A kernel executing on the GPU. This activity kind doesn't break kernel concurrency. The corresponding activity record structure is CUpti_ActivityKernel7.
  CUPTI_ACTIVITY_KIND_NAME = 11
    Resource naming done via NVTX APIs for thread, device, context, etc. The corresponding activity record structure is CUpti_ActivityName.
  CUPTI_ACTIVITY_KIND_MARKER = 12
    Instantaneous, start, or end NVTX marker. The corresponding activity record structure is CUpti_ActivityMarker2.
  CUPTI_ACTIVITY_KIND_MARKER_DATA = 13
    Extended, optional, data about a marker. The corresponding activity record structure is CUpti_ActivityMarkerData.
  CUPTI_ACTIVITY_KIND_SOURCE_LOCATOR = 14
    Source information about source level result. The corresponding activity record structure is CUpti_ActivitySourceLocator.
  CUPTI_ACTIVITY_KIND_GLOBAL_ACCESS = 15
    Results for source-level global acccess. The corresponding activity record structure is CUpti_ActivityGlobalAccess3.
  CUPTI_ACTIVITY_KIND_BRANCH = 16
    Results for source-level branch. The corresponding activity record structure is CUpti_ActivityBranch2.
  CUPTI_ACTIVITY_KIND_OVERHEAD = 17
    Overhead activity records. The corresponding activity record structure is CUpti_ActivityOverhead.
  CUPTI_ACTIVITY_KIND_CDP_KERNEL = 18
    A CDP (CUDA Dynamic Parallel) kernel executing on the GPU. The corresponding activity record structure is CUpti_ActivityCdpKernel. This activity can not be directly enabled or disabled. It is enabled and disabled through concurrent kernel activity i.e. _CONCURRENT_KERNEL.
  CUPTI_ACTIVITY_KIND_PREEMPTION = 19
    Preemption activity record indicating a preemption of a CDP (CUDA Dynamic Parallel) kernel executing on the GPU. The corresponding activity record structure is CUpti_ActivityPreemption.
  CUPTI_ACTIVITY_KIND_ENVIRONMENT = 20
    Environment activity records indicating power, clock, thermal, etc. levels of the GPU. The corresponding activity record structure is CUpti_ActivityEnvironment.
  CUPTI_ACTIVITY_KIND_EVENT_INSTANCE = 21
    An event value associated with a specific event domain instance. The corresponding activity record structure is CUpti_ActivityEventInstance.
  CUPTI_ACTIVITY_KIND_MEMCPY2 = 22
    A peer to peer memory copy. The corresponding activity record structure is CUpti_ActivityMemcpyPtoP4.
  CUPTI_ACTIVITY_KIND_METRIC_INSTANCE = 23
    A metric value associated with a specific metric domain instance. The corresponding activity record structure is CUpti_ActivityMetricInstance.
  CUPTI_ACTIVITY_KIND_INSTRUCTION_EXECUTION = 24
    Results for source-level instruction execution. The corresponding activity record structure is CUpti_ActivityInstructionExecution.
  CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER = 25
    Unified Memory counter record. The corresponding activity record structure is CUpti_ActivityUnifiedMemoryCounter2.
  CUPTI_ACTIVITY_KIND_FUNCTION = 26
    Device global/function record. The corresponding activity record structure is CUpti_ActivityFunction.
  CUPTI_ACTIVITY_KIND_MODULE = 27
    CUDA Module record. The corresponding activity record structure is CUpti_ActivityModule.
  CUPTI_ACTIVITY_KIND_DEVICE_ATTRIBUTE = 28
    A device attribute value. The corresponding activity record structure is CUpti_ActivityDeviceAttribute.
  CUPTI_ACTIVITY_KIND_SHARED_ACCESS = 29
    Results for source-level shared acccess. The corresponding activity record structure is CUpti_ActivitySharedAccess.
  CUPTI_ACTIVITY_KIND_PC_SAMPLING = 30
    Enable PC sampling for kernels. This will serialize kernels. The corresponding activity record structure is CUpti_ActivityPCSampling3.
  CUPTI_ACTIVITY_KIND_PC_SAMPLING_RECORD_INFO = 31
    Summary information about PC sampling records. The corresponding activity record structure is CUpti_ActivityPCSamplingRecordInfo.
  CUPTI_ACTIVITY_KIND_INSTRUCTION_CORRELATION = 32
    SASS/Source line-by-line correlation record. This will generate sass/source correlation for functions that have source level analysis or pc sampling results. The records will be generated only when either of source level analysis or pc sampling activity is enabled. The corresponding activity record structure is CUpti_ActivityInstructionCorrelation.
  CUPTI_ACTIVITY_KIND_OPENACC_DATA = 33
    OpenACC data events. The corresponding activity record structure is CUpti_ActivityOpenAccData.
  CUPTI_ACTIVITY_KIND_OPENACC_LAUNCH = 34
    OpenACC launch events. The corresponding activity record structure is CUpti_ActivityOpenAccLaunch.
  CUPTI_ACTIVITY_KIND_OPENACC_OTHER = 35
    OpenACC other events. The corresponding activity record structure is CUpti_ActivityOpenAccOther.
  CUPTI_ACTIVITY_KIND_CUDA_EVENT = 36
    Information about a CUDA event. The corresponding activity record structure is CUpti_ActivityCudaEvent.
  CUPTI_ACTIVITY_KIND_STREAM = 37
    Information about a CUDA stream. The corresponding activity record structure is CUpti_ActivityStream.
  CUPTI_ACTIVITY_KIND_SYNCHRONIZATION = 38
    Records for synchronization management. The corresponding activity record structure is CUpti_ActivitySynchronization.
  CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION = 39
    Records for correlation of different programming APIs. The corresponding activity record structure is CUpti_ActivityExternalCorrelation.
  CUPTI_ACTIVITY_KIND_NVLINK = 40
    NVLink information. The corresponding activity record structure is CUpti_ActivityNvLink4.
  CUPTI_ACTIVITY_KIND_INSTANTANEOUS_EVENT = 41
    Instantaneous Event information. The corresponding activity record structure is CUpti_ActivityInstantaneousEvent.
  CUPTI_ACTIVITY_KIND_INSTANTANEOUS_EVENT_INSTANCE = 42
    Instantaneous Event information for a specific event domain instance. The corresponding activity record structure is CUpti_ActivityInstantaneousEventInstance
  CUPTI_ACTIVITY_KIND_INSTANTANEOUS_METRIC = 43
    Instantaneous Metric information The corresponding activity record structure is CUpti_ActivityInstantaneousMetric.
  CUPTI_ACTIVITY_KIND_INSTANTANEOUS_METRIC_INSTANCE = 44
    Instantaneous Metric information for a specific metric domain instance. The corresponding activity record structure is CUpti_ActivityInstantaneousMetricInstance.
  CUPTI_ACTIVITY_KIND_MEMORY = 45
    Memory activity tracking allocation and freeing of the memory The corresponding activity record structure is CUpti_ActivityMemory.
  CUPTI_ACTIVITY_KIND_PCIE = 46
    PCI devices information used for PCI topology. The corresponding activity record structure is CUpti_ActivityPcie.
  CUPTI_ACTIVITY_KIND_OPENMP = 47
    OpenMP parallel events. The corresponding activity record structure is CUpti_ActivityOpenMp.
  CUPTI_ACTIVITY_KIND_INTERNAL_LAUNCH_API = 48
    A CUDA driver kernel launch occurring outside of any public API function execution. Tools can handle these like records for driver API launch functions, although the cbid field is not used here. The corresponding activity record structure is CUpti_ActivityAPI.
  CUPTI_ACTIVITY_KIND_MEMORY2 = 49
    Memory activity tracking allocation and freeing of the memory The corresponding activity record structure is CUpti_ActivityMemory3.
  CUPTI_ACTIVITY_KIND_MEMORY_POOL = 50
    Memory pool activity tracking creation, destruction and triming of the memory pool. The corresponding activity record structure is CUpti_ActivityMemoryPool2.
  CUPTI_ACTIVITY_KIND_GRAPH_TRACE = 51
    The corresponding activity record structure is CUpti_ActivityGraphTrace.
  CUPTI_ACTIVITY_KIND_COUNT
  CUPTI_ACTIVITY_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityLaunchType

  ###### Values

  CUPTI_ACTIVITY_LAUNCH_TYPE_REGULAR = 0
    The kernel was launched via a regular kernel call
  CUPTI_ACTIVITY_LAUNCH_TYPE_COOPERATIVE_SINGLE_DEVICE = 1
    The kernel was launched via API cudaLaunchCooperativeKernel() or cuLaunchCooperativeKernel()
  CUPTI_ACTIVITY_LAUNCH_TYPE_COOPERATIVE_MULTI_DEVICE = 2
    The kernel was launched via API cudaLaunchCooperativeKernelMultiDevice() or cuLaunchCooperativeKernelMultiDevice()
enum CUpti_ActivityMemcpyKind

  Each kind represents the source and destination targets of a memory copy. Targets are host, device, and array.

  ###### Values

  CUPTI_ACTIVITY_MEMCPY_KIND_UNKNOWN = 0
    The memory copy kind is not known.
  CUPTI_ACTIVITY_MEMCPY_KIND_HTOD = 1
    A host to device memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_DTOH = 2
    A device to host memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_HTOA = 3
    A host to device array memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_ATOH = 4
    A device array to host memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_ATOA = 5
    A device array to device array memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_ATOD = 6
    A device array to device memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_DTOA = 7
    A device to device array memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_DTOD = 8
    A device to device memory copy on the same device.
  CUPTI_ACTIVITY_MEMCPY_KIND_HTOH = 9
    A host to host memory copy.
  CUPTI_ACTIVITY_MEMCPY_KIND_PTOP = 10
    A peer to peer memory copy across different devices.
  CUPTI_ACTIVITY_MEMCPY_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityMemoryKind

  Each kind represents the type of the memory accessed by a memory operation/copy.

  ###### Values

  CUPTI_ACTIVITY_MEMORY_KIND_UNKNOWN = 0
    The memory kind is unknown.
  CUPTI_ACTIVITY_MEMORY_KIND_PAGEABLE = 1
    The memory is pageable.
  CUPTI_ACTIVITY_MEMORY_KIND_PINNED = 2
    The memory is pinned.
  CUPTI_ACTIVITY_MEMORY_KIND_DEVICE = 3
    The memory is on the device.
  CUPTI_ACTIVITY_MEMORY_KIND_ARRAY = 4
    The memory is an array.
  CUPTI_ACTIVITY_MEMORY_KIND_MANAGED = 5
    The memory is managed
  CUPTI_ACTIVITY_MEMORY_KIND_DEVICE_STATIC = 6
    The memory is device static
  CUPTI_ACTIVITY_MEMORY_KIND_MANAGED_STATIC = 7
    The memory is managed static
  CUPTI_ACTIVITY_MEMORY_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityMemoryOperationType

  Describes the type of memory operation, to be used with CUpti_ActivityMemory3.

  ###### Values

  CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_INVALID = 0
  CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_ALLOCATION = 1
    Memory is allocated.
  CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_RELEASE = 2
    Memory is released.
  CUPTI_ACTIVITY_MEMORY_OPERATION_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityMemoryPoolOperationType

  Describes the type of memory pool operation, to be used with CUpti_ActivityMemoryPool2.

  ###### Values

  CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_INVALID = 0
  CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_CREATED = 1
    Memory pool is created.
  CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_DESTROYED = 2
    Memory pool is destroyed.
  CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_TRIMMED = 3
    Memory pool is trimmed.
  CUPTI_ACTIVITY_MEMORY_POOL_OPERATION_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityMemoryPoolType

  Describes the type of memory pool, to be used with CUpti_ActivityMemory3.

  ###### Values

  CUPTI_ACTIVITY_MEMORY_POOL_TYPE_INVALID = 0
  CUPTI_ACTIVITY_MEMORY_POOL_TYPE_LOCAL = 1
    Memory pool is local to the process.
  CUPTI_ACTIVITY_MEMORY_POOL_TYPE_IMPORTED = 2
    Memory pool is imported by the process.
  CUPTI_ACTIVITY_MEMORY_POOL_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityObjectKind

  See also:

  CUpti_ActivityObjectKindId

  ###### Values

  CUPTI_ACTIVITY_OBJECT_UNKNOWN = 0
    The object kind is not known.
  CUPTI_ACTIVITY_OBJECT_PROCESS = 1
    A process.
  CUPTI_ACTIVITY_OBJECT_THREAD = 2
    A thread.
  CUPTI_ACTIVITY_OBJECT_DEVICE = 3
    A device.
  CUPTI_ACTIVITY_OBJECT_CONTEXT = 4
    A context.
  CUPTI_ACTIVITY_OBJECT_STREAM = 5
    A stream.
  CUPTI_ACTIVITY_OBJECT_FORCE_INT = 0x7fffffff
enum CUpti_ActivityOverheadKind

  ###### Values

  CUPTI_ACTIVITY_OVERHEAD_UNKNOWN = 0
    The overhead kind is not known.
  CUPTI_ACTIVITY_OVERHEAD_DRIVER_COMPILER = 1
    Compiler(JIT) overhead.
  CUPTI_ACTIVITY_OVERHEAD_CUPTI_BUFFER_FLUSH = 1<<16
    Activity buffer flush overhead.
  CUPTI_ACTIVITY_OVERHEAD_CUPTI_INSTRUMENTATION = 2<<16
    CUPTI instrumentation overhead.
  CUPTI_ACTIVITY_OVERHEAD_CUPTI_RESOURCE = 3<<16
    CUPTI resource creation and destruction overhead.
  CUPTI_ACTIVITY_OVERHEAD_FORCE_INT = 0x7fffffff
enum CUpti_ActivityPCSamplingPeriod

  Sampling period can be set using cuptiActivityConfigurePCSampling

  ###### Values

  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_INVALID = 0
    The PC sampling period is not set.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MIN = 1
    Minimum sampling period available on the device.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_LOW = 2
    Sampling period in lower range.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MID = 3
    Medium sampling period.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_HIGH = 4
    Sampling period in higher range.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_MAX = 5
    Maximum sampling period available on the device.
  CUPTI_ACTIVITY_PC_SAMPLING_PERIOD_FORCE_INT = 0x7fffffff
enum CUpti_ActivityPCSamplingStallReason

  ###### Values

  CUPTI_ACTIVITY_PC_SAMPLING_STALL_INVALID = 0
    Invalid reason
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_NONE = 1
    No stall, instruction is selected for issue
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_INST_FETCH = 2
    Warp is blocked because next instruction is not yet available, because of instruction cache miss, or because of branching effects
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_EXEC_DEPENDENCY = 3
    Instruction is waiting on an arithmatic dependency
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_MEMORY_DEPENDENCY = 4
    Warp is blocked because it is waiting for a memory access to complete.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_TEXTURE = 5
    Texture sub-system is fully utilized or has too many outstanding requests.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_SYNC = 6
    Warp is blocked as it is waiting at __syncthreads() or at memory barrier.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_CONSTANT_MEMORY_DEPENDENCY = 7
    Warp is blocked waiting for __constant__ memory and immediate memory access to complete.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_PIPE_BUSY = 8
    Compute operation cannot be performed due to the required resources not being available.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_MEMORY_THROTTLE = 9
    Warp is blocked because there are too many pending memory operations. In Kepler architecture it often indicates high number of memory replays.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_NOT_SELECTED = 10
    Warp was ready to issue, but some other warp issued instead.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_OTHER = 11
    Miscellaneous reasons
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_SLEEPING = 12
    Sleeping.
  CUPTI_ACTIVITY_PC_SAMPLING_STALL_FORCE_INT = 0x7fffffff
enum CUpti_ActivityPartitionedGlobalCacheConfig

  ###### Values

  CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_UNKNOWN = 0
    Partitioned global cache config unknown.
  CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_NOT_SUPPORTED = 1
    Partitioned global cache not supported.
  CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_OFF = 2
    Partitioned global cache config off.
  CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_ON = 3
    Partitioned global cache config on.
  CUPTI_ACTIVITY_PARTITIONED_GLOBAL_CACHE_CONFIG_FORCE_INT = 0x7fffffff
enum CUpti_ActivityPreemptionKind

  ###### Values

  CUPTI_ACTIVITY_PREEMPTION_KIND_UNKNOWN = 0
    The preemption kind is not known.
  CUPTI_ACTIVITY_PREEMPTION_KIND_SAVE = 1
    Preemption to save CDP block.
  CUPTI_ACTIVITY_PREEMPTION_KIND_RESTORE = 2
    Preemption to restore CDP block.
  CUPTI_ACTIVITY_PREEMPTION_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityStreamFlag

  The types of stream to be used with CUpti_ActivityStream.

  ###### Values

  CUPTI_ACTIVITY_STREAM_CREATE_FLAG_UNKNOWN = 0
    Unknown data.
  CUPTI_ACTIVITY_STREAM_CREATE_FLAG_DEFAULT = 1
    Default stream.
  CUPTI_ACTIVITY_STREAM_CREATE_FLAG_NON_BLOCKING = 2
    Non-blocking stream.
  CUPTI_ACTIVITY_STREAM_CREATE_FLAG_NULL = 3
    Null stream.
  CUPTI_ACTIVITY_STREAM_CREATE_MASK = 0xFFFF
    Stream create Mask
  CUPTI_ACTIVITY_STREAM_CREATE_FLAG_FORCE_INT = 0x7fffffff
enum CUpti_ActivitySynchronizationType

  The types of synchronization to be used with CUpti_ActivitySynchronization.

  ###### Values

  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_UNKNOWN = 0
    Unknown data.
  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_EVENT_SYNCHRONIZE = 1
    Event synchronize API.
  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_STREAM_WAIT_EVENT = 2
    Stream wait event API.
  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_STREAM_SYNCHRONIZE = 3
    Stream synchronize API.
  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_CONTEXT_SYNCHRONIZE = 4
    Context synchronize API.
  CUPTI_ACTIVITY_SYNCHRONIZATION_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityThreadIdType

  CUPTI uses different methods to obtain the thread-id depending on the support and the underlying platform. This enum documents these methods for each type. APIs cuptiSetThreadIdType and cuptiGetThreadIdType can be used to set and get the thread-id type.

  ###### Values

  CUPTI_ACTIVITY_THREAD_ID_TYPE_DEFAULT = 0
    Default type Windows uses API GetCurrentThreadId() Linux/Mac/Android/QNX use POSIX pthread API pthread_self()
  CUPTI_ACTIVITY_THREAD_ID_TYPE_SYSTEM = 1
    This type is based on the system API available on the underlying platform and thread-id obtained is supposed to be unique for the process lifetime. Windows uses API GetCurrentThreadId() Linux uses syscall SYS_gettid Mac uses syscall SYS_thread_selfid Android/QNX use gettid()
  CUPTI_ACTIVITY_THREAD_ID_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityUnifiedMemoryAccessType

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_GPU_PAGE_FAULT and CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_CPU_PAGE_FAULT_COUNT

  ###### Values

  CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_UNKNOWN = 0
    The unified memory access type is not known
  CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_READ = 1
    The page fault was triggered by read memory instruction
  CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_WRITE = 2
    The page fault was triggered by write memory instruction
  CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_ATOMIC = 3
    The page fault was triggered by atomic memory instruction
  CUPTI_ACTIVITY_UNIFIED_MEMORY_ACCESS_TYPE_PREFETCH = 4
    The page fault was triggered by memory prefetch operation
enum CUpti_ActivityUnifiedMemoryCounterKind

  Many activities are associated with Unified Memory mechanism; among them are tranfer from host to device, device to host, page fault at host side.

  ###### Values

  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_UNKNOWN = 0
    The unified memory counter kind is not known.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_HTOD = 1
    Number of bytes transfered from host to device
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOH = 2
    Number of bytes transfered from device to host
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_CPU_PAGE_FAULT_COUNT = 3
    Number of CPU page faults, this is only supported on 64 bit Linux and Mac platforms
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_GPU_PAGE_FAULT = 4
    Number of GPU page faults, this is only supported on devices with compute capability 6.0 and higher and 64 bit Linux platforms
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THRASHING = 5
    Thrashing occurs when data is frequently accessed by multiple processors and has to be constantly migrated around to achieve data locality. In this case the overhead of migration may exceed the benefits of locality. This is only supported on 64 bit Linux platforms.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_THROTTLING = 6
    Throttling is a prevention technique used by the driver to avoid further thrashing. Here, the driver doesn't service the fault for one of the contending processors for a specific period of time, so that the other processor can run at full-speed. This is only supported on 64 bit Linux platforms.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_REMOTE_MAP = 7
    In case throttling does not help, the driver tries to pin the memory to a processor for a specific period of time. One of the contending processors will have slow access to the memory, while the other will have fast access. This is only supported on 64 bit Linux platforms.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOD = 8
    Number of bytes transferred from one device to another device. This is only supported on 64 bit Linux platforms.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_COUNT
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_FORCE_INT = 0x7fffffff
enum CUpti_ActivityUnifiedMemoryCounterScope

  ###### Values

  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_UNKNOWN = 0
    The unified memory counter scope is not known.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_PROCESS_SINGLE_DEVICE = 1
    Collect unified memory counter for single process on one device
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_PROCESS_ALL_DEVICES = 2
    Collect unified memory counter for single process across all devices
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_COUNT
  CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_SCOPE_FORCE_INT = 0x7fffffff
enum CUpti_ActivityUnifiedMemoryMigrationCause

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_HTOD and CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_BYTES_TRANSFER_DTOH

  ###### Values

  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_UNKNOWN = 0
    The unified memory migration cause is not known
  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_USER = 1
    The unified memory migrated due to an explicit call from the user e.g. cudaMemPrefetchAsync
  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_COHERENCE = 2
    The unified memory migrated to guarantee data coherence e.g. CPU/GPU faults on Pascal+ and kernel launch on pre-Pascal GPUs
  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_PREFETCH = 3
    The unified memory was speculatively migrated by the UVM driver before being accessed by the destination processor to improve performance
  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_EVICTION = 4
    The unified memory migrated to the CPU because it was evicted to make room for another block of memory on the GPU
  CUPTI_ACTIVITY_UNIFIED_MEMORY_MIGRATION_CAUSE_ACCESS_COUNTERS = 5
    The unified memory migrated to another processor because of access counter notifications. Only frequently accessed pages are migrated between CPU and GPU, or between peer GPUs.
enum CUpti_ActivityUnifiedMemoryRemoteMapCause

  This is valid for CUPTI_ACTIVITY_UNIFIED_MEMORY_COUNTER_KIND_REMOTE_MAP

  ###### Values

  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_UNKNOWN = 0
    The cause of mapping to remote memory was unknown
  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_COHERENCE = 1
    Mapping to remote memory was added to maintain data coherence.
  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_THRASHING = 2
    Mapping to remote memory was added to prevent further thrashing
  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_POLICY = 3
    Mapping to remote memory was added to enforce the hints specified by the programmer or by performance heuristics of the UVM driver
  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_OUT_OF_MEMORY = 4
    Mapping to remote memory was added because there is no more memory available on the processor and eviction was not possible
  CUPTI_ACTIVITY_UNIFIED_MEMORY_REMOTE_MAP_CAUSE_EVICTION = 5
    Mapping to remote memory was added after the memory was evicted to make room for another block of memory on the GPU
enum CUpti_DevType

  ###### Values

  CUPTI_DEV_TYPE_INVALID = 0
  CUPTI_DEV_TYPE_GPU = 1
    The device type is GPU.
  CUPTI_DEV_TYPE_NPU = 2
    The device type is NVLink processing unit in CPU.
  CUPTI_DEV_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_DeviceVirtualizationMode

  This indicates the virtualization mode in which CUDA device is running

  ###### Values

  CUPTI_DEVICE_VIRTUALIZATION_MODE_NONE = 0
    No virtualization mode isassociated with the device i.e. it's a baremetal GPU
  CUPTI_DEVICE_VIRTUALIZATION_MODE_PASS_THROUGH = 1
    The device is associated with the pass-through GPU. In this mode, an entire physical GPU is directly assigned to one virtual machine (VM).
  CUPTI_DEVICE_VIRTUALIZATION_MODE_VIRTUAL_GPU = 2
    The device is associated with the virtual GPU (vGPU). In this mode multiple virtual machines (VMs) have simultaneous, direct access to a single physical GPU.
  CUPTI_DEVICE_VIRTUALIZATION_MODE_FORCE_INT = 0x7fffffff
enum CUpti_EnvironmentClocksThrottleReason

  The possible reasons that a clock can be throttled. There can be more than one reason that a clock is being throttled so these types can be combined by bitwise OR. These are used in the clocksThrottleReason field in the Environment Activity Record.

  ###### Values

  CUPTI_CLOCKS_THROTTLE_REASON_GPU_IDLE = 0x00000001
    Nothing is running on the GPU and the clocks are dropping to idle state.
  CUPTI_CLOCKS_THROTTLE_REASON_USER_DEFINED_CLOCKS = 0x00000002
    The GPU clocks are limited by a user specified limit.
  CUPTI_CLOCKS_THROTTLE_REASON_SW_POWER_CAP = 0x00000004
    A software power scaling algorithm is reducing the clocks below requested clocks.
  CUPTI_CLOCKS_THROTTLE_REASON_HW_SLOWDOWN = 0x00000008
    Hardware slowdown to reduce the clock by a factor of two or more is engaged. This is an indicator of one of the following: 1) Temperature is too high, 2) External power brake assertion is being triggered (e.g. by the system power supply), 3) Change in power state.
  CUPTI_CLOCKS_THROTTLE_REASON_UNKNOWN = 0x80000000
    Some unspecified factor is reducing the clocks.
  CUPTI_CLOCKS_THROTTLE_REASON_UNSUPPORTED = 0x40000000
    Throttle reason is not supported for this GPU.
  CUPTI_CLOCKS_THROTTLE_REASON_NONE = 0x00000000
    No clock throttling.
  CUPTI_CLOCKS_THROTTLE_REASON_FORCE_INT = 0x7fffffff
enum CUpti_ExternalCorrelationKind

  Custom correlation kinds are reserved for usage in external tools.

  See also:

  CUpti_ActivityExternalCorrelation

  ###### Values

  CUPTI_EXTERNAL_CORRELATION_KIND_INVALID = 0
  CUPTI_EXTERNAL_CORRELATION_KIND_UNKNOWN = 1
    The external API is unknown to CUPTI
  CUPTI_EXTERNAL_CORRELATION_KIND_OPENACC = 2
    The external API is OpenACC
  CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM0 = 3
    The external API is custom0
  CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM1 = 4
    The external API is custom1
  CUPTI_EXTERNAL_CORRELATION_KIND_CUSTOM2 = 5
    The external API is custom2
  CUPTI_EXTERNAL_CORRELATION_KIND_SIZE
    Add new kinds before this line
  CUPTI_EXTERNAL_CORRELATION_KIND_FORCE_INT = 0x7fffffff
enum CUpti_FuncShmemLimitConfig

  ###### Values

  CUPTI_FUNC_SHMEM_LIMIT_DEFAULT = 0x00
  CUPTI_FUNC_SHMEM_LIMIT_OPTIN = 0x01
  CUPTI_FUNC_SHMEM_LIMIT_FORCE_INT = 0x7fffffff
enum CUpti_LinkFlag

  Describes link properties, to be used with CUpti_ActivityNvLink.

  ###### Values

  CUPTI_LINK_FLAG_INVALID = 0
  CUPTI_LINK_FLAG_PEER_ACCESS = (1<<1)
    Is peer to peer access supported by this link.
  CUPTI_LINK_FLAG_SYSMEM_ACCESS = (1<<2)
    Is system memory access supported by this link.
  CUPTI_LINK_FLAG_PEER_ATOMICS = (1<<3)
    Is peer atomic access supported by this link.
  CUPTI_LINK_FLAG_SYSMEM_ATOMICS = (1<<4)
    Is system memory atomic access supported by this link.
  CUPTI_LINK_FLAG_FORCE_INT = 0x7fffffff
enum CUpti_OpenAccConstructKind

  ###### Values

  CUPTI_OPENACC_CONSTRUCT_KIND_UNKNOWN = 0
  CUPTI_OPENACC_CONSTRUCT_KIND_PARALLEL = 1
  CUPTI_OPENACC_CONSTRUCT_KIND_KERNELS = 2
  CUPTI_OPENACC_CONSTRUCT_KIND_LOOP = 3
  CUPTI_OPENACC_CONSTRUCT_KIND_DATA = 4
  CUPTI_OPENACC_CONSTRUCT_KIND_ENTER_DATA = 5
  CUPTI_OPENACC_CONSTRUCT_KIND_EXIT_DATA = 6
  CUPTI_OPENACC_CONSTRUCT_KIND_HOST_DATA = 7
  CUPTI_OPENACC_CONSTRUCT_KIND_ATOMIC = 8
  CUPTI_OPENACC_CONSTRUCT_KIND_DECLARE = 9
  CUPTI_OPENACC_CONSTRUCT_KIND_INIT = 10
  CUPTI_OPENACC_CONSTRUCT_KIND_SHUTDOWN = 11
  CUPTI_OPENACC_CONSTRUCT_KIND_SET = 12
  CUPTI_OPENACC_CONSTRUCT_KIND_UPDATE = 13
  CUPTI_OPENACC_CONSTRUCT_KIND_ROUTINE = 14
  CUPTI_OPENACC_CONSTRUCT_KIND_WAIT = 15
  CUPTI_OPENACC_CONSTRUCT_KIND_RUNTIME_API = 16
  CUPTI_OPENACC_CONSTRUCT_KIND_FORCE_INT = 0x7fffffff
enum CUpti_OpenAccEventKind

  See also:

  CUpti_ActivityKindOpenAcc

  ###### Values

  CUPTI_OPENACC_EVENT_KIND_INVALID = 0
  CUPTI_OPENACC_EVENT_KIND_DEVICE_INIT = 1
  CUPTI_OPENACC_EVENT_KIND_DEVICE_SHUTDOWN = 2
  CUPTI_OPENACC_EVENT_KIND_RUNTIME_SHUTDOWN = 3
  CUPTI_OPENACC_EVENT_KIND_ENQUEUE_LAUNCH = 4
  CUPTI_OPENACC_EVENT_KIND_ENQUEUE_UPLOAD = 5
  CUPTI_OPENACC_EVENT_KIND_ENQUEUE_DOWNLOAD = 6
  CUPTI_OPENACC_EVENT_KIND_WAIT = 7
  CUPTI_OPENACC_EVENT_KIND_IMPLICIT_WAIT = 8
  CUPTI_OPENACC_EVENT_KIND_COMPUTE_CONSTRUCT = 9
  CUPTI_OPENACC_EVENT_KIND_UPDATE = 10
  CUPTI_OPENACC_EVENT_KIND_ENTER_DATA = 11
  CUPTI_OPENACC_EVENT_KIND_EXIT_DATA = 12
  CUPTI_OPENACC_EVENT_KIND_CREATE = 13
  CUPTI_OPENACC_EVENT_KIND_DELETE = 14
  CUPTI_OPENACC_EVENT_KIND_ALLOC = 15
  CUPTI_OPENACC_EVENT_KIND_FREE = 16
  CUPTI_OPENACC_EVENT_KIND_FORCE_INT = 0x7fffffff
enum CUpti_PcieDeviceType

  Field to differentiate whether PCIE Activity record is of a GPU or a PCI Bridge

  ###### Values

  CUPTI_PCIE_DEVICE_TYPE_GPU = 0
    PCIE GPU record
  CUPTI_PCIE_DEVICE_TYPE_BRIDGE = 1
    PCIE Bridge record
  CUPTI_PCIE_DEVICE_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_PcieGen

  Enumeration of PCIE Generation for pcie activity attribute pcieGeneration

  ###### Values

  CUPTI_PCIE_GEN_GEN1 = 1
    PCIE Generation 1
  CUPTI_PCIE_GEN_GEN2 = 2
    PCIE Generation 2
  CUPTI_PCIE_GEN_GEN3 = 3
    PCIE Generation 3
  CUPTI_PCIE_GEN_GEN4 = 4
    PCIE Generation 4
  CUPTI_PCIE_GEN_GEN5 = 5
    PCIE Generation 5
  CUPTI_PCIE_GEN_FORCE_INT = 0x7fffffff

#### Functions

CUptiResult cuptiActivityConfigurePCSampling ( CUcontext ctx, CUpti_ActivityPCSamplingConfig* config )
  Set PC sampling configuration.

  ###### Parameters

  `ctx`
    The context
  `config`
    A pointer to CUpti_ActivityPCSamplingConfig structure containing PC sampling configuration.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this api is called while some valid event collection method is set.

  - CUPTI_ERROR_INVALID_PARAMETER

    if `config` is NULL or any parameter in the `config` structures is not a valid value

  - CUPTI_ERROR_NOT_SUPPORTED

    Indicates that the system/device does not support the unified memory counters

  ###### Description

  For Pascal and older GPU architectures this API must be called before enabling activity kind CUPTI_ACTIVITY_KIND_PC_SAMPLING. There is no such requirement for Volta and newer GPU architectures.

  For Volta and newer GPU architectures if this API is called in the middle of execution, PC sampling configuration will be updated for subsequent kernel launches.

CUptiResult cuptiActivityConfigureUnifiedMemoryCounter ( CUpti_ActivityUnifiedMemoryCounterConfig* config, uint32_t count )
  Set Unified Memory Counter configuration.

  ###### Parameters

  `config`
    A pointer to CUpti_ActivityUnifiedMemoryCounterConfig structures containing Unified Memory counter configuration.
  `count`
    Number of Unified Memory counter configuration structures

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `config` is NULL or any parameter in the `config` structures is not a valid value

  - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED

    One potential reason is that platform (OS/arch) does not support the unified memory counters

  - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_DEVICE

    Indicates that the device does not support the unified memory counters

  - CUPTI_ERROR_UM_PROFILING_NOT_SUPPORTED_ON_NON_P2P_DEVICES

    Indicates that multi-GPU configuration without P2P support between any pair of devices does not support the unified memory counters

  ###### Description

CUptiResult cuptiActivityDisable ( CUpti_ActivityKind kind )
  Disable collection of a specific kind of activity record.

  ###### Parameters

  `kind`
    The kind of activity record to stop collecting

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_KIND

    if the activity kind is not supported

  ###### Description

  Disable collection of a specific kind of activity record. Multiple kinds can be disabled by calling this function multiple times. By default all activity kinds are disabled for collection.

CUptiResult cuptiActivityDisableContext ( CUcontext context, CUpti_ActivityKind kind )
  Disable collection of a specific kind of activity record for a context.

  ###### Parameters

  `context`
    The context for which activity is to be disabled
  `kind`
    The kind of activity record to stop collecting

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_KIND

    if the activity kind is not supported

  ###### Description

  Disable collection of a specific kind of activity record for a context. This setting done by this API will supersede the global settings for activity records. Multiple kinds can be enabled by calling this function multiple times.

CUptiResult cuptiActivityEnable ( CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record.

  ###### Parameters

  `kind`
    The kind of activity record to collect

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_NOT_COMPATIBLE

    if the activity kind cannot be enabled

  - CUPTI_ERROR_INVALID_KIND

    if the activity kind is not supported

  ###### Description

  Enable collection of a specific kind of activity record. Multiple kinds can be enabled by calling this function multiple times. By default all activity kinds are disabled for collection.

CUptiResult cuptiActivityEnableAndDump ( CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record. For certain activity kinds it dumps existing records.

  ###### Parameters

  `kind`
    The kind of activity record to collect

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_UNKNOWN

    if buffer is not initialized.

  - CUPTI_ERROR_NOT_COMPATIBLE

    if the activity kind cannot be enabled

  - CUPTI_ERROR_INVALID_KIND

    if the activity kind is not supported

  ###### Description

  In general, the behavior of this API is similar to the API cuptiActivityEnable i.e. it enables the collection of a specific kind of activity record. Additionally, this API can help in dumping the records for activities which happened in the past before enabling the corresponding activity kind. The API allows to get records for the current resource allocations done in CUDA For CUPTI_ACTIVITY_KIND_DEVICE, existing device records are dumped For CUPTI_ACTIVITY_KIND_CONTEXT, existing context records are dumped For CUPTI_ACTIVITY_KIND_STREAM, existing stream records are dumped For CUPTI_ACTIVITY_KIND_ NVLINK, existing NVLINK records are dumped For CUPTI_ACTIVITY_KIND_PCIE, existing PCIE records are dumped For other activities, the behavior is similar to the API cuptiActivityEnable

  Device records are emitted in CUPTI on CUDA driver initialization. Those records can only be retrieved by the user if CUPTI is attached before CUDA initialization. Context and stream records are emitted on context and stream creation. The use case of the API is to provide the records for CUDA resources (contexs/streams/devices) that are currently active if user late attaches CUPTI.

  Before calling this function, the user must register buffer callbacks to get the activity records by calling cuptiActivityRegisterCallbacks. If the user does not register the buffers and calls API cuptiActivityEnableAndDump, then CUPTI will enable the activity kind but not provide any records for that activity kind.

CUptiResult cuptiActivityEnableContext ( CUcontext context, CUpti_ActivityKind kind )
  Enable collection of a specific kind of activity record for a context.

  ###### Parameters

  `context`
    The context for which activity is to be enabled
  `kind`
    The kind of activity record to collect

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_NOT_COMPATIBLE

    if the activity kind cannot be enabled

  - CUPTI_ERROR_INVALID_KIND

    if the activity kind is not supported

  ###### Description

  Enable collection of a specific kind of activity record for a context. This setting done by this API will supersede the global settings for activity records enabled by cuptiActivityEnable. Multiple kinds can be enabled by calling this function multiple times.

CUptiResult cuptiActivityEnableLatencyTimestamps ( uint8_t enable )
  Controls the collection of queued and submitted timestamps for kernels.

  ###### Parameters

  `enable`
    is a boolean, denoting whether these timestamps should be collected

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  ###### Description

  This API is used to control the collection of queued and submitted timestamps for kernels whose records are provided through the struct CUpti_ActivityKernel7. Default value is 0, i.e. these timestamps are not collected. This API needs to be called before initialization of CUDA and this setting should not be changed during the profiling session.

CUptiResult cuptiActivityEnableLaunchAttributes ( uint8_t enable )
  Controls the collection of launch attributes for kernels.

  ###### Parameters

  `enable`
    is a boolean denoting whether these launch attributes should be collected

  ###### Description

  This API is used to control the collection of launch attributes for kernels whose records are provided through the struct CUpti_ActivityKernel7. Default value is 0, i.e. these attributes are not collected.

CUptiResult cuptiActivityFlush ( CUcontext context, uint32_t streamId, uint32_t flag )
  Wait for all activity records to be delivered via the completion callback.

  ###### Parameters

  `context`
    A valid CUcontext or NULL.
  `streamId`
    The stream ID.
  `flag`
    The flag can be set to indicate a forced flush. See CUpti_ActivityFlag

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_CUPTI_ERROR_INVALID_OPERATION

    if not preceeded by a successful call to cuptiActivityRegisterCallbacks

  - CUPTI_ERROR_UNKNOWN

    an internal error occurred

  ###### Description

  This function does not return until all activity records associated with the specified context/stream are returned to the CUPTI client using the callback registered in cuptiActivityRegisterCallbacks. To ensure that all activity records are complete, the requested stream(s), if any, are synchronized.

  If `context` is NULL, the global activity records (i.e. those not associated with a particular stream) are flushed (in this case no streams are synchonized). If `context` is a valid CUcontext and `streamId` is 0, the buffers of all streams of this context are flushed. Otherwise, the buffers of the specified stream in this context is flushed.

  Before calling this function, the buffer handling callback api must be activated by calling cuptiActivityRegisterCallbacks.

  **DEPRECATED** This method is deprecated CONTEXT and STREAMID will be ignored. Use cuptiActivityFlushAll to flush all data.

CUptiResult cuptiActivityFlushAll ( uint32_t flag )
  Request to deliver activity records via the buffer completion callback.

  ###### Parameters

  `flag`
    The flag can be set to indicate a forced flush. See CUpti_ActivityFlag

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_OPERATION

    if not preceeded by a successful call to cuptiActivityRegisterCallbacks

  - CUPTI_ERROR_UNKNOWN

    an internal error occurred

  ###### Description

  This function returns the activity records associated with all contexts/streams (and the global buffers not associated with any stream) to the CUPTI client using the callback registered in cuptiActivityRegisterCallbacks.

  This is a blocking call but it doesn't issue any CUDA synchronization calls implicitly thus it's not guaranteed that all activities are completed on the underlying devices. Activity record is considered as completed if it has all the information filled up including the timestamps if any. It is the client's responsibility to issue necessary CUDA synchronization calls before calling this function if all activity records with complete information are expected to be delivered.

  Behavior of the function based on the input flag:

  - For default flush i.e. when flag is set as 0, it returns all the activity buffers which have all the activity records completed, buffers need not to be full though. It doesn't return buffers which have one or more incomplete records. Default flush can be done at a regular interval in a separate thread.

  - For forced flush i.e. when flag CUPTI_ACTIVITY_FLAG_FLUSH_FORCED is passed to the function, it returns all the activity buffers including the ones which have one or more incomplete activity records. It's suggested for clients to do the force flush before the termination of the profiling session to allow remaining buffers to be delivered. In general, it can be done in the at-exit handler.

  Before calling this function, the buffer handling callback api must be activated by calling cuptiActivityRegisterCallbacks.

  See also:

  cuptiActivityFlushPeriod

CUptiResult cuptiActivityFlushPeriod ( uint32_t time )
  Sets the flush period for the worker thread.

  ###### Parameters

  `time`
    flush period in msec

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  ###### Description

  CUPTI creates a worker thread to minimize the perturbance for the application created threads. CUPTI offloads certain operations from the application threads to the worker thread, this includes synchronization of profiling resources between host and device, delivery of the activity buffers to the client using the callback registered in cuptiActivityRegisterCallbacks. For performance reasons, CUPTI wakes up the worker thread based on certain heuristics.

  This API is used to control the flush period of the worker thread. This setting will override the CUPTI heurtistics. Setting time to zero disables the periodic flush and restores the default behavior.

  Periodic flush can return only those activity buffers which are full and have all the activity records completed.

  It's allowed to use the API cuptiActivityFlushAll to flush the data on-demand, even when client sets the periodic flush.

  See also:

  cuptiActivityFlushAll

CUptiResult cuptiActivityGetAttribute ( CUpti_ActivityAttribute attr, size_t* valueSize, void* value )
  Read an activity API attribute.

  ###### Parameters

  `attr`
    The attribute to read
  `valueSize`
    Size of buffer pointed by the value, and returns the number of bytes written to `value`
  `value`
    Returns the value of the attribute

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    Indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Read an activity API attribute and return it in `*value`.

CUptiResult cuptiActivityGetNextRecord ( uint8_t* buffer, size_t validBufferSizeBytes, CUpti_Activity** record )
  Iterate over the activity records in a buffer.

  ###### Parameters

  `buffer`
    The buffer containing activity records
  `validBufferSizeBytes`
    The number of valid bytes in the buffer.
  `record`
    Inputs the previous record returned by cuptiActivityGetNextRecord and returns the next activity record from the buffer. If input value is NULL, returns the first activity record in the buffer. Records of kind CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL may contain invalid (0) timestamps, indicating that no timing information could be collected for lack of device memory.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_MAX_LIMIT_REACHED

    if no more records in the buffer

  - CUPTI_ERROR_INVALID_PARAMETER

    if `buffer` is NULL.

  ###### Description

  This is a helper function to iterate over the activity records in a buffer. A buffer of activity records is typically obtained by receiving a CUpti_BuffersCallbackCompleteFunc callback.

  An example of typical usage:

      ‎ CUpti_Activity *record = NULL;
             CUptiResult status = CUPTI_SUCCESS;
               do {
                  status = cuptiActivityGetNextRecord(buffer, validSize, &record);
                  if(status == CUPTI_SUCCESS) {
                       // Use record here...
                  }
                  else if (status == CUPTI_ERROR_MAX_LIMIT_REACHED)
                      break;
                  else {
                      goto Error;
                  }
                } while (1);

CUptiResult cuptiActivityGetNumDroppedRecords ( CUcontext context, uint32_t streamId, size_t* dropped )
  Get the number of activity records that were dropped of insufficient buffer space.

  ###### Parameters

  `context`
    The context, or NULL to get dropped count from global queue
  `streamId`
    The stream ID
  `dropped`
    The number of records that were dropped since the last call to this function.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `dropped` is NULL

  ###### Description

  Get the number of records that were dropped because of insufficient buffer space. The dropped count includes records that could not be recorded because CUPTI did not have activity buffer space available for the record (because the CUpti_BuffersCallbackRequestFunc callback did not return an empty buffer of sufficient size) and also CDP records that could not be record because the device-size buffer was full (size is controlled by the CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE_CDP attribute). The dropped count maintained for the queue is reset to zero when this function is called.

CUptiResult cuptiActivityPopExternalCorrelationId ( CUpti_ExternalCorrelationKind kind, uint64_t* lastId )
  Pop an external correlation id for the calling thread.

  ###### Parameters

  `kind`
    The kind of external API activities should be correlated with.
  `lastId`
    If the function returns successful, contains the last external correlation id for this `kind`, can be NULL.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    The external API kind is invalid.

  - CUPTI_ERROR_QUEUE_EMPTY

    No external id is currently associated with `kind`.

  ###### Description

  This function notifies CUPTI that the calling thread is leaving an external API region.

CUptiResult cuptiActivityPushExternalCorrelationId ( CUpti_ExternalCorrelationKind kind, uint64_t id )
  Push an external correlation id for the calling thread.

  ###### Parameters

  `kind`
    The kind of external API activities should be correlated with.
  `id`
    External correlation id.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    The external API kind is invalid

  ###### Description

  This function notifies CUPTI that the calling thread is entering an external API region. When a CUPTI activity API record is created while within an external API region and CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION is enabled, the activity API record will be preceeded by a CUpti_ActivityExternalCorrelation record for each CUpti_ExternalCorrelationKind.

CUptiResult cuptiActivityRegisterCallbacks ( CUpti_BuffersCallbackRequestFunc funcBufferRequested, CUpti_BuffersCallbackCompleteFunc funcBufferCompleted )
  Registers callback functions with CUPTI for activity buffer handling.

  ###### Parameters

  `funcBufferRequested`
    callback which is invoked when an empty buffer is requested by CUPTI
  `funcBufferCompleted`
    callback which is invoked when a buffer containing activity records is available from CUPTI

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if either `funcBufferRequested` or `funcBufferCompleted` is NULL

  ###### Description

  This function registers two callback functions to be used in asynchronous buffer handling. If registered, activity record buffers are handled using asynchronous requested/completed callbacks from CUPTI.

  Registering these callbacks prevents the client from using CUPTI's blocking enqueue/dequeue functions.

CUptiResult cuptiActivityRegisterTimestampCallback ( CUpti_TimestampCallbackFunc funcTimestamp )
  Registers callback function with CUPTI for providing timestamp.

  ###### Parameters

  `funcTimestamp`
    callback which is invoked when a timestamp is needed by CUPTI

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `funcTimestamp` is NULL

  - CUPTI_ERROR_NOT_INITIALIZED

  ###### Description

  This function registers a callback function to obtain timestamp of user's choice instead of using CUPTI provided timestamp. By default CUPTI uses different methods, based on the underlying platform, to retrieve the timestamp Linux and Android use clock_gettime(CLOCK_REALTIME, ..) Windows uses QueryPerformanceCounter() Mac uses mach_absolute_time() QNX uses ClockCycles() Timestamps retrieved using these methods are converted to nanosecond if needed before usage.

  The registration of timestamp callback should be done before any of the CUPTI activity kinds are enabled to make sure that all the records report the timestamp using the callback function registered through cuptiActivityRegisterTimestampCallback API.

  Changing the timestamp callback function in CUPTI through cuptiActivityRegisterTimestampCallback API in the middle of the profiling session can cause records generated prior to the change to report timestamps through previous timestamp method.

CUptiResult cuptiActivitySetAttribute ( CUpti_ActivityAttribute attr, size_t* valueSize, void* value )
  Write an activity API attribute.

  ###### Parameters

  `attr`
    The attribute to write
  `valueSize`
    The size, in bytes, of the value
  `value`
    The attribute value to write

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attr` is not an activity attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    Indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Write an activity API attribute.

CUptiResult cuptiComputeCapabilitySupported ( int major, int minor, int* support )
  Check support for a compute capability.

  ###### Parameters

  `major`
    The major revision number of the compute capability
  `minor`
    The minor revision number of the compute capability
  `support`
    Pointer to an integer to return the support status

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `support` is NULL

  ###### Description

  This function is used to check the support for a device based on it's compute capability. It sets the `support` when the compute capability is supported by the current version of CUPTI, and clears it otherwise. This version of CUPTI might not support all GPUs sharing the same compute capability. It is suggested to use API cuptiDeviceSupported which provides correct information.

  See also:

  cuptiDeviceSupported

CUptiResult cuptiDeviceSupported ( CUdevice dev, int* support )
  Check support for a compute device.

  ###### Parameters

  `dev`
    The device handle returned by CUDA Driver API cuDeviceGet
  `support`
    Pointer to an integer to return the support status

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `support` is NULL

  - CUPTI_ERROR_INVALID_DEVICE

    if `dev` is not a valid device

  ###### Description

  This function is used to check the support for a compute device. It sets the `support` when the device is supported by the current version of CUPTI, and clears it otherwise.

  See also:

  cuptiComputeCapabilitySupported

CUptiResult cuptiDeviceVirtualizationMode ( CUdevice dev, CUpti_DeviceVirtualizationMode* mode )
  Query the virtualization mode of the device.

  ###### Parameters

  `dev`
    The device handle returned by CUDA Driver API cuDeviceGet
  `mode`
    Pointer to an CUpti_DeviceVirtualizationMode to return the virtualization mode

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_DEVICE

    if `dev` is not a valid device

  - CUPTI_ERROR_INVALID_PARAMETER

    if `mode` is NULL

  ###### Description

  This function is used to query the virtualization mode of the CUDA device.

CUptiResult cuptiFinalize ( void )
  Detach CUPTI from the running process.

  ###### Description

  This API detaches the CUPTI from the running process. It destroys and cleans up all the resources associated with CUPTI in the current process. After CUPTI detaches from the process, the process will keep on running with no CUPTI attached to it. For safe operation of the API, it is recommended this API is invoked from the exit callsite of any of the CUDA Driver or Runtime API. Otherwise CUPTI client needs to make sure that required CUDA synchronization and CUPTI activity buffer flush is done before calling the API. Sample code showing the usage of the API in the cupti callback handler code:

      ‎    void CUPTIAPI
                cuptiCallbackHandler(void *userdata, CUpti_CallbackDomain domain,
                    CUpti_CallbackId cbid, void *cbdata)
                {
                    const CUpti_CallbackData *cbInfo = (CUpti_CallbackData *)cbdata;

                    // Take this code path when CUPTI detach is requested
                    if (detachCupti) {
                        switch(domain)
                        {
                        case CUPTI_CB_DOMAIN_RUNTIME_API:
                        case CUPTI_CB_DOMAIN_DRIVER_API:
                            if (cbInfo->callbackSite == CUPTI_API_EXIT) {
                                // call the CUPTI detach API
                                cuptiFinalize();
                            }
                            break;
                        default:
                            break;
                        }
                    }
                }

CUptiResult cuptiGetAutoBoostState ( CUcontext context, CUpti_ActivityAutoBoostState* state )
  Get auto boost state.

  ###### Parameters

  `context`
    A valid CUcontext.
  `state`
    A pointer to CUpti_ActivityAutoBoostState structure which contains the current state and the id of the process that has requested the current state

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `CUcontext` or `state` is NULL

  - CUPTI_ERROR_NOT_SUPPORTED

    Indicates that the device does not support auto boost

  - CUPTI_ERROR_UNKNOWN

    an internal error occurred

  ###### Description

  The profiling results can be inconsistent in case auto boost is enabled. CUPTI tries to disable auto boost while profiling. It can fail to disable in cases where user does not have the permissions or CUDA_AUTO_BOOST env variable is set. The function can be used to query whether auto boost is enabled.

CUptiResult cuptiGetContextId ( CUcontext context, uint32_t* contextId )
  Get the ID of a context.

  ###### Parameters

  `context`
    The context
  `contextId`
    Returns a process-unique ID for the context

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

    The context is NULL or not valid.

  - CUPTI_ERROR_INVALID_PARAMETER

    if `contextId` is NULL

  ###### Description

  Get the ID of a context.

CUptiResult cuptiGetDeviceId ( CUcontext context, uint32_t* deviceId )
  Get the ID of a device.

  ###### Parameters

  `context`
    The context, or NULL to indicate the current context.
  `deviceId`
    Returns the ID of the device that is current for the calling thread.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

    if unable to get device ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `deviceId` is NULL

  ###### Description

  If `context` is NULL, returns the ID of the device that contains the currently active context. If `context` is non-NULL, returns the ID of the device which contains that context. Operates in a similar manner to cudaGetDevice() or cuCtxGetDevice() but may be called from within callback functions.

CUptiResult cuptiGetGraphId ( CUgraph graph, uint32_t* pId )
  Get the unique ID of graph.

  ###### Parameters

  `graph`
    The graph.
  `pId`
    Returns the unique ID of the graph

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `graph` is NULL

  ###### Description

  Returns the unique ID of CUDA graph.

CUptiResult cuptiGetGraphNodeId ( CUgraphNode node, uint64_t* nodeId )
  Get the unique ID of a graph node.

  ###### Parameters

  `node`
    The graph node.
  `nodeId`
    Returns the unique ID of the node

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `node` is NULL

  ###### Description

  Returns the unique ID of the CUDA graph node.

CUptiResult cuptiGetLastError ( void )
  Returns the last error from a cupti call or callback.

  ###### Description

  Returns the last error that has been produced by any of the cupti api calls or the callback in the same host thread and resets it to CUPTI_SUCCESS.

CUptiResult cuptiGetStreamId ( CUcontext context, CUstream stream, uint32_t* streamId )
  Get the ID of a stream.

  ###### Parameters

  `context`
    If non-NULL then the stream is checked to ensure that it belongs to this context. Typically this parameter should be null.
  `stream`
    The stream
  `streamId`
    Returns a context-unique ID for the stream

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_STREAM

    if unable to get stream ID, or if `context` is non-NULL and `stream` does not belong to the context

  - CUPTI_ERROR_INVALID_PARAMETER

    if `streamId` is NULL

  ###### Description

  Get the ID of a stream. The stream ID is unique within a context (i.e. all streams within a context will have unique stream IDs).

  **DEPRECATED** This method is deprecated as of CUDA 8.0. Use method cuptiGetStreamIdEx instead.

CUptiResult cuptiGetStreamIdEx ( CUcontext context, CUstream stream, uint8_t perThreadStream, uint32_t* streamId )
  Get the ID of a stream.

  ###### Parameters

  `context`
    If non-NULL then the stream is checked to ensure that it belongs to this context. Typically this parameter should be null.
  `stream`
    The stream
  `perThreadStream`
    Flag to indicate if program is compiled for per-thread streams
  `streamId`
    Returns a context-unique ID for the stream

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_STREAM

    if unable to get stream ID, or if `context` is non-NULL and `stream` does not belong to the context

  - CUPTI_ERROR_INVALID_PARAMETER

    if `streamId` is NULL

  ###### Description

  Get the ID of a stream. The stream ID is unique within a context (i.e. all streams within a context will have unique stream IDs).

CUptiResult cuptiGetThreadIdType ( CUpti_ActivityThreadIdType* type )
  Get the thread-id type.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `type` is NULL

  ###### Description

  Returns the thread-id type used in CUPTI

CUptiResult cuptiGetTimestamp ( uint64_t* timestamp )
  Get the CUPTI timestamp.

  ###### Parameters

  `timestamp`
    Returns the CUPTI timestamp

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `timestamp` is NULL

  ###### Description

  Returns a timestamp normalized to correspond with the start and end timestamps reported in the CUPTI activity records. The timestamp is reported in nanoseconds.

CUptiResult cuptiSetThreadIdType ( CUpti_ActivityThreadIdType type )
  Set the thread-id type.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_SUPPORTED

    if `type` is not supported on the platform

  ###### Description

  CUPTI uses the method corresponding to set type to generate the thread-id. See enum CUpti_ActivityThreadIdType for the list of methods. Activity records having thread-id field contain the same value. Thread id type must not be changed during the profiling session to avoid thread-id value mismatch across activity records.

### 5.4. CUPTI Callback API

Functions, types, and enums that implement the CUPTI Callback API.

#### Classes

struct
CUpti_CallbackData
  Data passed into a runtime or driver API callback function.
struct
CUpti_GraphData
  CUDA graphs data passed into a resource callback function.
struct
CUpti_ModuleResourceData
  Module data passed into a resource callback function.
struct
CUpti_NvtxData
  Data passed into a NVTX callback function.
struct
CUpti_ResourceData
  Data passed into a resource callback function.
struct
CUpti_SynchronizeData
  Data passed into a synchronize callback function.

#### Typedefs

typedef void ( *CUpti_CallbackFunc )( void* userdata, CUpti_CallbackDomain domain, CUpti_CallbackId cbid, const void* cbdata )
  Function type for a callback.
typedef uint32_t CUpti_CallbackId
  An ID for a driver API, runtime API, resource or synchronization callback.
typedef CUpti_CallbackDomain* CUpti_DomainTable
  Pointer to an array of callback domains.
typedef CUpti_Subscriber_st * CUpti_SubscriberHandle
  A callback subscriber.

#### Enumerations

enum CUpti_ApiCallbackSite
  Specifies the point in an API call that a callback is issued.
enum CUpti_CallbackDomain
  Callback domains.
enum CUpti_CallbackIdResource
  Callback IDs for resource domain.
enum CUpti_CallbackIdSync
  Callback IDs for synchronization domain.

#### Functions

CUptiResult cuptiEnableAllDomains ( uint32_t enable, CUpti_SubscriberHandle subscriber )
  Enable or disable all callbacks in all domains.
CUptiResult cuptiEnableCallback ( uint32_t enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain, CUpti_CallbackId cbid )
  Enable or disabled callbacks for a specific domain and callback ID.
CUptiResult cuptiEnableDomain ( uint32_t enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain )
  Enable or disabled all callbacks for a specific domain.
CUptiResult cuptiGetCallbackName ( CUpti_CallbackDomain domain, uint32_t cbid, const char** name )
  Get the name of a callback for a specific domain and callback ID.
CUptiResult cuptiGetCallbackState ( uint32_t* enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain, CUpti_CallbackId cbid )
  Get the current enabled/disabled state of a callback for a specific domain and function ID.
CUptiResult cuptiSubscribe ( CUpti_SubscriberHandle* subscriber, CUpti_CallbackFunc callback, void* userdata )
  Initialize a callback subscriber with a callback function and user data.
CUptiResult cuptiSupportedDomains ( size_t* domainCount, CUpti_DomainTable* domainTable )
  Get the available callback domains.
CUptiResult cuptiUnsubscribe ( CUpti_SubscriberHandle subscriber )
  Unregister a callback subscriber.

#### Typedefs

void ( *CUpti_CallbackFunc )( void* userdata, CUpti_CallbackDomain domain, CUpti_CallbackId cbid, const void* cbdata )

  Function type for a callback. Function type for a callback. The type of the data passed to the callback in `cbdata` depends on the `domain`. If `domain` is CUPTI_CB_DOMAIN_DRIVER_API or CUPTI_CB_DOMAIN_RUNTIME_API the type of `cbdata` will be CUpti_CallbackData. If `domain` is CUPTI_CB_DOMAIN_RESOURCE the type of `cbdata` will be CUpti_ResourceData. If `domain` is CUPTI_CB_DOMAIN_SYNCHRONIZE the type of `cbdata` will be CUpti_SynchronizeData. If `domain` is CUPTI_CB_DOMAIN_NVTX the type of `cbdata` will be CUpti_NvtxData.

###### Parameters

`userdata`
  User data supplied at subscription of the callback
`CUpti_CallbackDomain domain`
`CUpti_CallbackId cbid`
`cbdata`
  Data passed to the callback.

typedef uint32_t CUpti_CallbackId

  An ID for a driver API, runtime API, resource or synchronization callback. An ID for a driver API, runtime API, resource or synchronization callback. Within a driver API callback this should be interpreted as a CUpti_driver_api_trace_cbid value (these values are defined in cupti_driver_cbid.h). Within a runtime API callback this should be interpreted as a CUpti_runtime_api_trace_cbid value (these values are defined in cupti_runtime_cbid.h). Within a resource API callback this should be interpreted as a CUpti_CallbackIdResource value. Within a synchronize API callback this should be interpreted as a CUpti_CallbackIdSync value.

typedef CUpti_CallbackDomain* CUpti_DomainTable

  Pointer to an array of callback domains.

typedef CUpti_Subscriber_st * CUpti_SubscriberHandle

  A callback subscriber.

#### Enumerations

enum CUpti_ApiCallbackSite

  Specifies the point in an API call that a callback is issued. This value is communicated to the callback function via CUpti_CallbackData::callbackSite.

  ###### Values

  CUPTI_API_ENTER = 0
    The callback is at the entry of the API call.
  CUPTI_API_EXIT = 1
    The callback is at the exit of the API call.
  CUPTI_API_CBSITE_FORCE_INT = 0x7fffffff
enum CUpti_CallbackDomain

  Callback domains. Each domain represents callback points for a group of related API functions or CUDA driver activity.

  ###### Values

  CUPTI_CB_DOMAIN_INVALID = 0
    Invalid domain.
  CUPTI_CB_DOMAIN_DRIVER_API = 1
    Domain containing callback points for all driver API functions.
  CUPTI_CB_DOMAIN_RUNTIME_API = 2
    Domain containing callback points for all runtime API functions.
  CUPTI_CB_DOMAIN_RESOURCE = 3
    Domain containing callback points for CUDA resource tracking.
  CUPTI_CB_DOMAIN_SYNCHRONIZE = 4
    Domain containing callback points for CUDA synchronization.
  CUPTI_CB_DOMAIN_NVTX = 5
    Domain containing callback points for NVTX API functions.
  CUPTI_CB_DOMAIN_SIZE = 6
  CUPTI_CB_DOMAIN_FORCE_INT = 0x7fffffff
enum CUpti_CallbackIdResource

  Callback IDs for resource domain, CUPTI_CB_DOMAIN_RESOURCE. This value is communicated to the callback function via the `cbid` parameter.

  ###### Values

  CUPTI_CBID_RESOURCE_INVALID = 0
    Invalid resource callback ID.
  CUPTI_CBID_RESOURCE_CONTEXT_CREATED = 1
    A new context has been created.
  CUPTI_CBID_RESOURCE_CONTEXT_DESTROY_STARTING = 2
    A context is about to be destroyed.
  CUPTI_CBID_RESOURCE_STREAM_CREATED = 3
    A new stream has been created.
  CUPTI_CBID_RESOURCE_STREAM_DESTROY_STARTING = 4
    A stream is about to be destroyed.
  CUPTI_CBID_RESOURCE_CU_INIT_FINISHED = 5
    The driver has finished initializing.
  CUPTI_CBID_RESOURCE_MODULE_LOADED = 6
    A module has been loaded.
  CUPTI_CBID_RESOURCE_MODULE_UNLOAD_STARTING = 7
    A module is about to be unloaded.
  CUPTI_CBID_RESOURCE_MODULE_PROFILED = 8
    The current module which is being profiled.
  CUPTI_CBID_RESOURCE_GRAPH_CREATED = 9
    CUDA graph has been created.
  CUPTI_CBID_RESOURCE_GRAPH_DESTROY_STARTING = 10
    CUDA graph is about to be destroyed.
  CUPTI_CBID_RESOURCE_GRAPH_CLONED = 11
    CUDA graph is cloned.
  CUPTI_CBID_RESOURCE_GRAPHNODE_CREATE_STARTING = 12
    CUDA graph node is about to be created
  CUPTI_CBID_RESOURCE_GRAPHNODE_CREATED = 13
    CUDA graph node is created.
  CUPTI_CBID_RESOURCE_GRAPHNODE_DESTROY_STARTING = 14
    CUDA graph node is about to be destroyed.
  CUPTI_CBID_RESOURCE_GRAPHNODE_DEPENDENCY_CREATED = 15
    Dependency on a CUDA graph node is created.
  CUPTI_CBID_RESOURCE_GRAPHNODE_DEPENDENCY_DESTROY_STARTING = 16
    Dependency on a CUDA graph node is destroyed.
  CUPTI_CBID_RESOURCE_GRAPHEXEC_CREATE_STARTING = 17
    An executable CUDA graph is about to be created.
  CUPTI_CBID_RESOURCE_GRAPHEXEC_CREATED = 18
    An executable CUDA graph is created.
  CUPTI_CBID_RESOURCE_GRAPHEXEC_DESTROY_STARTING = 19
    An executable CUDA graph is about to be destroyed.
  CUPTI_CBID_RESOURCE_GRAPHNODE_CLONED = 20
    CUDA graph node is cloned.
  CUPTI_CBID_RESOURCE_SIZE
  CUPTI_CBID_RESOURCE_FORCE_INT = 0x7fffffff
enum CUpti_CallbackIdSync

  Callback IDs for synchronization domain, CUPTI_CB_DOMAIN_SYNCHRONIZE. This value is communicated to the callback function via the `cbid` parameter.

  ###### Values

  CUPTI_CBID_SYNCHRONIZE_INVALID = 0
    Invalid synchronize callback ID.
  CUPTI_CBID_SYNCHRONIZE_STREAM_SYNCHRONIZED = 1
    Stream synchronization has completed for the stream.
  CUPTI_CBID_SYNCHRONIZE_CONTEXT_SYNCHRONIZED = 2
    Context synchronization has completed for the context.
  CUPTI_CBID_SYNCHRONIZE_SIZE
  CUPTI_CBID_SYNCHRONIZE_FORCE_INT = 0x7fffffff

#### Functions

CUptiResult cuptiEnableAllDomains ( uint32_t enable, CUpti_SubscriberHandle subscriber )
  Enable or disable all callbacks in all domains.

  ###### Parameters

  `enable`
    New enable state for all callbacks in all domain. Zero disables all callbacks, non-zero enables all callbacks.
  `subscriber`
    - Handle to callback subscription

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialized CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `subscriber` is invalid

  ###### Description

  Enable or disable all callbacks in all domains.

  Note:

  Thread-safety: a subscriber must serialize access to cuptiGetCallbackState, cuptiEnableCallback, cuptiEnableDomain, and cuptiEnableAllDomains. For example, if cuptiGetCallbackState(sub, d, *) and cuptiEnableAllDomains(sub) are called concurrently, the results are undefined.

CUptiResult cuptiEnableCallback ( uint32_t enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain, CUpti_CallbackId cbid )
  Enable or disabled callbacks for a specific domain and callback ID.

  ###### Parameters

  `enable`
    New enable state for the callback. Zero disables the callback, non-zero enables the callback.
  `subscriber`
    - Handle to callback subscription
  `domain`
    The domain of the callback
  `cbid`
    The ID of the callback

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialized CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `subscriber`, `domain` or `cbid` is invalid.

  ###### Description

  Enable or disabled callbacks for a subscriber for a specific domain and callback ID.

  Note:

  Thread-safety: a subscriber must serialize access to cuptiGetCallbackState, cuptiEnableCallback, cuptiEnableDomain, and cuptiEnableAllDomains. For example, if cuptiGetCallbackState(sub, d, c) and cuptiEnableCallback(sub, d, c) are called concurrently, the results are undefined.

CUptiResult cuptiEnableDomain ( uint32_t enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain )
  Enable or disabled all callbacks for a specific domain.

  ###### Parameters

  `enable`
    New enable state for all callbacks in the domain. Zero disables all callbacks, non-zero enables all callbacks.
  `subscriber`
    - Handle to callback subscription
  `domain`
    The domain of the callback

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialized CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `subscriber` or `domain` is invalid

  ###### Description

  Enable or disabled all callbacks for a specific domain.

  Note:

  Thread-safety: a subscriber must serialize access to cuptiGetCallbackState, cuptiEnableCallback, cuptiEnableDomain, and cuptiEnableAllDomains. For example, if cuptiGetCallbackEnabled(sub, d, *) and cuptiEnableDomain(sub, d) are called concurrently, the results are undefined.

CUptiResult cuptiGetCallbackName ( CUpti_CallbackDomain domain, uint32_t cbid, const char** name )
  Get the name of a callback for a specific domain and callback ID.

  ###### Parameters

  `domain`
    The domain of the callback
  `cbid`
    The ID of the callback
  `name`
    Returns pointer to the name string on success, NULL otherwise

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_INVALID_PARAMETER

    if `name` is NULL, or if `domain` or `cbid` is invalid.

  ###### Description

  Returns a pointer to the name c_string in `**name`.

  Note:

  Names are available only for the DRIVER and RUNTIME domains.

CUptiResult cuptiGetCallbackState ( uint32_t* enable, CUpti_SubscriberHandle subscriber, CUpti_CallbackDomain domain, CUpti_CallbackId cbid )
  Get the current enabled/disabled state of a callback for a specific domain and function ID.

  ###### Parameters

  `enable`
    Returns non-zero if callback enabled, zero if not enabled
  `subscriber`
    Handle to the initialize subscriber
  `domain`
    The domain of the callback
  `cbid`
    The ID of the callback

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialized CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `enabled` is NULL, or if `subscriber`, `domain` or `cbid` is invalid.

  ###### Description

  Returns non-zero in `*enable` if the callback for a domain and callback ID is enabled, and zero if not enabled.

  Note:

  Thread-safety: a subscriber must serialize access to cuptiGetCallbackState, cuptiEnableCallback, cuptiEnableDomain, and cuptiEnableAllDomains. For example, if cuptiGetCallbackState(sub, d, c) and cuptiEnableCallback(sub, d, c) are called concurrently, the results are undefined.

CUptiResult cuptiSubscribe ( CUpti_SubscriberHandle* subscriber, CUpti_CallbackFunc callback, void* userdata )
  Initialize a callback subscriber with a callback function and user data.

  ###### Parameters

  `subscriber`
    Returns handle to initialize subscriber
  `callback`
    The callback function
  `userdata`
    A pointer to user data. This data will be passed to the callback function via the `userdata` paramater.

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialize CUPTI

  - CUPTI_ERROR_MULTIPLE_SUBSCRIBERS_NOT_SUPPORTED

    if there is already a CUPTI subscriber

  - CUPTI_ERROR_INVALID_PARAMETER

    if `subscriber` is NULL

  ###### Description

  Initializes a callback subscriber with a callback function and (optionally) a pointer to user data. The returned subscriber handle can be used to enable and disable the callback for specific domains and callback IDs.

  Note:

  - Only a single subscriber can be registered at a time. To ensure that no other CUPTI client interrupts the profiling session, it's the responsibility of all the CUPTI clients to call this function before starting the profling session. In case profiling session is already started by another CUPTI client, this function returns the error code CUPTI_ERROR_MULTIPLE_SUBSCRIBERS_NOT_SUPPORTED. Note that this function returns the same error when application is launched using NVIDIA tools like nvprof, Visual Profiler, Nsight Systems, Nsight Compute, cuda-gdb and cuda-memcheck.

  - This function does not enable any callbacks.

  - Thread-safety: this function is thread safe.

CUptiResult cuptiSupportedDomains ( size_t* domainCount, CUpti_DomainTable* domainTable )
  Get the available callback domains.

  ###### Parameters

  `domainCount`
    Returns number of callback domains
  `domainTable`
    Returns pointer to array of available callback domains

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialize CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `domainCount` or `domainTable` are NULL

  ###### Description

  Returns in `*domainTable` an array of size `*domainCount` of all the available callback domains.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiUnsubscribe ( CUpti_SubscriberHandle subscriber )
  Unregister a callback subscriber.

  ###### Parameters

  `subscriber`
    Handle to the initialize subscriber

  ###### Returns

  - CUPTI_SUCCESS

    on success

  - CUPTI_ERROR_NOT_INITIALIZED

    if unable to initialized CUPTI

  - CUPTI_ERROR_INVALID_PARAMETER

    if `subscriber` is NULL or not initialized

  ###### Description

  Removes a callback subscriber so that no future callbacks will be issued to that subscriber.

  Note:

  Thread-safety: this function is thread safe.

### 5.5. CUPTI Event API

Functions, types, and enums that implement the CUPTI Event API.

Note:

CUPTI event API from the header cupti_events.h are not supported on devices with compute capability 7.5 and higher (i.e. Turing and later GPU architectures). These API will be deprecated in a future CUDA release. These are replaced by Profiling API in the header cupti_profiler_target.h and Perfworks metrics API in the headers nvperf_host.h and nvperf_target.h which are supported on devices with compute capability 7.0 and higher (i.e. Volta and later GPU architectures).

#### Classes

struct
CUpti_EventGroupSet
  A set of event groups.
struct
CUpti_EventGroupSets
  A set of event group sets.

#### Defines

#define CUPTI_EVENT_INVALID
  The value that indicates the event value is invalid.
#define CUPTI_EVENT_OVERFLOW
  The overflow value for a CUPTI event.

#### Typedefs

typedef uint32_t CUpti_EventDomainID
  ID for an event domain.
typedef void * CUpti_EventGroup
  A group of events.
typedef uint32_t CUpti_EventID
  ID for an event.
typedef void ( *CUpti_KernelReplayUpdateFunc )( const char* kernelName, int numReplaysDone, void* customData )
  Function type for getting updates on kernel replay.

#### Enumerations

enum CUpti_DeviceAttribute
  Device attributes.
enum CUpti_DeviceAttributeDeviceClass
  Device class.
enum CUpti_EventAttribute
  Event attributes.
enum CUpti_EventCategory
  An event category.
enum CUpti_EventCollectionMethod
  The collection method used for an event.
enum CUpti_EventCollectionMode
  Event collection modes.
enum CUpti_EventDomainAttribute
  Event domain attributes.
enum CUpti_EventGroupAttribute
  Event group attributes.
enum CUpti_EventProfilingScope
  Profiling scope for event.
enum CUpti_ReadEventFlags
  Flags for cuptiEventGroupReadEvent an cuptiEventGroupReadAllEvents.

#### Functions

CUptiResult cuptiDeviceEnumEventDomains ( CUdevice device, size_t* arraySizeBytes, CUpti_EventDomainID* domainArray )
  Get the event domains for a device.
CUptiResult cuptiDeviceGetAttribute ( CUdevice device, CUpti_DeviceAttribute attrib, size_t* valueSize, void* value )
  Read a device attribute.
CUptiResult cuptiDeviceGetEventDomainAttribute ( CUdevice device, CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t* valueSize, void* value )
  Read an event domain attribute.
CUptiResult cuptiDeviceGetNumEventDomains ( CUdevice device, uint32_t* numDomains )
  Get the number of domains for a device.
CUptiResult cuptiDeviceGetTimestamp ( CUcontext context, uint64_t* timestamp )
  Read a device timestamp.
CUptiResult cuptiDisableKernelReplayMode ( CUcontext context )
  Disable kernel replay mode.
CUptiResult cuptiEnableKernelReplayMode ( CUcontext context )
  Enable kernel replay mode.
CUptiResult cuptiEnumEventDomains ( size_t* arraySizeBytes, CUpti_EventDomainID* domainArray )
  Get the event domains available on any device.
CUptiResult cuptiEventDomainEnumEvents ( CUpti_EventDomainID eventDomain, size_t* arraySizeBytes, CUpti_EventID* eventArray )
  Get the events in a domain.
CUptiResult cuptiEventDomainGetAttribute ( CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t* valueSize, void* value )
  Read an event domain attribute.
CUptiResult cuptiEventDomainGetNumEvents ( CUpti_EventDomainID eventDomain, uint32_t* numEvents )
  Get number of events in a domain.
CUptiResult cuptiEventGetAttribute ( CUpti_EventID event, CUpti_EventAttribute attrib, size_t* valueSize, void* value )
  Get an event attribute.
CUptiResult cuptiEventGetIdFromName ( CUdevice device, const char* eventName, CUpti_EventID* event )
  Find an event by name.
CUptiResult cuptiEventGroupAddEvent ( CUpti_EventGroup eventGroup, CUpti_EventID event )
  Add an event to an event group.
CUptiResult cuptiEventGroupCreate ( CUcontext context, CUpti_EventGroup* eventGroup, uint32_t flags )
  Create a new event group for a context.
CUptiResult cuptiEventGroupDestroy ( CUpti_EventGroup eventGroup )
  Destroy an event group.
CUptiResult cuptiEventGroupDisable ( CUpti_EventGroup eventGroup )
  Disable an event group.
CUptiResult cuptiEventGroupEnable ( CUpti_EventGroup eventGroup )
  Enable an event group.
CUptiResult cuptiEventGroupGetAttribute ( CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t* valueSize, void* value )
  Read an event group attribute.
CUptiResult cuptiEventGroupReadAllEvents ( CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, size_t* eventValueBufferSizeBytes, uint64_t* eventValueBuffer, size_t* eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t* numEventIdsRead )
  Read the values for all the events in an event group.
CUptiResult cuptiEventGroupReadEvent ( CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, CUpti_EventID event, size_t* eventValueBufferSizeBytes, uint64_t* eventValueBuffer )
  Read the value for an event in an event group.
CUptiResult cuptiEventGroupRemoveAllEvents ( CUpti_EventGroup eventGroup )
  Remove all events from an event group.
CUptiResult cuptiEventGroupRemoveEvent ( CUpti_EventGroup eventGroup, CUpti_EventID event )
  Remove an event from an event group.
CUptiResult cuptiEventGroupResetAllEvents ( CUpti_EventGroup eventGroup )
  Zero all the event counts in an event group.
CUptiResult cuptiEventGroupSetAttribute ( CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t valueSize, void* value )
  Write an event group attribute.
CUptiResult cuptiEventGroupSetDisable ( CUpti_EventGroupSet* eventGroupSet )
  Disable an event group set.
CUptiResult cuptiEventGroupSetEnable ( CUpti_EventGroupSet* eventGroupSet )
  Enable an event group set.
CUptiResult cuptiEventGroupSetsCreate ( CUcontext context, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, CUpti_EventGroupSets** eventGroupPasses )
  For a set of events, get the grouping that indicates the number of passes and the event groups necessary to collect the events.
CUptiResult cuptiEventGroupSetsDestroy ( CUpti_EventGroupSets* eventGroupSets )
  Destroy a event group sets object.
CUptiResult cuptiGetNumEventDomains ( uint32_t* numDomains )
  Get the number of event domains available on any device.
CUptiResult cuptiKernelReplaySubscribeUpdate ( CUpti_KernelReplayUpdateFunc updateFunc, void* customData )
  Subscribe to kernel replay updates.
CUptiResult cuptiSetEventCollectionMode ( CUcontext context, CUpti_EventCollectionMode mode )
  Set the event collection mode.

#### Defines

#define CUPTI_EVENT_INVALID

  ###### Value

  ((uint64_t)0xFFFFFFFFFFFFFFFEULL)

#define CUPTI_EVENT_OVERFLOW

  The CUPTI event value that indicates an overflow.

  ###### Value

  ((uint64_t)0xFFFFFFFFFFFFFFFFULL)

#### Typedefs

typedef uint32_t CUpti_EventDomainID

  ID for an event domain. ID for an event domain. An event domain represents a group of related events. A device may have multiple instances of a domain, indicating that the device can simultaneously record multiple instances of each event within that domain.

typedef void * CUpti_EventGroup

  A group of events. An event group is a collection of events that are managed together. All events in an event group must belong to the same domain.

typedef uint32_t CUpti_EventID

  ID for an event. An event represents a countable activity, action, or occurrence on the device.

void ( *CUpti_KernelReplayUpdateFunc )( const char* kernelName, int numReplaysDone, void* customData )

  Function type for getting updates on kernel replay.

###### Parameters

`kernelName`
  The mangled kernel name
`int numReplaysDone`
`customData`
  Pointer of any custom data passed in when subscribing

#### Enumerations

enum CUpti_DeviceAttribute

  CUPTI device attributes. These attributes can be read using cuptiDeviceGetAttribute.

  ###### Values

  CUPTI_DEVICE_ATTR_MAX_EVENT_ID = 1
    Number of event IDs for a device. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_MAX_EVENT_DOMAIN_ID = 2
    Number of event domain IDs for a device. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_GLOBAL_MEMORY_BANDWIDTH = 3
    Get global memory bandwidth in Kbytes/sec. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_INSTRUCTION_PER_CYCLE = 4
    Get theoretical maximum number of instructions per cycle. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_INSTRUCTION_THROUGHPUT_SINGLE_PRECISION = 5
    Get theoretical maximum number of single precision instructions that can be executed per second. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_FRAME_BUFFERS = 6
    Get number of frame buffers for device. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_LINK_RATE = 7
    Get PCIE link rate in Mega bits/sec for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_LINK_WIDTH = 8
    Get PCIE link width for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_GEN = 9
    Get PCIE generation for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_DEVICE_CLASS = 10
    Get the class for the device. Value is a CUpti_DeviceAttributeDeviceClass.
  CUPTI_DEVICE_ATTR_FLOP_SP_PER_CYCLE = 11
    Get the peak single precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_FLOP_DP_PER_CYCLE = 12
    Get the peak double precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_L2_UNITS = 13
    Get number of L2 units. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_SHARED = 14
    Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_SHARED preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_L1 = 15
    Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_L1 preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_EQUAL = 16
    Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_EQUAL preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_FLOP_HP_PER_CYCLE = 17
    Get the peak half precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_NVLINK_PRESENT = 18
    Check if Nvlink is connected to device. Returns 1, if at least one Nvlink is connected to the device, returns 0 otherwise. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_GPU_CPU_NVLINK_BW = 19
    Check if Nvlink is present between GPU and CPU. Returns Bandwidth, in Bytes/sec, if Nvlink is present, returns 0 otherwise. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_NVSWITCH_PRESENT = 20
    Check if NVSwitch is present in the underlying topology. Returns 1, if present, returns 0 otherwise. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_FORCE_INT = 0x7fffffff
enum CUpti_DeviceAttributeDeviceClass

  Enumeration of device classes for device attribute CUPTI_DEVICE_ATTR_DEVICE_CLASS.

  ###### Values

  CUPTI_DEVICE_ATTR_DEVICE_CLASS_TESLA = 0
  CUPTI_DEVICE_ATTR_DEVICE_CLASS_QUADRO = 1
  CUPTI_DEVICE_ATTR_DEVICE_CLASS_GEFORCE = 2
  CUPTI_DEVICE_ATTR_DEVICE_CLASS_TEGRA = 3
enum CUpti_EventAttribute

  Event attributes. These attributes can be read using cuptiEventGetAttribute.

  ###### Values

  CUPTI_EVENT_ATTR_NAME = 0
    Event name. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_SHORT_DESCRIPTION = 1
    Short description of event. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_LONG_DESCRIPTION = 2
    Long description of event. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_CATEGORY = 3
    Category of event. Value is CUpti_EventCategory.
  CUPTI_EVENT_ATTR_PROFILING_SCOPE = 5
    Profiling scope of the events. It can be either device or context or both. Value is a CUpti_EventProfilingScope.
  CUPTI_EVENT_ATTR_FORCE_INT = 0x7fffffff
enum CUpti_EventCategory

  Each event is assigned to a category that represents the general type of the event. A event's category is accessed using cuptiEventGetAttribute and the CUPTI_EVENT_ATTR_CATEGORY attribute.

  ###### Values

  CUPTI_EVENT_CATEGORY_INSTRUCTION = 0
    An instruction related event.
  CUPTI_EVENT_CATEGORY_MEMORY = 1
    A memory related event.
  CUPTI_EVENT_CATEGORY_CACHE = 2
    A cache related event.
  CUPTI_EVENT_CATEGORY_PROFILE_TRIGGER = 3
    A profile-trigger event.
  CUPTI_EVENT_CATEGORY_SYSTEM = 4
    A system event.
  CUPTI_EVENT_CATEGORY_FORCE_INT = 0x7fffffff
enum CUpti_EventCollectionMethod

  The collection method indicates how an event is collected.

  ###### Values

  CUPTI_EVENT_COLLECTION_METHOD_PM = 0
    Event is collected using a hardware global performance monitor.
  CUPTI_EVENT_COLLECTION_METHOD_SM = 1
    Event is collected using a hardware SM performance monitor.
  CUPTI_EVENT_COLLECTION_METHOD_INSTRUMENTED = 2
    Event is collected using software instrumentation.
  CUPTI_EVENT_COLLECTION_METHOD_NVLINK_TC = 3
    Event is collected using NvLink throughput counter method.
  CUPTI_EVENT_COLLECTION_METHOD_FORCE_INT = 0x7fffffff
enum CUpti_EventCollectionMode

  The event collection mode determines the period over which the events within the enabled event groups will be collected.

  ###### Values

  CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS = 0
    Events are collected for the entire duration between the cuptiEventGroupEnable and cuptiEventGroupDisable calls. Event values are reset when the events are read. For CUDA toolkit v6.0 and older this was the default mode.
  CUPTI_EVENT_COLLECTION_MODE_KERNEL = 1
    Events are collected only for the durations of kernel executions that occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls. Event collection begins when a kernel execution begins, and stops when kernel execution completes. Event values are reset to zero when each kernel execution begins. If multiple kernel executions occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls then the event values must be read after each kernel launch if those events need to be associated with the specific kernel launch. Note that collection in this mode may significantly change the overall performance characteristics of the application because kernel executions that occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls are serialized on the GPU. This is the default mode from CUDA toolkit v6.5
  CUPTI_EVENT_COLLECTION_MODE_FORCE_INT = 0x7fffffff
enum CUpti_EventDomainAttribute

  Event domain attributes. Except where noted, all the attributes can be read using either cuptiDeviceGetEventDomainAttribute or cuptiEventDomainGetAttribute.

  ###### Values

  CUPTI_EVENT_DOMAIN_ATTR_NAME = 0
    Event domain name. Value is a null terminated const c-string.
  CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT = 1
    Number of instances of the domain for which event counts will be collected. The domain may have additional instances that cannot be profiled (see CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT). Can be read only with cuptiDeviceGetEventDomainAttribute. Value is a uint32_t.
  CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT = 3
    Total number of instances of the domain, including instances that cannot be profiled. Use CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT to get the number of instances that can be profiled. Can be read only with cuptiDeviceGetEventDomainAttribute. Value is a uint32_t.
  CUPTI_EVENT_DOMAIN_ATTR_COLLECTION_METHOD = 4
    Collection method used for events contained in the event domain. Value is a CUpti_EventCollectionMethod.
  CUPTI_EVENT_DOMAIN_ATTR_FORCE_INT = 0x7fffffff
enum CUpti_EventGroupAttribute

  Event group attributes. These attributes can be read using cuptiEventGroupGetAttribute. Attributes marked [rw] can also be written using cuptiEventGroupSetAttribute.

  ###### Values

  CUPTI_EVENT_GROUP_ATTR_EVENT_DOMAIN_ID = 0
    The domain to which the event group is bound. This attribute is set when the first event is added to the group. Value is a CUpti_EventDomainID.
  CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES = 1
    [rw] Profile all the instances of the domain for this eventgroup. This feature can be used to get load balancing across all instances of a domain. Value is an integer.
  CUPTI_EVENT_GROUP_ATTR_USER_DATA = 2
    [rw] Reserved for user data.
  CUPTI_EVENT_GROUP_ATTR_NUM_EVENTS = 3
    Number of events in the group. Value is a uint32_t.
  CUPTI_EVENT_GROUP_ATTR_EVENTS = 4
    Enumerates events in the group. Value is a pointer to buffer of size sizeof(CUpti_EventID) * num_of_events in the eventgroup. num_of_events can be queried using CUPTI_EVENT_GROUP_ATTR_NUM_EVENTS.
  CUPTI_EVENT_GROUP_ATTR_INSTANCE_COUNT = 5
    Number of instances of the domain bound to this event group that will be counted. Value is a uint32_t.
  CUPTI_EVENT_GROUP_ATTR_PROFILING_SCOPE = 6
    Event group scope can be set to CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT for an eventGroup, before adding any event. Sets the scope of eventgroup as CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT when the scope of the events that will be added is CUPTI_EVENT_PROFILING_SCOPE_BOTH. If profiling scope of event is either CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT then setting this attribute will not affect the default scope. It is not allowed to add events of different scope to same eventgroup. Value is a uint32_t.
  CUPTI_EVENT_GROUP_ATTR_FORCE_INT = 0x7fffffff
enum CUpti_EventProfilingScope

  Profiling scope of event indicates if the event can be collected at context scope or device scope or both i.e. it can be collected at any of context or device scope.

  ###### Values

  CUPTI_EVENT_PROFILING_SCOPE_CONTEXT = 0
    Event is collected at context scope.
  CUPTI_EVENT_PROFILING_SCOPE_DEVICE = 1
    Event is collected at device scope.
  CUPTI_EVENT_PROFILING_SCOPE_BOTH = 2
    Event can be collected at device or context scope. The scope can be set using cuptiEventGroupSetAttribute API.
  CUPTI_EVENT_PROFILING_SCOPE_FORCE_INT = 0x7fffffff
enum CUpti_ReadEventFlags

  Flags for cuptiEventGroupReadEvent an cuptiEventGroupReadAllEvents.

  ###### Values

  CUPTI_EVENT_READ_FLAG_NONE = 0
    No flags.
  CUPTI_EVENT_READ_FLAG_FORCE_INT = 0x7fffffff

#### Functions

CUptiResult cuptiDeviceEnumEventDomains ( CUdevice device, size_t* arraySizeBytes, CUpti_EventDomainID* domainArray )
  Get the event domains for a device.

  ###### Parameters

  `device`
    The CUDA device
  `arraySizeBytes`
    The size of `domainArray` in bytes, and returns the number of bytes written to `domainArray`
  `domainArray`
    Returns the IDs of the event domains for the device

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `arraySizeBytes` or `domainArray` are NULL

  ###### Description

  Returns the event domains IDs in `domainArray` for a device. The size of the `domainArray` buffer is given by `*arraySizeBytes`. The size of the `domainArray` buffer must be at least `numdomains` * sizeof(CUpti_EventDomainID) or else all domains will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `domainArray`.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiDeviceGetAttribute ( CUdevice device, CUpti_DeviceAttribute attrib, size_t* valueSize, void* value )
  Read a device attribute.

  ###### Parameters

  `device`
    The CUDA device
  `attrib`
    The attribute to read
  `valueSize`
    Size of buffer pointed by the value, and returns the number of bytes written to `value`
  `value`
    Returns the value of the attribute

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not a device attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Read a device attribute and return it in `*value`.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiDeviceGetEventDomainAttribute ( CUdevice device, CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t* valueSize, void* value )
  Read an event domain attribute.

  ###### Parameters

  `device`
    The CUDA device
  `eventDomain`
    ID of the event domain
  `attrib`
    The event domain attribute to read
  `valueSize`
    The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  `value`
    Returns the attribute's value

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not an event domain attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Returns an event domain attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

  If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiDeviceGetNumEventDomains ( CUdevice device, uint32_t* numDomains )
  Get the number of domains for a device.

  ###### Parameters

  `device`
    The CUDA device
  `numDomains`
    Returns the number of domains

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numDomains` is NULL

  ###### Description

  Returns the number of domains in `numDomains` for a device.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiDeviceGetTimestamp ( CUcontext context, uint64_t* timestamp )
  Read a device timestamp.

  ###### Parameters

  `context`
    A context on the device from which to get the timestamp
  `timestamp`
    Returns the device timestamp

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_PARAMETER

    is `timestamp` is NULL

  ###### Description

  Returns the device timestamp in `*timestamp`. The timestamp is reported in nanoseconds and indicates the time since the device was last reset.

  Note:

  Thread-safety: this function is thread safe.

  **DEPRECATED** This API is deprecated as of CUDA 11.3

CUptiResult cuptiDisableKernelReplayMode ( CUcontext context )
  Disable kernel replay mode.

  ###### Parameters

  `context`
    The context

  ###### Returns

  - CUPTI_SUCCESS

  ###### Description

  Set profiling mode for the context to non-replay (default) mode. Event collection mode will be set to CUPTI_EVENT_COLLECTION_MODE_KERNEL. All previously enabled event groups and event group sets will be disabled.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEnableKernelReplayMode ( CUcontext context )
  Enable kernel replay mode.

  ###### Parameters

  `context`
    The context

  ###### Returns

  - CUPTI_SUCCESS

  ###### Description

  Set profiling mode for the context to replay mode. In this mode, any number of events can be collected in one run of the kernel. The event collection mode will automatically switch to CUPTI_EVENT_COLLECTION_MODE_KERNEL. In this mode, cuptiSetEventCollectionMode will return CUPTI_ERROR_INVALID_OPERATION.

  Note:

  - Kernels might take longer to run if many events are enabled.

  - Thread-safety: this function is thread safe.

CUptiResult cuptiEnumEventDomains ( size_t* arraySizeBytes, CUpti_EventDomainID* domainArray )
  Get the event domains available on any device.

  ###### Parameters

  `arraySizeBytes`
    The size of `domainArray` in bytes, and returns the number of bytes written to `domainArray`
  `domainArray`
    Returns all the event domains

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `arraySizeBytes` or `domainArray` are NULL

  ###### Description

  Returns all the event domains available on any CUDA-capable device. Event domain IDs are returned in `domainArray`. The size of the `domainArray` buffer is given by `*arraySizeBytes`. The size of the `domainArray` buffer must be at least `numDomains` * sizeof(CUpti_EventDomainID) or all domains will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `domainArray`.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventDomainEnumEvents ( CUpti_EventDomainID eventDomain, size_t* arraySizeBytes, CUpti_EventID* eventArray )
  Get the events in a domain.

  ###### Parameters

  `eventDomain`
    ID of the event domain
  `arraySizeBytes`
    The size of `eventArray` in bytes, and returns the number of bytes written to `eventArray`
  `eventArray`
    Returns the IDs of the events in the domain

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `arraySizeBytes` or `eventArray` are NULL

  ###### Description

  Returns the event IDs in `eventArray` for a domain. The size of the `eventArray` buffer is given by `*arraySizeBytes`. The size of the `eventArray` buffer must be at least `numdomainevents` * sizeof(CUpti_EventID) or else all events will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `eventArray`.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventDomainGetAttribute ( CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t* valueSize, void* value )
  Read an event domain attribute.

  ###### Parameters

  `eventDomain`
    ID of the event domain
  `attrib`
    The event domain attribute to read
  `valueSize`
    The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  `value`
    Returns the attribute's value

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not an event domain attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Returns an event domain attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

  If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventDomainGetNumEvents ( CUpti_EventDomainID eventDomain, uint32_t* numEvents )
  Get number of events in a domain.

  ###### Parameters

  `eventDomain`
    ID of the event domain
  `numEvents`
    Returns the number of events in the domain

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numEvents` is NULL

  ###### Description

  Returns the number of events in `numEvents` for a domain.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGetAttribute ( CUpti_EventID event, CUpti_EventAttribute attrib, size_t* valueSize, void* value )
  Get an event attribute.

  ###### Parameters

  `event`
    ID of the event
  `attrib`
    The event attribute to read
  `valueSize`
    The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  `value`
    Returns the attribute's value

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not an event attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Returns an event attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

  If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGetIdFromName ( CUdevice device, const char* eventName, CUpti_EventID* event )
  Find an event by name.

  ###### Parameters

  `device`
    The CUDA device
  `eventName`
    The name of the event to find
  `event`
    Returns the ID of the found event or undefined if unable to find the event

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_EVENT_NAME

    if unable to find an event with name `eventName`. In this case `*event` is undefined

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventName` or `event` are NULL

  ###### Description

  Find an event by name and return the event ID in `*event`.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupAddEvent ( CUpti_EventGroup eventGroup, CUpti_EventID event )
  Add an event to an event group.

  ###### Parameters

  `eventGroup`
    The event group
  `event`
    The event to add to the group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_ID

  - CUPTI_ERROR_OUT_OF_MEMORY

  - CUPTI_ERROR_INVALID_OPERATION

    if `eventGroup` is enabled

  - CUPTI_ERROR_NOT_COMPATIBLE

    if `event` belongs to a different event domain than the events already in `eventGroup`, or if a device limitation prevents `event` from being collected at the same time as the events already in `eventGroup`

  - CUPTI_ERROR_MAX_LIMIT_REACHED

    if `eventGroup` is full

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Add an event to an event group. The event add can fail for a number of reasons:

  - The event group is enabled

  - The event does not belong to the same event domain as the events that are already in the event group

  - Device limitations on the events that can belong to the same group

  - The event group is full

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupCreate ( CUcontext context, CUpti_EventGroup* eventGroup, uint32_t flags )
  Create a new event group for a context.

  ###### Parameters

  `context`
    The context for the event group
  `eventGroup`
    Returns the new event group
  `flags`
    Reserved - must be zero

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_OUT_OF_MEMORY

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Creates a new event group for `context` and returns the new group in `*eventGroup`.

  Note:

  - `flags` are reserved for future use and should be set to zero.

  - Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupDestroy ( CUpti_EventGroup eventGroup )
  Destroy an event group.

  ###### Parameters

  `eventGroup`
    The event group to destroy

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_OPERATION

    if the event group is enabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if eventGroup is NULL

  ###### Description

  Destroy an `eventGroup` and free its resources. An event group cannot be destroyed if it is enabled.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupDisable ( CUpti_EventGroup eventGroup )
  Disable an event group.

  ###### Parameters

  `eventGroup`
    The event group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Disable an event group. Disabling an event group stops collection of events contained in the group.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupEnable ( CUpti_EventGroup eventGroup )
  Enable an event group.

  ###### Parameters

  `eventGroup`
    The event group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_NOT_READY

    if `eventGroup` does not contain any events

  - CUPTI_ERROR_NOT_COMPATIBLE

    if `eventGroup` cannot be enabled due to other already enabled event groups

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  - CUPTI_ERROR_HARDWARE_BUSY

    if another client is profiling and hardware is busy

  ###### Description

  Enable an event group. Enabling an event group zeros the value of all the events in the group and then starts collection of those events.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupGetAttribute ( CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t* valueSize, void* value )
  Read an event group attribute.

  ###### Parameters

  `eventGroup`
    The event group
  `attrib`
    The attribute to read
  `valueSize`
    Size of buffer pointed by the value, and returns the number of bytes written to `value`
  `value`
    Returns the value of the attribute

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not an eventgroup attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Read an event group attribute and return it in `*value`.

  Note:

  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.).

CUptiResult cuptiEventGroupReadAllEvents ( CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, size_t* eventValueBufferSizeBytes, uint64_t* eventValueBuffer, size_t* eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t* numEventIdsRead )
  Read the values for all the events in an event group.

  ###### Parameters

  `eventGroup`
    The event group
  `flags`
    Flags controlling the reading mode
  `eventValueBufferSizeBytes`
    The size of `eventValueBuffer` in bytes, and returns the number of bytes written to `eventValueBuffer`
  `eventValueBuffer`
    Returns the event values
  `eventIdArraySizeBytes`
    The size of `eventIdArray` in bytes, and returns the number of bytes written to `eventIdArray`
  `eventIdArray`
    Returns the IDs of the events in the same order as the values return in eventValueBuffer.
  `numEventIdsRead`
    Returns the number of event IDs returned in `eventIdArray`

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_INVALID_OPERATION

    if `eventGroup` is disabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup`, `eventValueBufferSizeBytes`, `eventValueBuffer`, `eventIdArraySizeBytes`, `eventIdArray` or `numEventIdsRead` is NULL

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    if size of `eventValueBuffer` or `eventIdArray` is not sufficient

  ###### Description

  Read the values for all the events in an event group. The event values are returned in the `eventValueBuffer` buffer. `eventValueBufferSizeBytes` indicates the size of `eventValueBuffer`. The buffer must be at least (sizeof(uint64) * number of events in group) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is not set on the group containing the events. The buffer must be at least (sizeof(uint64) * number of domain instances * number of events in group) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is set on the group.

  The data format returned in `eventValueBuffer` is:

  - domain instance 0: event0 event1 ... eventN

  - domain instance 1: event0 event1 ... eventN

  - ...

  - domain instance M: event0 event1 ... eventN

  The event order in `eventValueBuffer` is returned in `eventIdArray`. The size of `eventIdArray` is specified in `eventIdArraySizeBytes`. The size should be at least (sizeof(CUpti_EventID) * number of events in group).

  If any instance of any event counter overflows, the value returned for that event instance will be CUPTI_EVENT_OVERFLOW.

  The only allowed value for `flags` is CUPTI_EVENT_READ_FLAG_NONE.

  Reading events from a disabled event group is not allowed. After being read, an event's value is reset to zero.

  Note:

  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.). If cuptiEventGroupResetAllEvents is called simultaneously with this function, then returned event values are undefined.

CUptiResult cuptiEventGroupReadEvent ( CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, CUpti_EventID event, size_t* eventValueBufferSizeBytes, uint64_t* eventValueBuffer )
  Read the value for an event in an event group.

  ###### Parameters

  `eventGroup`
    The event group
  `flags`
    Flags controlling the reading mode
  `event`
    The event to read
  `eventValueBufferSizeBytes`
    The size of `eventValueBuffer` in bytes, and returns the number of bytes written to `eventValueBuffer`
  `eventValueBuffer`
    Returns the event value(s)

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_ID

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_INVALID_OPERATION

    if `eventGroup` is disabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup`, `eventValueBufferSizeBytes` or `eventValueBuffer` is NULL

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    if size of `eventValueBuffer` is not sufficient

  ###### Description

  Read the value for an event in an event group. The event value is returned in the `eventValueBuffer` buffer. `eventValueBufferSizeBytes` indicates the size of the `eventValueBuffer` buffer. The buffer must be at least sizeof(uint64) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is not set on the group containing the event. The buffer must be at least (sizeof(uint64) * number of domain instances) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is set on the group.

  If any instance of an event counter overflows, the value returned for that event instance will be CUPTI_EVENT_OVERFLOW.

  The only allowed value for `flags` is CUPTI_EVENT_READ_FLAG_NONE.

  Reading an event from a disabled event group is not allowed. After being read, an event's value is reset to zero.

  Note:

  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.). If cuptiEventGroupResetAllEvents is called simultaneously with this function, then returned event values are undefined.

CUptiResult cuptiEventGroupRemoveAllEvents ( CUpti_EventGroup eventGroup )
  Remove all events from an event group.

  ###### Parameters

  `eventGroup`
    The event group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_OPERATION

    if `eventGroup` is enabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Remove all events from an event group. Events cannot be removed if the event group is enabled.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupRemoveEvent ( CUpti_EventGroup eventGroup, CUpti_EventID event )
  Remove an event from an event group.

  ###### Parameters

  `eventGroup`
    The event group
  `event`
    The event to remove from the group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_EVENT_ID

  - CUPTI_ERROR_INVALID_OPERATION

    if `eventGroup` is enabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Remove `event` from the an event group. The event cannot be removed if the event group is enabled.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupResetAllEvents ( CUpti_EventGroup eventGroup )
  Zero all the event counts in an event group.

  ###### Parameters

  `eventGroup`
    The event group

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroup` is NULL

  ###### Description

  Zero all the event counts in an event group.

  Note:

  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.).

CUptiResult cuptiEventGroupSetAttribute ( CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t valueSize, void* value )
  Write an event group attribute.

  ###### Parameters

  `eventGroup`
    The event group
  `attrib`
    The attribute to write
  `valueSize`
    The size, in bytes, of the value
  `value`
    The attribute value to write

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not an event group attribute, or if `attrib` is not a writable attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    Indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Write an event group attribute.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupSetDisable ( CUpti_EventGroupSet* eventGroupSet )
  Disable an event group set.

  ###### Parameters

  `eventGroupSet`
    The pointer to the event group set

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroupSet` is NULL

  ###### Description

  Disable a set of event groups. Disabling a set of event groups stops collection of events contained in the groups.

  Note:

  - Thread-safety: this function is thread safe.

  - If this call fails, some of the event groups in the set may be disabled and other event groups may remain enabled.

CUptiResult cuptiEventGroupSetEnable ( CUpti_EventGroupSet* eventGroupSet )
  Enable an event group set.

  ###### Parameters

  `eventGroupSet`
    The pointer to the event group set

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_HARDWARE

  - CUPTI_ERROR_NOT_READY

    if `eventGroup` does not contain any events

  - CUPTI_ERROR_NOT_COMPATIBLE

    if `eventGroup` cannot be enabled due to other already enabled event groups

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroupSet` is NULL

  - CUPTI_ERROR_HARDWARE_BUSY

    if other client is profiling and hardware is busy

  ###### Description

  Enable a set of event groups. Enabling a set of event groups zeros the value of all the events in all the groups and then starts collection of those events.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiEventGroupSetsCreate ( CUcontext context, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, CUpti_EventGroupSets** eventGroupPasses )
  For a set of events, get the grouping that indicates the number of passes and the event groups necessary to collect the events.

  ###### Parameters

  `context`
    The context for event collection
  `eventIdArraySizeBytes`
    Size of `eventIdArray` in bytes
  `eventIdArray`
    Array of event IDs that need to be grouped
  `eventGroupPasses`
    Returns a CUpti_EventGroupSets object that indicates the number of passes required to collect the events and the events to collect on each pass

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_EVENT_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventIdArray` or `eventGroupPasses` is NULL

  ###### Description

  The number of events that can be collected simultaneously varies by device and by the type of the events. When events can be collected simultaneously, they may need to be grouped into multiple event groups because they are from different event domains. This function takes a set of events and determines how many passes are required to collect all those events, and which events can be collected simultaneously in each pass.

  The CUpti_EventGroupSets returned in `eventGroupPasses` indicates how many passes are required to collect the events with the `numSets` field. Within each event group set, the `sets` array indicates the event groups that should be collected on each pass.

  Note:

  Thread-safety: this function is thread safe, but client must guard against another thread simultaneously destroying `context`.

CUptiResult cuptiEventGroupSetsDestroy ( CUpti_EventGroupSets* eventGroupSets )
  Destroy a event group sets object.

  ###### Parameters

  `eventGroupSets`
    The object to destroy

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_OPERATION

    if any of the event groups contained in the sets is enabled

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventGroupSets` is NULL

  ###### Description

  Destroy a CUpti_EventGroupSets object.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiGetNumEventDomains ( uint32_t* numDomains )
  Get the number of event domains available on any device.

  ###### Parameters

  `numDomains`
    Returns the number of domains

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numDomains` is NULL

  ###### Description

  Returns the total number of event domains available on any CUDA-capable device.

  Note:

  Thread-safety: this function is thread safe.

CUptiResult cuptiKernelReplaySubscribeUpdate ( CUpti_KernelReplayUpdateFunc updateFunc, void* customData )
  Subscribe to kernel replay updates.

  ###### Parameters

  `updateFunc`
    The update function pointer
  `customData`
    Pointer to any custom data

  ###### Returns

  - CUPTI_SUCCESS

  ###### Description

  When subscribed, the function pointer passed in will be called each time a kernel run is finished during kernel replay. Previously subscribed function pointer will be replaced. Pass in NULL as the function pointer unsubscribes the update.

CUptiResult cuptiSetEventCollectionMode ( CUcontext context, CUpti_EventCollectionMode mode )
  Set the event collection mode.

  ###### Parameters

  `context`
    The context
  `mode`
    The event collection mode

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_OPERATION

    if called when replay mode is enabled

  - CUPTI_ERROR_NOT_SUPPORTED

    if mode is not supported on the device

  ###### Description

  Set the event collection mode for a `context`. The `mode` controls the event collection behavior of all events in event groups created in the `context`. This API is invalid in kernel replay mode.

  Note:

  Thread-safety: this function is thread safe.

### 5.6. CUPTI Metric API

Functions, types, and enums that implement the CUPTI Metric API.

Note:

CUPTI metric API from the header cupti_metrics.h are not supported on devices with compute capability 7.5 and higher (i.e. Turing and later GPU architectures). These API will be deprecated in a future CUDA release. These are replaced by Profiling API in the header cupti_profiler_target.h and Perfworks metrics API in the headers nvperf_host.h and nvperf_target.h which are supported on devices with compute capability 7.0 and higher (i.e. Volta and later GPU architectures).

#### Classes

union
CUpti_MetricValue
  A metric value.

#### Typedefs

typedef uint32_t CUpti_MetricID
  ID for a metric.

#### Enumerations

enum CUpti_MetricAttribute
  Metric attributes.
enum CUpti_MetricCategory
  A metric category.
enum CUpti_MetricEvaluationMode
  A metric evaluation mode.
enum CUpti_MetricPropertyDeviceClass
  Device class.
enum CUpti_MetricPropertyID
  Metric device properties.
enum CUpti_MetricValueKind
  Kinds of metric values.
enum CUpti_MetricValueUtilizationLevel
  Enumeration of utilization levels for metrics values of kind CUPTI_METRIC_VALUE_KIND_UTILIZATION_LEVEL. Utilization values can vary from IDLE (0) to MAX (10) but the enumeration only provides specific names for a few values.

#### Functions

CUptiResult cuptiDeviceEnumMetrics ( CUdevice device, size_t* arraySizeBytes, CUpti_MetricID* metricArray )
  Get the metrics for a device.
CUptiResult cuptiDeviceGetNumMetrics ( CUdevice device, uint32_t* numMetrics )
  Get the number of metrics for a device.
CUptiResult cuptiEnumMetrics ( size_t* arraySizeBytes, CUpti_MetricID* metricArray )
  Get all the metrics available on any device.
CUptiResult cuptiGetNumMetrics ( uint32_t* numMetrics )
  Get the total number of metrics available on any device.
CUptiResult cuptiMetricCreateEventGroupSets ( CUcontext context, size_t metricIdArraySizeBytes, CUpti_MetricID* metricIdArray, CUpti_EventGroupSets** eventGroupPasses )
  For a set of metrics, get the grouping that indicates the number of passes and the event groups necessary to collect the events required for those metrics.
CUptiResult cuptiMetricEnumEvents ( CUpti_MetricID metric, size_t* eventIdArraySizeBytes, CUpti_EventID* eventIdArray )
  Get the events required to calculating a metric.
CUptiResult cuptiMetricEnumProperties ( CUpti_MetricID metric, size_t* propIdArraySizeBytes, CUpti_MetricPropertyID* propIdArray )
  Get the properties required to calculating a metric.
CUptiResult cuptiMetricGetAttribute ( CUpti_MetricID metric, CUpti_MetricAttribute attrib, size_t* valueSize, void* value )
  Get a metric attribute.
CUptiResult cuptiMetricGetIdFromName ( CUdevice device, const char* metricName, CUpti_MetricID* metric )
  Find an metric by name.
CUptiResult cuptiMetricGetNumEvents ( CUpti_MetricID metric, uint32_t* numEvents )
  Get number of events required to calculate a metric.
CUptiResult cuptiMetricGetNumProperties ( CUpti_MetricID metric, uint32_t* numProp )
  Get number of properties required to calculate a metric.
CUptiResult cuptiMetricGetRequiredEventGroupSets ( CUcontext context, CUpti_MetricID metric, CUpti_EventGroupSets** eventGroupSets )
  For a metric get the groups of events that must be collected in the same pass.
CUptiResult cuptiMetricGetValue ( CUdevice device, CUpti_MetricID metric, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t eventValueArraySizeBytes, uint64_t* eventValueArray, uint64_t timeDuration, CUpti_MetricValue* metricValue )
  Calculate the value for a metric.
CUptiResult cuptiMetricGetValue2 ( CUpti_MetricID metric, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t eventValueArraySizeBytes, uint64_t* eventValueArray, size_t propIdArraySizeBytes, CUpti_MetricPropertyID* propIdArray, size_t propValueArraySizeBytes, uint64_t* propValueArray, CUpti_MetricValue* metricValue )
  Calculate the value for a metric.

#### Typedefs

typedef uint32_t CUpti_MetricID

  ID for a metric. A metric provides a measure of some aspect of the device.

#### Enumerations

enum CUpti_MetricAttribute

  Metric attributes describe properties of a metric. These attributes can be read using cuptiMetricGetAttribute.

  ###### Values

  CUPTI_METRIC_ATTR_NAME = 0
    Metric name. Value is a null terminated const c-string.
  CUPTI_METRIC_ATTR_SHORT_DESCRIPTION = 1
    Short description of metric. Value is a null terminated const c-string.
  CUPTI_METRIC_ATTR_LONG_DESCRIPTION = 2
    Long description of metric. Value is a null terminated const c-string.
  CUPTI_METRIC_ATTR_CATEGORY = 3
    Category of the metric. Value is of type CUpti_MetricCategory.
  CUPTI_METRIC_ATTR_VALUE_KIND = 4
    Value type of the metric. Value is of type CUpti_MetricValueKind.
  CUPTI_METRIC_ATTR_EVALUATION_MODE = 5
    Metric evaluation mode. Value is of type CUpti_MetricEvaluationMode.
  CUPTI_METRIC_ATTR_FORCE_INT = 0x7fffffff
enum CUpti_MetricCategory

  Each metric is assigned to a category that represents the general type of the metric. A metric's category is accessed using cuptiMetricGetAttribute and the CUPTI_METRIC_ATTR_CATEGORY attribute.

  ###### Values

  CUPTI_METRIC_CATEGORY_MEMORY = 0
    A memory related metric.
  CUPTI_METRIC_CATEGORY_INSTRUCTION = 1
    An instruction related metric.
  CUPTI_METRIC_CATEGORY_MULTIPROCESSOR = 2
    A multiprocessor related metric.
  CUPTI_METRIC_CATEGORY_CACHE = 3
    A cache related metric.
  CUPTI_METRIC_CATEGORY_TEXTURE = 4
    A texture related metric.
  CUPTI_METRIC_CATEGORY_NVLINK = 5
    A Nvlink related metric.
  CUPTI_METRIC_CATEGORY_PCIE = 6
    A PCIe related metric.
  CUPTI_METRIC_CATEGORY_FORCE_INT = 0x7fffffff
enum CUpti_MetricEvaluationMode

  A metric can be evaluated per hardware instance to know the load balancing across instances of a domain or the metric can be evaluated in aggregate mode when the events involved in metric evaluation are from different event domains. It might be possible to evaluate some metrics in both modes for convenience. A metric's evaluation mode is accessed using CUpti_MetricEvaluationMode and the CUPTI_METRIC_ATTR_EVALUATION_MODE attribute.

  ###### Values

  CUPTI_METRIC_EVALUATION_MODE_PER_INSTANCE = 1
    If this bit is set, the metric can be profiled for each instance of the domain. The event values passed to cuptiMetricGetValue can contain values for one instance of the domain. And cuptiMetricGetValue can be called for each instance.
  CUPTI_METRIC_EVALUATION_MODE_AGGREGATE = 1<<1
    If this bit is set, the metric can be profiled over all instances. The event values passed to cuptiMetricGetValue can be aggregated values of events for all instances of the domain.
  CUPTI_METRIC_EVALUATION_MODE_FORCE_INT = 0x7fffffff
enum CUpti_MetricPropertyDeviceClass

  Enumeration of device classes for metric property CUPTI_METRIC_PROPERTY_DEVICE_CLASS.

  ###### Values

  CUPTI_METRIC_PROPERTY_DEVICE_CLASS_TESLA = 0
  CUPTI_METRIC_PROPERTY_DEVICE_CLASS_QUADRO = 1
  CUPTI_METRIC_PROPERTY_DEVICE_CLASS_GEFORCE = 2
  CUPTI_METRIC_PROPERTY_DEVICE_CLASS_TEGRA = 3
enum CUpti_MetricPropertyID

  Metric device properties describe device properties which are needed for a metric. Some of these properties can be collected using cuDeviceGetAttribute.

  ###### Values

  CUPTI_METRIC_PROPERTY_MULTIPROCESSOR_COUNT
  CUPTI_METRIC_PROPERTY_WARPS_PER_MULTIPROCESSOR
  CUPTI_METRIC_PROPERTY_KERNEL_GPU_TIME
  CUPTI_METRIC_PROPERTY_CLOCK_RATE
  CUPTI_METRIC_PROPERTY_FRAME_BUFFER_COUNT
  CUPTI_METRIC_PROPERTY_GLOBAL_MEMORY_BANDWIDTH
  CUPTI_METRIC_PROPERTY_PCIE_LINK_RATE
  CUPTI_METRIC_PROPERTY_PCIE_LINK_WIDTH
  CUPTI_METRIC_PROPERTY_PCIE_GEN
  CUPTI_METRIC_PROPERTY_DEVICE_CLASS
  CUPTI_METRIC_PROPERTY_FLOP_SP_PER_CYCLE
  CUPTI_METRIC_PROPERTY_FLOP_DP_PER_CYCLE
  CUPTI_METRIC_PROPERTY_L2_UNITS
  CUPTI_METRIC_PROPERTY_ECC_ENABLED
  CUPTI_METRIC_PROPERTY_FLOP_HP_PER_CYCLE
  CUPTI_METRIC_PROPERTY_GPU_CPU_NVLINK_BANDWIDTH
enum CUpti_MetricValueKind

  Metric values can be one of several different kinds. Corresponding to each kind is a member of the CUpti_MetricValue union. The metric value returned by cuptiMetricGetValue should be accessed using the appropriate member of that union based on its value kind.

  ###### Values

  CUPTI_METRIC_VALUE_KIND_DOUBLE = 0
    The metric value is a 64-bit double.
  CUPTI_METRIC_VALUE_KIND_UINT64 = 1
    The metric value is a 64-bit unsigned integer.
  CUPTI_METRIC_VALUE_KIND_PERCENT = 2
    The metric value is a percentage represented by a 64-bit double. For example, 57.5% is represented by the value 57.5.
  CUPTI_METRIC_VALUE_KIND_THROUGHPUT = 3
    The metric value is a throughput represented by a 64-bit integer. The unit for throughput values is bytes/second.
  CUPTI_METRIC_VALUE_KIND_INT64 = 4
    The metric value is a 64-bit signed integer.
  CUPTI_METRIC_VALUE_KIND_UTILIZATION_LEVEL = 5
    The metric value is a utilization level, as represented by CUpti_MetricValueUtilizationLevel.
  CUPTI_METRIC_VALUE_KIND_FORCE_INT = 0x7fffffff
enum CUpti_MetricValueUtilizationLevel

  ###### Values

  CUPTI_METRIC_VALUE_UTILIZATION_IDLE = 0
  CUPTI_METRIC_VALUE_UTILIZATION_LOW = 2
  CUPTI_METRIC_VALUE_UTILIZATION_MID = 5
  CUPTI_METRIC_VALUE_UTILIZATION_HIGH = 8
  CUPTI_METRIC_VALUE_UTILIZATION_MAX = 10
  CUPTI_METRIC_VALUE_UTILIZATION_FORCE_INT = 0x7fffffff

#### Functions

CUptiResult cuptiDeviceEnumMetrics ( CUdevice device, size_t* arraySizeBytes, CUpti_MetricID* metricArray )
  Get the metrics for a device.

  ###### Parameters

  `device`
    The CUDA device
  `arraySizeBytes`
    The size of `metricArray` in bytes, and returns the number of bytes written to `metricArray`
  `metricArray`
    Returns the IDs of the metrics for the device

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `arraySizeBytes` or `metricArray` are NULL

  ###### Description

  Returns the metric IDs in `metricArray` for a device. The size of the `metricArray` buffer is given by `*arraySizeBytes`. The size of the `metricArray` buffer must be at least `numMetrics` * sizeof(CUpti_MetricID) or else all metric IDs will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `metricArray`.

CUptiResult cuptiDeviceGetNumMetrics ( CUdevice device, uint32_t* numMetrics )
  Get the number of metrics for a device.

  ###### Parameters

  `device`
    The CUDA device
  `numMetrics`
    Returns the number of metrics available for the device

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numMetrics` is NULL

  ###### Description

  Returns the number of metrics available for a device.

CUptiResult cuptiEnumMetrics ( size_t* arraySizeBytes, CUpti_MetricID* metricArray )
  Get all the metrics available on any device.

  ###### Parameters

  `arraySizeBytes`
    The size of `metricArray` in bytes, and returns the number of bytes written to `metricArray`
  `metricArray`
    Returns the IDs of the metrics

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `arraySizeBytes` or `metricArray` are NULL

  ###### Description

  Returns the metric IDs in `metricArray` for all CUDA-capable devices. The size of the `metricArray` buffer is given by `*arraySizeBytes`. The size of the `metricArray` buffer must be at least `numMetrics` * sizeof(CUpti_MetricID) or all metric IDs will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `metricArray`.

CUptiResult cuptiGetNumMetrics ( uint32_t* numMetrics )
  Get the total number of metrics available on any device.

  ###### Parameters

  `numMetrics`
    Returns the number of metrics

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numMetrics` is NULL

  ###### Description

  Returns the total number of metrics available on any CUDA-capable devices.

CUptiResult cuptiMetricCreateEventGroupSets ( CUcontext context, size_t metricIdArraySizeBytes, CUpti_MetricID* metricIdArray, CUpti_EventGroupSets** eventGroupPasses )
  For a set of metrics, get the grouping that indicates the number of passes and the event groups necessary to collect the events required for those metrics.

  ###### Parameters

  `context`
    The context for event collection
  `metricIdArraySizeBytes`
    Size of the metricIdArray in bytes
  `metricIdArray`
    Array of metric IDs
  `eventGroupPasses`
    Returns a CUpti_EventGroupSets object that indicates the number of passes required to collect the events and the events to collect on each pass

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `metricIdArray` or `eventGroupPasses` is NULL

  ###### Description

  For a set of metrics, get the grouping that indicates the number of passes and the event groups necessary to collect the events required for those metrics.

  See also:

  cuptiEventGroupSetsCreate for details on event group set creation.

CUptiResult cuptiMetricEnumEvents ( CUpti_MetricID metric, size_t* eventIdArraySizeBytes, CUpti_EventID* eventIdArray )
  Get the events required to calculating a metric.

  ###### Parameters

  `metric`
    ID of the metric
  `eventIdArraySizeBytes`
    The size of `eventIdArray` in bytes, and returns the number of bytes written to `eventIdArray`
  `eventIdArray`
    Returns the IDs of the events required to calculate `metric`

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `eventIdArraySizeBytes` or `eventIdArray` are NULL.

  ###### Description

  Gets the event IDs in `eventIdArray` required to calculate a `metric`. The size of the `eventIdArray` buffer is given by `*eventIdArraySizeBytes` and must be at least `numEvents` * sizeof(CUpti_EventID) or all events will not be returned. The value returned in `*eventIdArraySizeBytes` contains the number of bytes returned in `eventIdArray`.

CUptiResult cuptiMetricEnumProperties ( CUpti_MetricID metric, size_t* propIdArraySizeBytes, CUpti_MetricPropertyID* propIdArray )
  Get the properties required to calculating a metric.

  ###### Parameters

  `metric`
    ID of the metric
  `propIdArraySizeBytes`
    The size of `propIdArray` in bytes, and returns the number of bytes written to `propIdArray`
  `propIdArray`
    Returns the IDs of the properties required to calculate `metric`

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `propIdArraySizeBytes` or `propIdArray` are NULL.

  ###### Description

  Gets the property IDs in `propIdArray` required to calculate a `metric`. The size of the `propIdArray` buffer is given by `*propIdArraySizeBytes` and must be at least `numProp` * sizeof(CUpti_DeviceAttribute) or all properties will not be returned. The value returned in `*propIdArraySizeBytes` contains the number of bytes returned in `propIdArray`.

CUptiResult cuptiMetricGetAttribute ( CUpti_MetricID metric, CUpti_MetricAttribute attrib, size_t* valueSize, void* value )
  Get a metric attribute.

  ###### Parameters

  `metric`
    ID of the metric
  `attrib`
    The metric attribute to read
  `valueSize`
    The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  `value`
    Returns the attribute's value

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `valueSize` or `value` is NULL, or if `attrib` is not a metric attribute

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

  ###### Description

  Returns a metric attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

  If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

CUptiResult cuptiMetricGetIdFromName ( CUdevice device, const char* metricName, CUpti_MetricID* metric )
  Find an metric by name.

  ###### Parameters

  `device`
    The CUDA device
  `metricName`
    The name of metric to find
  `metric`
    Returns the ID of the found metric or undefined if unable to find the metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_DEVICE

  - CUPTI_ERROR_INVALID_METRIC_NAME

    if unable to find a metric with name `metricName`. In this case `*metric` is undefined

  - CUPTI_ERROR_INVALID_PARAMETER

    if `metricName` or `metric` are NULL.

  ###### Description

  Find a metric by name and return the metric ID in `*metric`.

CUptiResult cuptiMetricGetNumEvents ( CUpti_MetricID metric, uint32_t* numEvents )
  Get number of events required to calculate a metric.

  ###### Parameters

  `metric`
    ID of the metric
  `numEvents`
    Returns the number of events required for the metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numEvents` is NULL

  ###### Description

  Returns the number of events in `numEvents` that are required to calculate a metric.

CUptiResult cuptiMetricGetNumProperties ( CUpti_MetricID metric, uint32_t* numProp )
  Get number of properties required to calculate a metric.

  ###### Parameters

  `metric`
    ID of the metric
  `numProp`
    Returns the number of properties required for the metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_PARAMETER

    if `numProp` is NULL

  ###### Description

  Returns the number of properties in `numProp` that are required to calculate a metric.

CUptiResult cuptiMetricGetRequiredEventGroupSets ( CUcontext context, CUpti_MetricID metric, CUpti_EventGroupSets** eventGroupSets )
  For a metric get the groups of events that must be collected in the same pass.

  ###### Parameters

  `context`
    The context for event collection
  `metric`
    The metric ID
  `eventGroupSets`
    Returns a CUpti_EventGroupSets object that indicates the events that must be collected in the same pass to ensure the metric is calculated correctly. Returns NULL if no grouping is required for metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  ###### Description

  For a metric get the groups of events that must be collected in the same pass to ensure that the metric is calculated correctly. If the events are not collected as specified then the metric value may be inaccurate.

  The function returns NULL if a metric does not have any required event group. In this case the events needed for the metric can be grouped in any manner for collection.

CUptiResult cuptiMetricGetValue ( CUdevice device, CUpti_MetricID metric, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t eventValueArraySizeBytes, uint64_t* eventValueArray, uint64_t timeDuration, CUpti_MetricValue* metricValue )
  Calculate the value for a metric.

  ###### Parameters

  `device`
    The CUDA device that the metric is being calculated for
  `metric`
    The metric ID
  `eventIdArraySizeBytes`
    The size of `eventIdArray` in bytes
  `eventIdArray`
    The event IDs required to calculate `metric`
  `eventValueArraySizeBytes`
    The size of `eventValueArray` in bytes
  `eventValueArray`
    The normalized event values required to calculate `metric`. The values must be order to match the order of events in `eventIdArray`
  `timeDuration`
    The duration over which the events were collected, in ns
  `metricValue`
    Returns the value for the metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_OPERATION

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    if the eventIdArray does not contain all the events needed for metric

  - CUPTI_ERROR_INVALID_EVENT_VALUE

    if any of the event values required for the metric is CUPTI_EVENT_OVERFLOW

  - CUPTI_ERROR_INVALID_METRIC_VALUE

    if the computed metric value cannot be represented in the metric's value type. For example, if the metric value type is unsigned and the computed metric value is negative

  - CUPTI_ERROR_INVALID_PARAMETER

    if `metricValue`, `eventIdArray` or `eventValueArray` is NULL

  ###### Description

  Use the events collected for a metric to calculate the metric value. Metric value evaluation depends on the evaluation mode CUpti_MetricEvaluationMode that the metric supports. If a metric has evaluation mode as CUPTI_METRIC_EVALUATION_MODE_PER_INSTANCE, then it assumes that the input event value is for one domain instance. If a metric has evaluation mode as CUPTI_METRIC_EVALUATION_MODE_AGGREGATE, it assumes that input event values are normalized to represent all domain instances on a device. For the most accurate metric collection, the events required for the metric should be collected for all profiled domain instances. For example, to collect all instances of an event, set the CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES attribute on the group containing the event to 1. The normalized value for the event is then: (`sum_event_values` * `totalInstanceCount`) / `instanceCount`, where `sum_event_values` is the summation of the event values across all profiled domain instances, `totalInstanceCount` is obtained from querying CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT and `instanceCount` is obtained from querying CUPTI_EVENT_GROUP_ATTR_INSTANCE_COUNT (or CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT).

CUptiResult cuptiMetricGetValue2 ( CUpti_MetricID metric, size_t eventIdArraySizeBytes, CUpti_EventID* eventIdArray, size_t eventValueArraySizeBytes, uint64_t* eventValueArray, size_t propIdArraySizeBytes, CUpti_MetricPropertyID* propIdArray, size_t propValueArraySizeBytes, uint64_t* propValueArray, CUpti_MetricValue* metricValue )
  Calculate the value for a metric.

  ###### Parameters

  `metric`
    The metric ID
  `eventIdArraySizeBytes`
    The size of `eventIdArray` in bytes
  `eventIdArray`
    The event IDs required to calculate `metric`
  `eventValueArraySizeBytes`
    The size of `eventValueArray` in bytes
  `eventValueArray`
    The normalized event values required to calculate `metric`. The values must be order to match the order of events in `eventIdArray`
  `propIdArraySizeBytes`
    The size of `propIdArray` in bytes
  `propIdArray`
    The metric property IDs required to calculate `metric`
  `propValueArraySizeBytes`
    The size of `propValueArray` in bytes
  `propValueArray`
    The metric property values required to calculate `metric`. The values must be order to match the order of metric properties in `propIdArray`
  `metricValue`
    Returns the value for the metric

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_NOT_INITIALIZED

  - CUPTI_ERROR_INVALID_METRIC_ID

  - CUPTI_ERROR_INVALID_OPERATION

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    if the eventIdArray does not contain all the events needed for metric

  - CUPTI_ERROR_INVALID_EVENT_VALUE

    if any of the event values required for the metric is CUPTI_EVENT_OVERFLOW

  - CUPTI_ERROR_NOT_COMPATIBLE

    if the computed metric value cannot be represented in the metric's value type. For example, if the metric value type is unsigned and the computed metric value is negative

  - CUPTI_ERROR_INVALID_PARAMETER

    if `metricValue`, `eventIdArray` or `eventValueArray` is NULL

  ###### Description

  Use the events and properties collected for a metric to calculate the metric value. Metric value evaluation depends on the evaluation mode CUpti_MetricEvaluationMode that the metric supports. If a metric has evaluation mode as CUPTI_METRIC_EVALUATION_MODE_PER_INSTANCE, then it assumes that the input event value is for one domain instance. If a metric has evaluation mode as CUPTI_METRIC_EVALUATION_MODE_AGGREGATE, it assumes that input event values are normalized to represent all domain instances on a device. For the most accurate metric collection, the events required for the metric should be collected for all profiled domain instances. For example, to collect all instances of an event, set the CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES attribute on the group containing the event to 1. The normalized value for the event is then: (`sum_event_values` * `totalInstanceCount`) / `instanceCount`, where `sum_event_values` is the summation of the event values across all profiled domain instances, `totalInstanceCount` is obtained from querying CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT and `instanceCount` is obtained from querying CUPTI_EVENT_GROUP_ATTR_INSTANCE_COUNT (or CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT).

### 5.7. CUPTI Profiling API

Functions, types, and enums that implement the CUPTI Profiling API.

#### Classes

struct
CUpti_Profiler_BeginPass_Params
  Params for cuptiProfilerBeginPass.
struct
CUpti_Profiler_BeginSession_Params
  Params for cuptiProfilerBeginSession.
struct
CUpti_Profiler_CounterDataImageOptions
  Input parameter to define the counterDataImage.
struct
CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params
  Params for cuptiProfilerCounterDataImageCalculateScratchBufferSize.
struct
CUpti_Profiler_CounterDataImage_CalculateSize_Params
  Params for cuptiProfilerCounterDataImageCalculateSize.
struct
CUpti_Profiler_CounterDataImage_InitializeScratchBuffer_Params
  Params for cuptiProfilerCounterDataImageInitializeScratchBuffer.
struct
CUpti_Profiler_CounterDataImage_Initialize_Params
  Params for cuptiProfilerCounterDataImageInitialize.
struct
CUpti_Profiler_DeInitialize_Params
  Default parameter for cuptiProfilerDeInitialize.
struct
CUpti_Profiler_DeviceSupported_Params
  Params for cuptiProfilerDeviceSupported.
struct
CUpti_Profiler_DisableProfiling_Params
  Params for cuptiProfilerDisableProfiling.
struct
CUpti_Profiler_EnableProfiling_Params
  Params for cuptiProfilerEnableProfiling.
struct
CUpti_Profiler_EndPass_Params
  Params for cuptiProfilerEndPass.
struct
CUpti_Profiler_EndSession_Params
  Params for cuptiProfilerEndSession.
struct
CUpti_Profiler_FlushCounterData_Params
  Params for cuptiProfilerFlushCounterData.
struct
CUpti_Profiler_GetCounterAvailability_Params
  Params for cuptiProfilerGetCounterAvailability.
struct
CUpti_Profiler_Initialize_Params
  Default parameter for cuptiProfilerInitialize.
struct
CUpti_Profiler_IsPassCollected_Params
  Params for cuptiProfilerIsPassCollected.
struct
CUpti_Profiler_SetConfig_Params
  Params for cuptiProfilerSetConfig.
struct
CUpti_Profiler_UnsetConfig_Params
  Params for cuptiProfilerUnsetConfig.

#### Enumerations

enum CUpti_ProfilerRange
  Profiler range attribute.
enum CUpti_ProfilerReplayMode
  Profiler replay attribute.
enum CUpti_Profiler_Support_Level
  Generic support level enum for CUPTI.

#### Functions

CUptiResult cuptiProfilerBeginPass ( CUpti_Profiler_BeginPass_Params* pParams )
  Replay API: used for multipass collection.
CUptiResult cuptiProfilerBeginSession ( CUpti_Profiler_BeginSession_Params* pParams )
  Begin profiling session sets up the profiling on the device.
CUptiResult cuptiProfilerCounterDataImageCalculateScratchBufferSize ( CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params* pParams )
  A temporary storage for CounterData image needed for internal operations.
CUptiResult cuptiProfilerCounterDataImageCalculateSize ( CUpti_Profiler_CounterDataImage_CalculateSize_Params* pParams )
  A CounterData image allocates space for values for each counter for each range.
CUptiResult cuptiProfilerDeInitialize ( CUpti_Profiler_DeInitialize_Params* pParams )
  DeInitializes the profiler interface.
CUptiResult cuptiProfilerDeviceSupported ( CUpti_Profiler_DeviceSupported_Params* pParams )
  Query device compatibility with Profiling API.
CUptiResult cuptiProfilerDisableProfiling ( CUpti_Profiler_DisableProfiling_Params* pParams )
  Disable Profiling.
CUptiResult cuptiProfilerEnableProfiling ( CUpti_Profiler_EnableProfiling_Params* pParams )
  Enables Profiling.
CUptiResult cuptiProfilerEndPass ( CUpti_Profiler_EndPass_Params* pParams )
  Replay API: used for multipass collection.
CUptiResult cuptiProfilerEndSession ( CUpti_Profiler_EndSession_Params* pParams )
  Ends profiling session.
CUptiResult cuptiProfilerFlushCounterData ( CUpti_Profiler_FlushCounterData_Params* pParams )
  Decode all the submitted passes.
CUptiResult cuptiProfilerGetCounterAvailability ( CUpti_Profiler_GetCounterAvailability_Params* pParams )
  Query counter availibility.
CUptiResult cuptiProfilerInitialize ( CUpti_Profiler_Initialize_Params* pParams )
  Initializes the profiler interface.
CUptiResult cuptiProfilerIsPassCollected ( CUpti_Profiler_IsPassCollected_Params* pParams )
  Asynchronous call to query if the submitted pass to GPU is collected.
CUptiResult cuptiProfilerPopRange ( CUpti_Profiler_PopRange_Params* pParams )
  Range API's : Pop user range.
CUptiResult cuptiProfilerPushRange ( CUpti_Profiler_PushRange_Params* pParams )
  Range API's : Push user range.
CUptiResult cuptiProfilerSetConfig ( CUpti_Profiler_SetConfig_Params* pParams )
  Set metrics configuration to be profiled.
CUptiResult cuptiProfilerUnsetConfig ( CUpti_Profiler_UnsetConfig_Params* pParams )
  Unset metrics configuration profiled.

#### Enumerations

enum CUpti_ProfilerRange

  A metric enabled in the session's configuration is collected separately per unique range-stack in the pass. This is an attribute to collect metrics around each kernel in a profiling session or in an user defined range.

  ###### Values

  CUPTI_Range_INVALID
    Invalid value
  CUPTI_AutoRange
    Ranges are auto defined around each kernel in a profiling session
  CUPTI_UserRange
    A range in which metric data to be collected is defined by the user
  CUPTI_Range_COUNT
    Range count
enum CUpti_ProfilerReplayMode

  For metrics which require multipass collection, a replay of the GPU kernel(s) is required. This is an attribute which specify how the replay of the kernel(s) to be measured is done.

  ###### Values

  CUPTI_Replay_INVALID
    Invalid Value
  CUPTI_ApplicationReplay
    Replay is done by CUPTI user around the process
  CUPTI_KernelReplay
    Replay is done around kernel implicitly by CUPTI
  CUPTI_UserReplay
    Replay is done by CUPTI user within a process
  CUPTI_Replay_COUNT
    Replay count
enum CUpti_Profiler_Support_Level

  ###### Values

  CUPTI_PROFILER_CONFIGURATION_UNKNOWN = 0
    Configuration support level unknown - either detection code errored out before setting this value, or unable to determine it.
  CUPTI_PROFILER_CONFIGURATION_UNSUPPORTED
    Profiling is unavailable. For specific feature fields, this means that the current configuration of this feature does not work with profiling. For instance, SLI-enabled devices do not support profiling, and this value would be returned for SLI on an SLI-enabled device.
  CUPTI_PROFILER_CONFIGURATION_DISABLED
    Profiling would be available for this configuration, but was disabled by the system.
  CUPTI_PROFILER_CONFIGURATION_SUPPORTED
    Profiling is supported. For specific feature fields, this means that the current configuration of this feature works with profiling. For instance, SLI-enabled devices do not support profiling, and this value would only be returned for devices which are not SLI-enabled.

#### Functions

CUptiResult cuptiProfilerBeginPass ( CUpti_Profiler_BeginPass_Params* pParams )
  Replay API: used for multipass collection.

  ###### Description

  These APIs are used if user chooses to replay by itself CUPTI_UserReplay or CUPTI_ApplicationReplay for multipass collection of the metrics configurations. It's a no-op in case of CUPTI_KernelReplay.

CUptiResult cuptiProfilerBeginSession ( CUpti_Profiler_BeginSession_Params* pParams )
  Begin profiling session sets up the profiling on the device.

  ###### Description

  Although, it doesn't start the profiling but GPU resources needed for profiling are allocated. Outside of a session, the GPU will return to its normal operating state.

CUptiResult cuptiProfilerCounterDataImageCalculateScratchBufferSize ( CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params* pParams )
  A temporary storage for CounterData image needed for internal operations.

  ###### Description

  Use these APIs to calculate the allocation size and initialize counterData image scratch buffer.

CUptiResult cuptiProfilerCounterDataImageCalculateSize ( CUpti_Profiler_CounterDataImage_CalculateSize_Params* pParams )
  A CounterData image allocates space for values for each counter for each range.

  ###### Description

  User borne the resposibility of managing the counterDataImage allocations. CounterDataPrefix contains meta data about the metrics that will be stored in counterDataImage. Use these APIs to calculate the allocation size and initialize counterData image.

CUptiResult cuptiProfilerDeInitialize ( CUpti_Profiler_DeInitialize_Params* pParams )
  DeInitializes the profiler interface.

  ###### Description

CUptiResult cuptiProfilerDeviceSupported ( CUpti_Profiler_DeviceSupported_Params* pParams )
  Query device compatibility with Profiling API.

  ###### Description

  Use this call to determine whether a compute device and configuration are compatible with the Profiling API. If the configuration does not support profiling, one of several flags will indicate why.

CUptiResult cuptiProfilerDisableProfiling ( CUpti_Profiler_DisableProfiling_Params* pParams )
  Disable Profiling.

  ###### Description

  In CUPTI_AutoRange, these APIs are used to enable/disable profiling for the kernels to be executed in a profiling session.

CUptiResult cuptiProfilerEnableProfiling ( CUpti_Profiler_EnableProfiling_Params* pParams )
  Enables Profiling.

  ###### Description

  In CUPTI_AutoRange, these APIs are used to enable/disable profiling for the kernels to be executed in a profiling session.

CUptiResult cuptiProfilerEndPass ( CUpti_Profiler_EndPass_Params* pParams )
  Replay API: used for multipass collection.

  ###### Description

  These APIs are used if user chooses to replay by itself CUPTI_UserReplay or CUPTI_ApplicationReplay for multipass collection of the metrics configurations. Its a no-op in case of CUPTI_KernelReplay. Returns information for next pass.

CUptiResult cuptiProfilerEndSession ( CUpti_Profiler_EndSession_Params* pParams )
  Ends profiling session.

  ###### Description

  Frees up the GPU resources acquired for profiling. Outside of a session, the GPU will return to it's normal operating state.

CUptiResult cuptiProfilerFlushCounterData ( CUpti_Profiler_FlushCounterData_Params* pParams )
  Decode all the submitted passes.

  ###### Description

  Flush Counter data API to ensure every pass is decoded into the counterDataImage passed at beginSession. This will cause the CPU/GPU sync to collect all the undecoded pass.

CUptiResult cuptiProfilerGetCounterAvailability ( CUpti_Profiler_GetCounterAvailability_Params* pParams )
  Query counter availibility.

  ###### Description

  Use this API to query counter availability information in a buffer which can be used to filter unavailable raw metrics on host. Note: This API may fail, if any profiling or sampling session is active on the specified context or its device.

CUptiResult cuptiProfilerInitialize ( CUpti_Profiler_Initialize_Params* pParams )
  Initializes the profiler interface.

  ###### Description

  Loads the required libraries in the process address space. Sets up the hooks with the CUDA driver.

CUptiResult cuptiProfilerIsPassCollected ( CUpti_Profiler_IsPassCollected_Params* pParams )
  Asynchronous call to query if the submitted pass to GPU is collected.

  ###### Description

CUptiResult cuptiProfilerPopRange ( CUpti_Profiler_PopRange_Params* pParams )
  Range API's : Pop user range.

  ###### Description

  Counter data is collected per unique range-stack. Identified by a string label passsed by the user. It's an invalid operation in case of CUPTI_AutoRange.

CUptiResult cuptiProfilerPushRange ( CUpti_Profiler_PushRange_Params* pParams )
  Range API's : Push user range.

  ###### Description

  Counter data is collected per unique range-stack. Identified by a string label passsed by the user. It's an invalid operation in case of CUPTI_AutoRange.

CUptiResult cuptiProfilerSetConfig ( CUpti_Profiler_SetConfig_Params* pParams )
  Set metrics configuration to be profiled.

  ###### Description

  Use these APIs to set the config to profile in a session. It can be used for advanced cases such as where multiple configurations are collected into a single CounterData Image on the need basis, without restarting the session.

CUptiResult cuptiProfilerUnsetConfig ( CUpti_Profiler_UnsetConfig_Params* pParams )
  Unset metrics configuration profiled.

  ###### Description

### 5.8. CUPTI Checkpoint API

Functions, types, and enums that implement the CUPTI Checkpoint API.

#### Classes

struct
NV::Cupti::Checkpoint::CUpti_Checkpoint
  Configuration and handle for a CUPTI Checkpoint.

#### Enumerations

enum NV::Cupti::Checkpoint::CUpti_CheckpointOptimizations
  Specifies optimization options for a checkpoint, may be OR'd together to specify multiple options.

#### Functions

CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointFree ( const CUpti_Checkpoint* handle )
  Free the backing data for a checkpoint.
CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointRestore ( const CUpti_Checkpoint* handle )
  Restore a checkpoint to the device associated with its context.
CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointSave ( const CUpti_Checkpoint* handle )
  Initialize and save a checkpoint of the device state associated with the handle context.

#### Enumerations

enum NV::Cupti::Checkpoint::CUpti_CheckpointOptimizations

  ###### Values

  CUPTI_CHECKPOINT_OPT_NONE = 0
    Default behavior.
  CUPTI_CHECKPOINT_OPT_TRANSFER = 1
    Determine which mem blocks have changed, and only restore those. This optimization is cached, which means cuptiCheckpointRestore must always be called at the same point in the application when this option is enabled, or the result may be incorrect.

#### Functions

CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointFree ( const CUpti_Checkpoint* handle )
  Free the backing data for a checkpoint.

  ###### Parameters

  `handle`
    A pointer to a previously saved CUpti_Checkpoint object

  ###### Returns

  - CUPTI_SUCCESS

    if the handle was successfully freed

  - CUPTI_ERROR_INVALID_PARAMETER

    if the handle was already freed or appears invalid

  - CUPTI_ERROR_INVALID_CONTEXT

    if the context is no longer valid

  ###### Description

  Frees all associated device, host memory and filesystem storage used for this context. After freeing a handle, it may be re-used as if it was new - options may be re-configured and will take effect on the next call to `cuptiCheckpointSave`.

CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointRestore ( const CUpti_Checkpoint* handle )
  Restore a checkpoint to the device associated with its context.

  ###### Parameters

  `handle`
    A pointer to a previously saved CUpti_Checkpoint object

  ###### Returns

  - CUTPI_SUCCESS

    if the checkpoint was successfully restored

  - CUPTI_ERROR_NOT_INITIALIZED

    if the checkpoint was not previously initialized

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_PARAMETER

    if the handle appears invalid

  - CUPTI_ERROR_UNKNOWN

    if the restore or optimization operation fails

  ###### Description

  Restores device, pinned, and allocated memory to the state when the checkpoint was saved

CUptiResult NV::Cupti::Checkpoint::cuptiCheckpointSave ( const CUpti_Checkpoint* handle )
  Initialize and save a checkpoint of the device state associated with the handle context.

  ###### Parameters

  `handle`
    A pointer to a CUpti_Checkpoint object

  ###### Returns

  - CUPTI_SUCCESS

    if a checkpoint was successfully initialized and saved

  - CUPTI_ERROR_INVALID_PARAMETER

    if `handle` does not appear to refer to a valid CUpti_Checkpoint

  - CUPTI_ERROR_INVALID_CONTEXT

  - CUPTI_ERROR_INVALID_DEVICE

    if device associated with context is not compatible with checkpoint API

  - CUPTI_ERROR_INVALID_OPERATION

    if Save is requested over an existing checkpoint, but `allowOverwrite` was not originally specified

  - CUPTI_ERROR_OUT_OF_MEMORY

    if as configured, not enough backing storage space to save the checkpoint

  ###### Description

  Uses the handle options to configure and save a checkpoint of the device state associated with the specified context.

### 5.9. CUPTI PC Sampling API

Functions, types, and enums that implement the CUPTI PC Sampling API.

#### Classes

struct
CUpti_GetCubinCrcParams
  Params for cuptiGetCubinCrc.
struct
CUpti_GetSassToSourceCorrelationParams
  Params for cuptiGetSassToSourceCorrelation.
struct
CUpti_PCSamplingConfigurationInfo
  PC sampling configuration information structure.
struct
CUpti_PCSamplingConfigurationInfoParams
  PC sampling configuration structure.
struct
CUpti_PCSamplingData
  Collected PC Sampling data.
struct
CUpti_PCSamplingDisableParams
  Params for cuptiPCSamplingDisable.
struct
CUpti_PCSamplingEnableParams
  Params for cuptiPCSamplingEnable.
struct
CUpti_PCSamplingGetDataParams
  Params for cuptiPCSamplingEnable.
struct
CUpti_PCSamplingGetNumStallReasonsParams
  Params for cuptiPCSamplingGetNumStallReasons.
struct
CUpti_PCSamplingGetStallReasonsParams
  Params for cuptiPCSamplingGetStallReasons.
struct
CUpti_PCSamplingPCData
  PC Sampling data.
struct
CUpti_PCSamplingStallReason
  PC Sampling stall reasons.
struct
CUpti_PCSamplingStartParams
  Params for cuptiPCSamplingStart.
struct
CUpti_PCSamplingStopParams
  Params for cuptiPCSamplingStop.

#### Typedefs

typedef void ( *CUpti_ComputeCrcCallbackFunc )( const void* cubin, size_t cubinSize, uint64_t* cubinCrc )
  Function type for callback used by CUPTI to request crc of loaded module.

#### Enumerations

enum CUpti_PCSamplingCollectionMode
  PC Sampling collection mode.
enum CUpti_PCSamplingConfigurationAttributeType
  PC Sampling configuration attributes.
enum CUpti_PCSamplingOutputDataFormat
  PC Sampling output data format.

#### Functions

CUptiResult cuptiGetCubinCrc ( CUpti_GetCubinCrcParams* pParams )
  Get the CRC of cubin.
CUptiResult cuptiGetSassToSourceCorrelation ( CUpti_GetSassToSourceCorrelationParams* pParams )
  SASS to Source correlation.
CUptiResult cuptiPCSamplingDisable ( CUpti_PCSamplingDisableParams* pParams )
  Disable PC sampling.
CUptiResult cuptiPCSamplingEnable ( CUpti_PCSamplingEnableParams* pParams )
  Enable PC sampling.
CUptiResult cuptiPCSamplingGetConfigurationAttribute ( CUpti_PCSamplingConfigurationInfoParams* pParams )
  Read PC Sampling configuration attribute.
CUptiResult cuptiPCSamplingGetData ( CUpti_PCSamplingGetDataParams* pParams )
  Flush GPU PC sampling data periodically.
CUptiResult cuptiPCSamplingGetNumStallReasons ( CUpti_PCSamplingGetNumStallReasonsParams* pParams )
  Get PC sampling stall reason count.
CUptiResult cuptiPCSamplingGetStallReasons ( CUpti_PCSamplingGetStallReasonsParams* pParams )
  Get PC sampling stall reasons.
CUptiResult cuptiPCSamplingSetConfigurationAttribute ( CUpti_PCSamplingConfigurationInfoParams* pParams )
  Write PC Sampling configuration attribute.
CUptiResult cuptiPCSamplingStart ( CUpti_PCSamplingStartParams* pParams )
  Start PC sampling.
CUptiResult cuptiPCSamplingStop ( CUpti_PCSamplingStopParams* pParams )
  Stop PC sampling.
CUptiResult cuptiRegisterComputeCrcCallback ( CUpti_ComputeCrcCallbackFunc funcComputeCubinCrc )
  Register callback function with CUPTI to use your own algorithm to compute cubin crc.

#### Typedefs

void ( *CUpti_ComputeCrcCallbackFunc )( const void* cubin, size_t cubinSize, uint64_t* cubinCrc )

  Function type for callback used by CUPTI to request crc of loaded module. This callback function ask for crc of provided module in function. The provided crc will be stored in PC sampling records i.e. in the field 'cubinCrc' of the PC sampling struct CUpti_PCSamplingPCData. The CRC is uses during the offline source correlation to uniquely identify the module.

###### Parameters

`cubin`
  The pointer to cubin binary
`size_t cubinSize`
`cubinCrc`
  Returns the computed crc of cubin.

#### Enumerations

enum CUpti_PCSamplingCollectionMode

  ###### Values

  CUPTI_PC_SAMPLING_COLLECTION_MODE_INVALID = 0
    INVALID Value
  CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS = 1
    Continuous mode. Kernels are not serialized in this mode.
  CUPTI_PC_SAMPLING_COLLECTION_MODE_KERNEL_SERIALIZED = 2
    Serialized mode. Kernels are serialized in this mode.
enum CUpti_PCSamplingConfigurationAttributeType

  PC Sampling configuration attribute types. These attributes can be read using cuptiPCSamplingGetConfigurationAttribute and can be written using cuptiPCSamplingSetConfigurationAttribute. Attributes marked [r] can only be read using cuptiPCSamplingGetConfigurationAttribute [w] can only be written using cuptiPCSamplingSetConfigurationAttribute [rw] can be read using cuptiPCSamplingGetConfigurationAttribute and written using cuptiPCSamplingSetConfigurationAttribute

  ###### Values

  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_INVALID = 0
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_SAMPLING_PERIOD = 1
    [rw] Sampling period for PC Sampling. DEFAULT - CUPTI defined value based on number of SMs Valid values for the sampling periods are between 5 to 31 both inclusive. This will set the sampling period to (2^samplingPeriod) cycles. For e.g. for sampling period = 5 to 31, cycles = 32, 64, 128,..., 2^31 Value is a uint32_t
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_STALL_REASON = 2
    [w] Number of stall reasons to collect. DEFAULT - All stall reasons will be collected Value is a size_t [w] Stall reasons to collect DEFAULT - All stall reasons will be collected Input value should be a pointer pointing to array of stall reason indexes containing all the stall reason indexes to collect.
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_SCRATCH_BUFFER_SIZE = 3
    [rw] Size of SW buffer for raw PC counter data downloaded from HW buffer DEFAULT - 1 MB, which can accommodate approximately 5500 PCs with all stall reasons Approximately it takes 16 Bytes (and some fixed size memory) to accommodate one PC with one stall reason For e.g. 1 PC with 1 stall reason = 32 Bytes 1 PC with 2 stall reason = 48 Bytes 1 PC with 4 stall reason = 96 Bytes Value is a size_t
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_HARDWARE_BUFFER_SIZE = 4
    [rw] Size of HW buffer in bytes DEFAULT - 512 MB If sampling period is too less, HW buffer can overflow and drop PC data Value is a size_t
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_COLLECTION_MODE = 5
    [rw] PC Sampling collection mode DEFAULT - CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS Input value should be of type CUpti_PCSamplingCollectionMode.
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL = 6
    [rw] Control over PC Sampling data collection range Default - 0 1 - Allows user to start and stop PC Sampling using APIs - cuptiPCSamplingStart() - Start PC Sampling cuptiPCSamplingStop() - Stop PC Sampling Value is a uint32_t
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_OUTPUT_DATA_FORMAT = 7
    [w] Value for output data format Default - CUPTI_PC_SAMPLING_OUTPUT_DATA_FORMAT_PARSED Input value should be of type CUpti_PCSamplingOutputDataFormat.
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_SAMPLING_DATA_BUFFER = 8
    [w] Data buffer to hold collected PC Sampling data PARSED_DATA Default - none. Buffer type is void * which can point to PARSED_DATA Refer CUpti_PCSamplingData for buffer format for PARSED_DATA
  CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_FORCE_INT = 0x7fffffff
enum CUpti_PCSamplingOutputDataFormat

  ###### Values

  CUPTI_PC_SAMPLING_OUTPUT_DATA_FORMAT_INVALID = 0
  CUPTI_PC_SAMPLING_OUTPUT_DATA_FORMAT_PARSED = 1
    HW buffer data will be parsed during collection of data

#### Functions

CUptiResult cuptiGetCubinCrc ( CUpti_GetCubinCrcParams* pParams )
  Get the CRC of cubin.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if parameter cubin is NULL or provided cubinSize is zero or size field is not set.

  ###### Description

  This function returns the CRC of provided cubin binary.

CUptiResult cuptiGetSassToSourceCorrelation ( CUpti_GetSassToSourceCorrelationParams* pParams )
  SASS to Source correlation.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if either of the parameters cubin or functionName is NULL or cubinSize is zero or size field is not set correctly.

  - CUPTI_ERROR_INVALID_MODULE

    provided cubin is invalid.

  - CUPTI_ERROR_UNKNOWN

    an internal error occurred. This error code is also used for cases when the function is not present in the module. A better error code will be returned in the future release.

  ###### Description

  It is expected from user to free allocated memory for fileName and dirName after use.

CUptiResult cuptiPCSamplingDisable ( CUpti_PCSamplingDisableParams* pParams )
  Disable PC sampling.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

  For application which doesn't destroy the CUDA context explicitly, this API does the PC Sampling tear-down, joins threads and copies PC records in the buffer provided during the PC sampling configuration. PC records which can't be accommodated in the buffer are discarded.

CUptiResult cuptiPCSamplingEnable ( CUpti_PCSamplingEnableParams* pParams )
  Enable PC sampling.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

CUptiResult cuptiPCSamplingGetConfigurationAttribute ( CUpti_PCSamplingConfigurationInfoParams* pParams )
  Read PC Sampling configuration attribute.

  ###### Parameters

  `pParams`
    A pointer to CUpti_PCSamplingConfigurationInfoParams containing PC sampling configuration.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this API is called with some invalid attribute.

  - CUPTI_ERROR_INVALID_PARAMETER

    if `attrib` is not valid or any `pParams` is not valid

  - CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT

    indicates that the `value` buffer is too small to hold the attribute value

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

CUptiResult cuptiPCSamplingGetData ( CUpti_PCSamplingGetDataParams* pParams )
  Flush GPU PC sampling data periodically.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this API is called without enabling PC sampling.

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

  Flushing of GPU PC Sampling data is required at following point to maintain uniqueness of PCs: For CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS, after every module load-unload-load For CUPTI_PC_SAMPLING_COLLECTION_MODE_KERNEL_SERIALIZED, after every kernel ends If configuration option CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL is enabled, then after every range end i.e. cuptiPCSamplingStop() If application is profiled in CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS, with disabled CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL, and there is no module unload, user can collect data in two ways: Use cuptiPCSamplingGetData() API periodically Use cuptiPCSamplingDisable() on application exit and read GPU PC sampling data from sampling data buffer passed during configuration. Note: In case, cuptiPCSamplingGetData() API is not called periodically, then sampling data buffer passed during configuration should be large enough to hold all PCs data. cuptiPCSamplingGetData() API never does device synchronization. It is possible that when the API is called there is some unconsumed data from the HW buffer. In this case CUPTI provides only the data available with it at that moment.

CUptiResult cuptiPCSamplingGetNumStallReasons ( CUpti_PCSamplingGetNumStallReasonsParams* pParams )
  Get PC sampling stall reason count.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

CUptiResult cuptiPCSamplingGetStallReasons ( CUpti_PCSamplingGetStallReasonsParams* pParams )
  Get PC sampling stall reasons.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

CUptiResult cuptiPCSamplingSetConfigurationAttribute ( CUpti_PCSamplingConfigurationInfoParams* pParams )
  Write PC Sampling configuration attribute.

  ###### Parameters

  `pParams`
    A pointer to CUpti_PCSamplingConfigurationInfoParams containing PC sampling configuration.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this API is called with some invalid `attrib`.

  - CUPTI_ERROR_INVALID_PARAMETER

    if attribute `value` is not valid or any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

CUptiResult cuptiPCSamplingStart ( CUpti_PCSamplingStartParams* pParams )
  Start PC sampling.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this API is called with incorrect PC Sampling configuration.

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

  User can collect PC Sampling data for user-defined range specified by Start/Stop APIs. This API can be used to mark starting of range. Set configuration option CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL to use this API.

CUptiResult cuptiPCSamplingStop ( CUpti_PCSamplingStopParams* pParams )
  Stop PC sampling.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_OPERATION

    if this API is called with incorrect PC Sampling configuration.

  - CUPTI_ERROR_INVALID_PARAMETER

    if any `pParams` is not valid

  - CUPTI_ERROR_NOT_SUPPORTED

    indicates that the system/device does not support the API

  ###### Description

  User can collect PC Sampling data for user-defined range specified by Start/Stop APIs. This API can be used to mark end of range. Set configuration option CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL to use this API.

CUptiResult cuptiRegisterComputeCrcCallback ( CUpti_ComputeCrcCallbackFunc funcComputeCubinCrc )
  Register callback function with CUPTI to use your own algorithm to compute cubin crc.

  ###### Parameters

  `funcComputeCubinCrc`
    callback is invoked when a CUDA module is loaded.

  ###### Returns

  - CUPTI_SUCCESS

  - CUPTI_ERROR_INVALID_PARAMETER

    if `funcComputeCubinCrc` is NULL.

  ###### Description

  This function registers a callback function and it gets called from CUPTI when a CUDA module is loaded.

### 5.10. CUPTI PC Sampling Utility API

Functions, types, and enums that implement the CUPTI PC Sampling Utility API.

#### Classes

struct
BufferInfo
  BufferInfo will be stored in the file for every buffer i.e for every call of UtilDumpPcSamplingBufferInFile() API.
struct
CUPTI::PcSamplingUtil::CUptiUtil_GetBufferInfoParams
  Params for CuptiUtilGetBufferInfo.
struct
CUPTI::PcSamplingUtil::CUptiUtil_GetHeaderDataParams
  Params for CuptiUtilGetHeaderData.
struct
CUPTI::PcSamplingUtil::CUptiUtil_GetPcSampDataParams
  Params for CuptiUtilGetPcSampData.
struct
CUPTI::PcSamplingUtil::CUptiUtil_MergePcSampDataParams
  Params for CuptiUtilMergePcSampData.
struct
CUPTI::PcSamplingUtil::CUptiUtil_PutPcSampDataParams
  Params for CuptiUtilPutPcSampData.
struct
Header
  Header info will be stored in file.
struct
PcSamplingStallReasons
  All available stall reasons name and respective indexes will be stored in it.

#### Enumerations

enum CUPTI::PcSamplingUtil::CUptiUtilResult
  CUPTI PC sampling utility API result codes.

#### Functions

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetBufferInfo ( CUptiUtil_GetBufferInfoParams* pParams )
  Get buffer info data of file.
CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetHeaderData ( CUptiUtil_GetHeaderDataParams* pParams )
  Get header data of file.
CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetPcSampData ( CUptiUtil_GetPcSampDataParams* pParams )
  Retrieve PC sampling data from file into allocated buffer.
CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilMergePcSampData ( CUptiUtil_MergePcSampDataParams* pParams )
  Merge PC sampling data range id wise.
CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilPutPcSampData ( CUptiUtil_PutPcSampDataParams* pParams )
  Dump PC sampling data into the file.

#### Enumerations

enum CUPTI::PcSamplingUtil::CUptiUtilResult

  Error and result codes returned by CUPTI PC sampling utility API.

  ###### Values

  CUPTI_UTIL_SUCCESS = 0
    No error
  CUPTI_UTIL_ERROR_INVALID_PARAMETER = 1
    One or more of the parameters are invalid.
  CUPTI_UTIL_ERROR_UNABLE_TO_CREATE_FILE = 2
    Unable to create a new file
  CUPTI_UTIL_ERROR_UNABLE_TO_OPEN_FILE = 3
    Unable to open a file
  CUPTI_UTIL_ERROR_READ_WRITE_OPERATION_FAILED = 4
    Read or write operation failed
  CUPTI_UTIL_ERROR_FILE_HANDLE_CORRUPTED = 5
    Provided file handle is corrupted.
  CUPTI_UTIL_ERROR_SEEK_OPERATION_FAILED = 6
    seek operation failed.
  CUPTI_UTIL_ERROR_OUT_OF_MEMORY = 7
    Unable to allocate enough memory to perform the requested operation.
  CUPTI_UTIL_ERROR_UNKNOWN = 999
    An unknown internal error has occurred.
  CUPTI_UTIL_ERROR_FORCE_INT = 0x7fffffff

#### Functions

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetBufferInfo ( CUptiUtil_GetBufferInfoParams* pParams )
  Get buffer info data of file.

  ###### Returns

  - CUPTI_UTIL_SUCCESS

  - CUPTI_UTIL_ERROR_INVALID_PARAMETER

    error out if either of pParam or fileHandle is NULL or param struct size is incorrect.

  - CUPTI_UTIL_ERROR_FILE_HANDLE_CORRUPTED

    file handle is not in good state to read data from file.

  - CUPTI_UTIL_ERROR_READ_WRITE_OPERATION_FAILED

    failed to read data from file.

  ###### Description

  This API must be called every time before calling CuptiUtilGetPcSampData API. BufferInfo structure, it gives info about recordCount and stallReasonCount of every record in the buffer. This will help to allocate exact buffer to retrieve data into it.

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetHeaderData ( CUptiUtil_GetHeaderDataParams* pParams )
  Get header data of file.

  ###### Returns

  - CUPTI_UTIL_SUCCESS

  - CUPTI_UTIL_ERROR_INVALID_PARAMETER

    error out if either of pParam or fileHandle is NULL or param struct size is incorrect.

  - CUPTI_UTIL_ERROR_FILE_HANDLE_CORRUPTED

    file handle is not in good state to read data from file

  - CUPTI_UTIL_ERROR_READ_WRITE_OPERATION_FAILED

    failed to read data from file.

  ###### Description

  This API must be called once initially while retrieving data from file. Header structure, it gives info about total number of buffers present in the file.

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilGetPcSampData ( CUptiUtil_GetPcSampDataParams* pParams )
  Retrieve PC sampling data from file into allocated buffer.

  ###### Returns

  - CUPTI_UTIL_SUCCESS

  - CUPTI_UTIL_ERROR_INVALID_PARAMETER

    error out if buffer type is invalid or if either of pSampData, pParams is NULL. If pPcSamplingStallReasons is not NULL then error out if either of stallReasonIndex, stallReasons or stallReasons array element pointer is NULL. or filename is empty.

  - CUPTI_UTIL_ERROR_READ_WRITE_OPERATION_FAILED

  - CUPTI_UTIL_ERROR_FILE_HANDLE_CORRUPTED

    file handle is not in good state to read data from file.

  ###### Description

  This API must be called after CuptiUtilGetBufferInfo API. It will retrieve data from file into allocated buffer.

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilMergePcSampData ( CUptiUtil_MergePcSampDataParams* pParams )
  Merge PC sampling data range id wise.

  ###### Returns

  - CUPTI_UTIL_SUCCESS

  - CUPTI_UTIL_ERROR_INVALID_PARAMETER

    error out if param struct size is invalid or count of buffers to merge is invalid i.e less than 1 or either of PcSampDataBuffer, MergedPcSampDataBuffers, numMergedBuffer is NULL

  - CUPTI_UTIL_ERROR_OUT_OF_MEMORY

    Unable to allocate memory for merged buffer.

  ###### Description

  This API merge PC sampling data range id wise. It allocates memory for merged data and fill data in it and provide buffer pointer in MergedPcSampDataBuffers field. It is expected from user to free merge data buffers after use.

CUptiUtilResult CUPTIUTILAPI CUPTI::PcSamplingUtil::CuptiUtilPutPcSampData ( CUptiUtil_PutPcSampDataParams* pParams )
  Dump PC sampling data into the file.

  ###### Returns

  - CUPTI_UTIL_SUCCESS

  - CUPTI_UTIL_ERROR_INVALID_PARAMETER

    error out if buffer type is invalid or if either of pSamplingData, pParams pointer is NULL or stall reason configuration details not provided or filename is empty.

  - CUPTI_UTIL_ERROR_UNABLE_TO_CREATE_FILE

  - CUPTI_UTIL_ERROR_UNABLE_TO_OPEN_FILE

  - CUPTI_UTIL_ERROR_READ_WRITE_OPERATION_FAILED

  ###### Description

  This API can be called multiple times. It will append buffer in the file. For every buffer it will store BufferInfo so that before retrieving data it will help to allocate buffer to store retrieved data. This API creates file if file does not present. If stallReasonIndex or stallReasons pointer of CUptiUtil_PutPcSampDataParams is NULL then stall reasons data will not be stored in file. It is expected to store all available stall reason data at least once to refer it during offline correlation.