-->
CUPTI (PDF) - v11.8 (older) - Last updated Aug 18, 2022 - Send Feedback -

## 2. Usage

### 2.1. CUPTI Compatibility and Requirements

New versions of the CUDA driver are backwards compatible with older versions of CUPTI. For example, a developer using a profiling tool based on CUPTI 10.0 can update to a more recently released CUDA driver. Refer to the table CUDA Toolkit and Compatible Driver Versions for minimum version of the CUDA driver required for each release of CUPTI from the corresponding CUDA Toolkit release. CUPTI calls will fail with error code `CUPTI_ERROR_NOT_INITIALIZED` if the CUDA driver version is not compatible with the CUPTI version.

### 2.2. CUPTI Initialization

CUPTI initialization occurs lazily the first time you invoke any CUPTI function. For the Activity, Event, Metric, and Callback APIs there are no requirements on when this initialization must occur (i.e. you can invoke the first CUPTI function at any point). See the CUPTI Activity API section for more information on CUPTI initialization requirements for the activity API.

It is recommended for CUPTI clients to call the API `cuptiSubscribe()` before starting the profiling session i.e. API `cuptiSubscribe()` should be called before calling any other CUPTI API. This API will return the error code `CUPTI_ERROR_MULTIPLE_SUBSCRIBERS_NOT_SUPPORTED` when another CUPTI client is already subscribed. CUPTI client should error out and not make further CUPTI calls if `cuptiSubscribe()` returns an error. This would prevent multiple CUPTI clients to be active at the same time otherwise those might interfere with the profiling state of each other.

### 2.3. CUPTI Activity API

The CUPTI Activity API allows you to asynchronously collect a trace of an application's CPU and GPU CUDA activity. The following terminology is used by the activity API.

Activity Record
  CPU and GPU activity is reported in C data structures called activity records. There is a different C structure type for each activity kind (e.g. `CUpti_ActivityAPI`). Records are generically referred to using the `CUpti_Activity` type. This type contains only a field that indicates the kind of the activity record. Using this kind, the object can be cast from the generic `CUpti_Activity` type to the specific type representing the activity. See the `printActivity` function in the activity_trace_async sample for an example.
Activity Buffer
  An activity buffer is used to transfer one or more activity records from CUPTI to the client. CUPTI fills activity buffers with activity records as the corresponding activities occur on the CPU and GPU. But CUPTI doesn't guarantee any ordering of the activities in the activity buffer as activity records for few activity kinds are added lazily. The CUPTI client is responsible for providing empty activity buffers as necessary to ensure that no records are dropped.

An asynchronous buffering API is implemented by `cuptiActivityRegisterCallbacks` and `cuptiActivityFlushAll`.

It is not required that the activity API be initalized before CUDA initialization. All related activities occuring after initializing the activity API are collected. You can force initialization of the activity API by enabling one or more activity kinds using `cuptiActivityEnable` or `cuptiActivityEnableContext`, as shown in the `initTrace` function of the activity_trace_async sample. Some activity kinds cannot be directly enabled, see the API documentation for `CUpti_ActivityKind` for details. The functions `cuptiActivityEnable` and `cuptiActivityEnableContext` will return `CUPTI_ERROR_NOT_COMPATIBLE` if the requested activity kind cannot be enabled.

The activity buffer API uses callbacks to request and return buffers of activity records. To use the asynchronous buffering API, you must first register two callbacks using `cuptiActivityRegisterCallbacks`. One of these callbacks will be invoked whenever CUPTI needs an empty activity buffer. The other callback is used to deliver a buffer containing one or more activity records to the client. To minimize profiling overhead the client should return as quickly as possible from these callbacks. Client can pre-allocate a pool of activity buffers and return an empty buffer from the pool when requested by CUPTI. Activity buffer size should be chosen carefully, smaller buffers can result in frequent requests by CUPTI and bigger buffers can delay the automatic delivery of completed activity buffers. For typical workloads, it's suggested to choose a size between 1 and 10 MB. The functions `cuptiActivityGetAttribute` and `cuptiActivitySetAttribute` can be used to read and write attributes that control how the buffering API behaves. See the API documentation for more information.

Flushing of the activity buffers

CUPTI is expected to deliver the activity buffer automatically as soon as it gets full and all the activity records in it are completed. For performance reasons, CUPTI calls the underlying methods based on certain heuristics, thus it can cause delay in the delivery of the buffer. However client can make a request to deliver the activity buffer/s at any time, and this can be achieved using the APIs `cuptiActivityFlushAll` and `cuptiActivityFlushPeriod`. Behavior of these APIs is as follows:

- For on-demand flush using the API `cuptiActivityFlushAll` with the flag set as 0, CUPTI returns all the activity buffers which have all the activity records completed, buffers need not to be full though. It doesn't return buffers which have one or more incomplete records. This flush can be done at a regular interval in a separate thread.
- For on-demand forced flush using the API `cuptiActivityFlushAll` with the flag set as CUPTI_ACTIVITY_FLAG_FLUSH_FORCED, CUPTI returns all the activity buffers including the ones which have one or more incomplete activity records. It's suggested to do the forced flush before the termination of the profiling session to allow remaining buffers to be delivered.
- For periodic flush using the API `cuptiActivityFlushPeriod`, CUPTI returns only those activity buffers which are full and have all the activity records completed. It's allowed to use the API `cuptiActivityFlushAll` to flush the buffers on-demand, even when client sets the periodic flush.

Note that activity record is considered as completed if it has all the information filled up including the timestamps (if any).

The activity_trace_async sample shows how to use the activity buffer API to collect a trace of CPU and GPU activity for a simple application.

CUPTI Threads

CUPTI creates a worker thread to minimize the perturbance for the application created threads. CUPTI offloads certain operations from the application threads to the worker thread, this incldues synchronization of profiling resources between host and device, delivery of the activity buffers to the client using the buffer completed callback registered in the API `cuptiActivityRegisterCallbacks` etc. To minimize the overhead, CUPTI wakes up the worker thread based on certain heuristics. API `cuptiActivityFlushPeriod` introduced in CUDA 11.1 can be used to control the flush period of the worker thread. This setting overrides the CUPTI heurtistics. It's allowed to use the API `cuptiActivityFlushAll` to flush the data on-demand, even when client sets the periodic flush.

Further, CUPTI creates separate threads when certain activity kinds are enabled. For example, CUPTI creates one thread each for activity kinds `CUPTI_ACTIVITY_KIND_UNIFIED_MEMORY_COUNTER` and `CUPTI_ACTIVITY_KIND_ENVIRONMENT` to collect the information from the backend.

#### 2.3.1. SASS Source Correlation

While high-level languages for GPU programming like CUDA C offer a useful level of abstraction, convenience, and maintainability, they inherently hide some of the details of the execution on the hardware. It is sometimes helpful to analyze performance problems for a kernel at the assembly instruction level. Reading assembly language is tedious and challenging; CUPTI can help you to build the correlation between lines in your high-level source code and the executed assembly instructions.
Building SASS source correlation for a PC can be split into two parts:

- Correlation of the PC to SASS instruction - subscribe to any one of the `CUPTI_CBID_RESOURCE_MODULE_LOADED`, `CUPTI_CBID_RESOURCE_MODULE_UNLOAD_STARTING`, or `CUPTI_CBID_RESOURCE_MODULE_PROFILED` callbacks. This returns a `CUpti_ModuleResourceData` structure having the CUDA binary. The binary can be disassembled using the nvdisasm utility that comes with the CUDA toolkit. An application can have multiple functions and modules, to uniquely identify there is a `functionId` field in all source level activity records. This uniquely corresponds to a `CUPTI_ACTIVITY_KIND_FUNCTION`, which has the unique module ID and function ID in the module.
- Correlation of the SASS instruction to CUDA source line - every source level activity has a `sourceLocatorId` field which uniquely maps to a record of kind `CUPTI_ACTIVITY_KIND_SOURCE_LOCATOR`, containing the line and file name information. Please note that multiple PCs can correspond to a single source line.

When any source level activity (global access, branch, PC Sampling, etc.) is enabled, a source locator record is generated for the PCs that have the source level results. The record `CUpti_ActivityInstructionCorrelation` can be used, along with source level activities, to generate SASS assembly instructions to CUDA C source code mapping for all the PCs of the function, and not just the PCs that have the source level results. This can be enabled using the activity kind `CUPTI_ACTIVITY_KIND_INSTRUCTION_CORRELATION`.

The sass_source_map sample shows how to map SASS assembly instructions to CUDA C source.

#### 2.3.2. PC Sampling

CUPTI supports device-wide sampling of the program counter (PC). The PC Sampling gives the number of samples for each source and assembly line with various stall reasons. Using this information, you can pinpoint portions of your kernel that are introducing latencies and the reason for the latency. Samples are taken in round robin order for all active warps at a fixed number of cycles, regardless of whether the warp is issuing an instruction or not.

Devices with compute capability 6.0 and higher have a new feature that gives latency reasons. The latency samples indicate the reasons for holes in the issue pipeline. While collecting these samples, there is no instruction issued in the respective warp scheduler, hence these give the latency reasons. The latency reasons will be one of the stall reasons listed in the enum `CUpti_ActivityPCSamplingStallReason`, except stall reason `CUPTI_ACTIVITY_PC_SAMPLING_STALL_NOT_SELECTED`.

The activity record `CUpti_ActivityPCSampling3`, enabled using activity kind `CUPTI_ACTIVITY_KIND_PC_SAMPLING`, outputs the stall reason along with PC and other related information. The enum `CUpti_ActivityPCSamplingStallReason` lists all the stall reasons. Sampling period is configurable and can be tuned using API `cuptiActivityConfigurePCSampling`. A wide range of sampling periods, ranging from 2^5 cycles to 2^31 cycles per sample, is supported. This can be controlled through the field `samplingPeriod2` in the PC sampling configuration struct `CUpti_ActivityPCSamplingConfig`. The activity record `CUpti_ActivityPCSamplingRecordInfo` provides the total and dropped samples for each kernel profiled for PC sampling.

This feature is available on devices with compute capability 5.2 and higher, excluding mobile devices. For Pascal and older chips `cuptiActivityConfigurePCSampling` api must be called before enabling activity kind `CUPTI_ACTIVITY_KIND_PC_SAMPLING`, for Volta and newer chips order does not matter. For Volta and newer GPU architectures if `cuptiActivityConfigurePCSampling` API is called in the middle of execution, PC sampling configuration will be updated for subsequent kernel launches. PC sampling can significantly change the overall performance characteristics of the application because all kernel executions are serialized on the GPU.

The pc_sampling sample shows how to use these APIs to collect PC Sampling profiling information for a kernel.

Note: A new set of PC Sampling APIs was introduced in the CUDA 11.3 release, which supports continuous mode data collection without serializing kernel execution and have a lower runtime overhead. Refer to the section CUPTI PC Sampling API for more details. PC Sampling APIs from the header `cupti_activity.h` would be referred as PC Sampling Activity APIs and APIs from the header `cupti_pcsampling.h` would be referred as PC Sampling APIs.

#### 2.3.3. NVLink

NVIDIA NVLink is a high-bandwidth, energy-efficient interconnect that enables fast communication between the CPU and GPU, and between GPUs. CUPTI provides NVLink topology information and NVLink transmit/receive throughput metrics.

The activity record `CUpti_ActivityNVLink3`, enabled using activity kind `CUPTI_ACTIVITY_KIND_NVLink`, outputs NVLink topology information in terms of logical NVLinks. A logical NVLink is connected between 2 devices, the device can be of type NPU (NVLink Processing Unit), which can be CPU or GPU. Each device can support up to 12 NVLinks, hence one logical link can comprise of 1 to 12 physical NVLinks. The field `physicalNvLinkCount` gives the number of physical links in this logical link. The fields `portDev0` and `portDev1` give information about the slot in which physical NVLinks are connected for a logical link. This port is the same as the instance of NVLink metrics profiled from a device. Therefore, port and instance information should be used to correlate the per-instance metric values with the physical NVLinks, and in turn to the topology. The field `flag` gives the properties of a logical link, whether the link has access to system memory or peer device memory, and has capabilities to do system memory or peer memmory atomics. The field `bandwidth` gives the bandwidth of the logical link in kilobytes/sec.

CUPTI provides some metrics for each physical link. Metrics are provided for data transmitted/received, transmit/receive throughput, and header versus user data overhead for each physical NVLink. These metrics are also provided per packet type (read/write/ atomics/response) to get more detailed insight in the NVLink traffic.

This feature is available on devices with compute capability 6.0 and 7.0. For devices with compute capability 8.0, the NVLink topology information is available but NVLink performance metrics (`nvlrx__*` and `nvltx__*`) are not supported due to a potential application hang during data collection.

The nvlink_bandwidth sample shows how to use these APIs to collect NVLink metrics and topology, as well as how to correlate metrics with the topology.

#### 2.3.4. OpenACC

CUPTI supports collecting information for OpenACC applications using the OpenACC tools interface implementation of the PGI runtime. OpenACC profiling is available only on Linux x86_64, IBM POWER and Arm server platform (arm64 SBSA) platforms. This feature also requires PGI runtime version 19.1 or higher.
The activity records `CUpti_ActivityOpenAccData`, `CUpti_ActivityOpenAccLaunch`, and `CUpti_ActivityOpenAccOther` are created, representing the three groups of callback events specified in the OpenACC tools interface. `CUPTI_ACTIVITY_KIND_OPENACC_DATA`, `CUPTI_ACTIVITY_KIND_OPENACC_LAUNCH`, and `CUPTI_ACTIVITY_KIND_OPENACC_OTHER` can be enabled to collect the respective activity records.
Due to the restrictions of the OpenACC tools interface, CUPTI cannot record OpenACC records from within the client application. Instead, a shared library that exports the `acc_register_library` function defined in the OpenACC tools interface specification must be implemented. Parameters passed into this function from the OpenACC runtime can be used to initialize the CUPTI OpenACC measurement using `cuptiOpenACCInitialize`. Before starting the client application, the environment variable `ACC_PROFLIB` must be set to point to this shared library.
`cuptiOpenACCInitialize` is defined in `cupti_openacc.h`, which is included by `cupti_activity.h`. Since the CUPTI OpenACC header is only available on supported platforms, CUPTI clients must define `CUPTI_OPENACC_SUPPORT` when compiling.
The openacc_trace sample shows how to use CUPTI APIs for OpenACC data collection.

#### 2.3.5. CUDA Graphs

CUPTI can collect trace of CUDA Graphs applications without breaking driver performance optimizations. CUPTI has added fields `graphId` and `graphNodeId` in the kernel, memcpy and memset activity records to denote the unique ID of the graph and the graph node respectively of the GPU activity. CUPTI issues callbacks for graph operations like graph and graph node creation/destruction/cloning and also for executable graph creation/destruction. The cuda_graphs_trace sample shows how to collect GPU trace and API trace for CUDA Graphs and how to correlate a graph node launch to the node creation API by using CUPTI callbacks for graph operations.

#### 2.3.6. External Correlation

CUPTI supports correlation of CUDA API activity records with external APIs. Such APIs include OpenACC, OpenMP, and MPI. This associates CUPTI correlation IDs with IDs provided by the external API. Both IDs are stored in a new activity record of type `CUpti_ActivityExternalCorrelation`.
CUPTI maintains a stack of external correlation IDs per CPU thread and per `CUpti_ExternalCorrelationKind`. Clients must use `cuptiActivityPushExternalCorrelationId` to push an external ID of a specific kind to this stack and `cuptiActivityPopExternalCorrelationId` to remove the latest ID. If a CUDA API activity record is generated while any `CUpti_ExternalCorrelationKind`-stack on the same CPU thread is non-empty, one `CUpti_ActivityExternalCorrelation` record per `CUpti_ExternalCorrelationKind`-stack is inserted into the activity buffer before the respective CUDA API activity record. The CUPTI client is responsible for tracking passed external API correlation IDs, in order to eventually associate external API calls with CUDA API calls. Along with the activity kind `CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION`, it is necessary to enable the CUDA API activity kinds i.e. `CUPTI_ACTIVITY_KIND_RUNTIME` and `CUPTI_ACTIVITY_KIND_DRIVER` to generate external correlation activity records.
If both `CUPTI_ACTIVITY_KIND_EXTERNAL_CORRELATION` and any of `CUPTI_ACTIVITY_KIND_OPENACC_*` activity kinds are enabled, CUPTI will generate external correlation activity records for OpenACC with `externalKind` `CUPTI_EXTERNAL_CORRELATION_KIND_OPENACC`.
The cupti_external_correlation sample shows how to use CUPTI APIs for external correlation.

#### 2.3.7. Dynamic Attach and Detach

CUPTI provides mechanisms for attaching to or detaching from a running process to support on-demand profiling. CUPTI can be attached by calling any CUPTI API as CUPTI supports lazy initialization. To detach CUPTI, call the API `cuptiFinalize()` which destroys and cleans up all the resources associated with CUPTI in the current process. After CUPTI detaches from the process, the process will keep on running with no CUPTI attached to it. Any subsequent CUPTI API call will reinitialize the CUPTI. You can attach and detach CUPTI any number of times. For safe operation of the API, it is recommended that API `cuptiFinalize()` is invoked from the exit call site of any of the CUDA Driver or Runtime API. Otherwise, CUPTI client needs to make sure that CUDA synchronization and CUPTI activity buffer flush is done before calling the API `cuptiFinalize()`. To understand the need for calling the API `cuptiFinalize()` from specific point/s in the code flow, consider multiple application threads performing various CUDA activities. While one thread is in the middle of the `cuptiFinalize()`, it is quite possible that other threads continue to call into the CUPTI and try to access the state of various objects (device, context, thread state etc) maintained by CUPTI, which might be rendered invalid as part of the `cuptiFinalize()`, thus resulting in the crash. We have to block the other threads until CUPTI teardown is completed via `cuptiFinalize()`. API exit call site is one such location where we can ensure that the work submitted by all the threads has been completed and we can safely teardown CUPTI. `cuptiFinalize()` is a heavy operation as it does context synchronization for all active CUDA contexts and blocks all the application threads until CUPTI teardown is completed. Sample code showing the usage of the API `cuptiFinalize()` in the cupti callback handler code:

    void CUPTIAPI
    cuptiCallbackHandler(void *userdata, CUpti_CallbackDomain domain,
        CUpti_CallbackId cbid, void *cbdata)
    {
        const CUpti_CallbackData *cbInfo = (CUpti_CallbackData *)cbdata;

        // Take this code path when CUPTI detach is requested
        if (detachCupti) {
            switch(domain)
            {
            case CUPTI_CB_DOMAIN_RUNTIME_API:
            case CUPTI_CB_DOMAIN_DRIVER_API:
                if (cbInfo->callbackSite == CUPTI_API_EXIT) {
                    // call the CUPTI detach API
                    cuptiFinalize();
                }
                break;
            default:
                break;
            }
        }
    }

Full code can be found in the sample cupti_finalize.

### 2.4. CUPTI Callback API

The CUPTI Callback API allows you to register a callback into your own code. Your callback will be invoked when the application being profiled calls a CUDA runtime or driver function, or when certain events occur in the CUDA driver. The following terminology is used by the callback API.

Callback Domain
  Callbacks are grouped into domains to make it easier to associate your callback functions with groups of related CUDA functions or events. There are currently four callback domains, as defined by `CUpti_CallbackDomain`: a domain for CUDA runtime functions, a domain for CUDA driver functions, a domain for CUDA resource tracking, and a domain for CUDA synchronization notification.
Callback ID
  Each callback is given a unique ID within the corresponding callback domain so that you can identify it within your callback function. The CUDA driver API IDs are defined in `cupti_driver_cbid.h` and the CUDA runtime API IDs are defined in `cupti_runtime_cbid.h`. Both of these headers are included for you when you include `cupti.h`. The CUDA resource callback IDs are defined by `CUpti_CallbackIdResource`, and the CUDA synchronization callback IDs are defined by `CUpti_CallbackIdSync`.
Callback Function
  Your callback function must be of type `CUpti_CallbackFunc`. This function type has two arguments that specify the callback domain and ID so that you know why the callback is occurring. The type also has a `cbdata` argument that is used to pass data specific to the callback.
Subscriber
  A subscriber is used to associate each of your callback functions with one or more CUDA API functions. There can be at most one subscriber initialized with `cuptiSubscribe()` at any time. Before initializing a new subscriber, the existing subscriber must be finalized with `cuptiUnsubscribe()`.

Each callback domain is described in detail below. Unless explicitly stated, it is not supported to call any CUDA runtime or driver API from within a callback function. Doing so may cause the application to hang.

#### 2.4.1. Driver and Runtime API Callbacks

Using the callback API with the `CUPTI_CB_DOMAIN_DRIVER_API` or `CUPTI_CB_DOMAIN_RUNTIME_API` domains, you can associate a callback function with one or more CUDA API functions. When those CUDA functions are invoked in the application, your callback function is invoked as well. For these domains, the `cbdata` argument to your callback function will be of the type `CUpti_CallbackData`.

It is legal to call `cudaThreadSynchronize()`, `cudaDeviceSynchronize()`, `cudaStreamSynchronize()`, `cuCtxSynchronize()`, and `cuStreamSynchronize()` from within a driver or runtime API callback function.

The following code shows a typical sequence used to associate a callback function with one or more CUDA API functions. To simplify the presentation, error checking code has been removed.

      CUpti_SubscriberHandle subscriber;
      MyDataStruct *my_data = ...;
      ...
      cuptiSubscribe(&subscriber,
                     (CUpti_CallbackFunc)my_callback , my_data);
      cuptiEnableDomain(1, subscriber,
                        CUPTI_CB_DOMAIN_RUNTIME_API);

First, `cuptiSubscribe` is used to initialize a subscriber with the `my_callback` callback function. Next, `cuptiEnableDomain` is used to associate that callback with all the CUDA runtime API functions. Using this code sequence will cause `my_callback` to be called twice each time any of the CUDA runtime API functions are invoked, once on entry to the CUDA function and once just before exit from the CUDA function. CUPTI callback API functions `cuptiEnableCallback` and `cuptiEnableAllDomains` can also be used to associate CUDA API functions with a callback (see reference below for more information).

The following code shows a typical callback function.

    void CUPTIAPI
    my_callback(void *userdata, CUpti_CallbackDomain domain,
                CUpti_CallbackId cbid, const void *cbdata)
    {
      const CUpti_CallbackData *cbInfo = (CUpti_CallbackData *)cbdata;
      MyDataStruct *my_data = (MyDataStruct *)userdata;

      if ((domain == CUPTI_CB_DOMAIN_RUNTIME_API) &&
          (cbid == CUPTI_RUNTIME_TRACE_CBID_cudaMemcpy_v3020))  {
        if (cbInfo->callbackSite == CUPTI_API_ENTER) {
            cudaMemcpy_v3020_params *funcParams =
                 (cudaMemcpy_v3020_params *)(cbInfo->
                     functionParams);

            size_t count = funcParams->count;
            enum cudaMemcpyKind kind = funcParams->kind;
            ...
          }
      ...

In your callback function, you use the `CUpti_CallbackDomain` and `CUpti_CallbackID` parameters to determine which CUDA API function invocation is causing this callback. In the example above, we are checking for the CUDA runtime `cudaMemcpy` function. The `cbdata` parameter holds a structure of useful information that can be used within the callback. In this case, we use the `callbackSite` member of the structure to detect that the callback is occurring on entry to `cudaMemcpy`, and we use the `functionParams` member to access the parameters that were passed to `cudaMemcpy`. To access the parameters, we first cast `functionParams` to a structure type corresponding to the `cudaMemcpy` function. These parameter structures are contained in `generated_cuda_runtime_api_meta.h`, `generated_cuda_meta.h`, and a number of other files. When possible, these files are included for you by `cupti.h`.

The callback_event and callback_timestamp samples described on the samples page both show how to use the callback API for the driver and runtime API domains.

#### 2.4.2. Resource Callbacks

Using the callback API with the `CUPTI_CB_DOMAIN_RESOURCE` domain, you can associate a callback function with some CUDA resource creation and destruction events. For example, when a CUDA context is created, your callback function will be invoked with a callback ID equal to `CUPTI_CBID_RESOURCE_CONTEXT_CREATED`. For this domain, the `cbdata` argument to your callback function will be of the type `CUpti_ResourceData`.

Note that APIs `cuptiActivityFlush` and `cuptiActivityFlushAll` will result in deadlock when called from stream destroy starting callback identified using callback ID `CUPTI_CBID_RESOURCE_STREAM_DESTROY_STARTING`.

#### 2.4.3. Synchronization Callbacks

Using the callback API with the `CUPTI_CB_DOMAIN_SYNCHRONIZE` domain, you can associate a callback function with CUDA context and stream synchronizations. For example, when a CUDA context is synchronized, your callback function will be invoked with a callback ID equal to `CUPTI_CBID_SYNCHRONIZE_CONTEXT_SYNCHRONIZED`. For this domain, the `cbdata` argument to your callback function will be of the type `CUpti_SynchronizeData`.

#### 2.4.4. NVIDIA Tools Extension Callbacks

Using the callback API with the `CUPTI_CB_DOMAIN_NVTX` domain, you can associate a callback function with NVIDIA Tools Extension (NVTX) API functions. When an NVTX function is invoked in the application, your callback function is invoked as well. For these domains, the `cbdata` argument to your callback function will be of the type `CUpti_NvtxData`.

The NVTX library has its own convention for discovering the profiling library that will provide the implementation of the NVTX callbacks. To receive callbacks, you must set the NVTX environment variables appropriately so that when the application calls an NVTX function, your profiling library receives the callbacks. The following code sequence shows a typical initialization sequence to enable NVTX callbacks and activity records.

    /* Set env so CUPTI-based profiling library loads on first nvtx call. */
    char *inj32_path = "/path/to/32-bit/version/of/cupti/based/profiling/library";
    char *inj64_path = "/path/to/64-bit/version/of/cupti/based/profiling/library";
    setenv("NVTX_INJECTION32_PATH", inj32_path, 1);
    setenv("NVTX_INJECTION64_PATH", inj64_path, 1);

The following code shows a typical sequence used to associate a callback function with one or more NVTX functions. To simplify the presentation, error checking code has been removed.

    CUpti_SubscriberHandle subscriber;
    MyDataStruct *my_data = ...;
    ...
    cuptiSubscribe(&subscriber,
                   (CUpti_CallbackFunc)my_callback , my_data);
    cuptiEnableDomain(1, subscriber,
                      CUPTI_CB_DOMAIN_NVTX);

First, `cuptiSubscribe` is used to initialize a subscriber with the `my_callback` callback function. Next, `cuptiEnableDomain` is used to associate that callback with all the NVTX functions. Using this code sequence will cause `my_callback` to be called once each time any of the NVTX functions are invoked. CUPTI callback API functions `cuptiEnableCallback` and `cuptiEnableAllDomains` can also be used to associate NVTX API functions with a callback (see reference below for more information).

The following code shows a typical callback function.

    void CUPTIAPI
    my_callback(void *userdata, CUpti_CallbackDomain domain,
                CUpti_CallbackId cbid, const void *cbdata)
    {
      const CUpti_NvtxData *nvtxInfo = (CUpti_NvtxData *)cbdata;
      MyDataStruct *my_data = (MyDataStruct *)userdata;

      if ((domain == CUPTI_CB_DOMAIN_NVTX) &&
          (cbid == CUPTI_CBID_NVTX_nvtxRangeStartEx))  {
        nvtxRangeStartEx_params *params = (nvtxRangeStartEx_params *)nvtxInfo->
                 functionParams;
        nvtxRangeId_t *id = (nvtxRangeId_t *)nvtxInfo->functionReturnValue;
        ...
      }
      ...

In your callback function, you use the `CUpti_CallbackDomain` and `CUpti_CallbackID` parameters to determine which NVTX API function invocation is causing this callback. In the example above, we are checking for the `nvtxRangeStartEx` function. The `cbdata` parameter holds a structure of useful information that can be used within the callback. In this case, we use the `functionParams` member to access the parameters that were passed to `nvtxRangeStartEx`. To access the parameters, we first cast `functionParams` to a structure type corresponding to the `nvtxRangeStartEx` function. These parameter structures are contained in `generated_nvtx_meta.h`. We also use `functionReturnValue` member to access the value returned by `nvtxRangeStartEx`. To access the return value, we first cast `functionReturnValue` to the return type corresponding to the `nvtxRangeStartEx` function. If there is no return value for the NVTX function, `functionReturnValue` is NULL.

The sample cupti_nvtx shows the initialization sequence to enable NVTX callbacks and activity records.

If your CUPTI-based profiling library links static CUPTI library, you can define and export your own NvtxInitializeInjection and NvtxInitializeInjection2 functions, which would be called by setting the NVTX environment variables.

If you want CUPTI to handle NVTX calls, these functions should call CUPTI's corresponding initialization functions, as shown in the example below so that when the application calls a NVTX function, your profiling library receives the callbacks. The following code sequence shows how this can be done to receive callbacks and activity records when linking static CUPTI library.

    /* Set env so CUPTI-based profiling library loads on first nvtx call. */
    char *inj32_path = "/path/to/32-bit/version/of/cupti/based/profiling/library";
    char *inj64_path = "/path/to/64-bit/version/of/cupti/based/profiling/library";
    setenv("NVTX_INJECTION32_PATH", inj32_path, 1);
    setenv("NVTX_INJECTION64_PATH", inj64_path, 1);

    /* Extern the CUPTI NVTX initialization APIs. The APIs are thread-safe */
    extern "C" CUptiResult CUPTIAPI cuptiNvtxInitialize(void* pfnGetExportTable);
    extern "C" CUptiResult CUPTIAPI cuptiNvtxInitialize2(void* pfnGetExportTable);

    extern "C" int InitializeInjectionNvtx(void* p)
    {
      CUptiResult res = cuptiNvtxInitialize(p);
      return (res == CUPTI_SUCCESS) ? 1 : 0;
    }

    extern "C" int InitializeInjectionNvtx2(void* p)
    {
      CUptiResult res = cuptiNvtxInitialize2(p);
      return (res == CUPTI_SUCCESS) ? 1 : 0;
    }

Alternatively, if you want to handle NVTX calls directly in your profiling library, you can attach your own callbacks to the NVTX client in these functions.

NVTX v1 and v2 both have the initialization code in a single injection library shared by all users of NVTX in the whole process, so the initialization will happen only once per process. NVTX v3 embeds the initialization code into your own binaries, so if NVTX v3 is in multiple dynamic libraries, each one of those sites will initialize the first time a NVTX call is made from that dynamic library. These first calls could be on different threads. So if you are wiring up your own NVTX handlers, you should ensure that code is thread-safe when called from multiple threads at once.

### 2.5. CUPTI Event API

The CUPTI Event API allows you to query, configure, start, stop, and read the event counters on a CUDA-enabled device. The following terminology is used by the event API.

Event
  An event is a countable activity, action, or occurrence on a device.
Event ID
  Each event is assigned a unique identifier. A named event will represent the same activity, action, or occurrence on all device types. But the named event may have different IDs on different device families. Use `cuptiEventGetIdFromName` to get the ID for a named event on a particular device.
Event Category
  Each event is placed in one of the categories defined by `CUpti_EventCategory`. The category indicates the general type of activity, action, or occurrence measured by the event.
Event Domain
  A device exposes one or more event domains. Each event domain represents a group of related events available on that device. A device may have multiple instances of a domain, indicating that the device can simultaneously record multiple instances of each event within that domain.
Event Group
  An event group is a collection of events that are managed together. The number and type of events that can be added to an event group are subject to device-specific limits. At any given time, a device may be configured to count events from a limited number of event groups. All events in an event group must belong to the same event domain.
Event Group Set
  An event group set is a collection of event groups that can be enabled at the same time. Event group sets are created by `cuptiEventGroupSetsCreate` and `cuptiMetricCreateEventGroupSets`.

You can determine the events available on a device using the `cuptiDeviceEnumEventDomains` and `cuptiEventDomainEnumEvents` functions. The cupti_query sample described on the samples page shows how to use these functions. You can also enumerate all the CUPTI events available on any device using the `cuptiEnumEventDomains` function.

Configuring and reading event counts requires the following steps. First, select your event collection mode. If you want to count events that occur during the execution of a kernel, use `cuptiSetEventCollectionMode` to set mode `CUPTI_EVENT_COLLECTION_MODE_KERNEL`. If you want to continuously sample the event counts, use mode `CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS`. Next, determine the names of the events that you want to count, and then use the `cuptiEventGroupCreate`, `cuptiEventGetIdFromName`, and `cuptiEventGroupAddEvent` functions to create and initialize an event group with those events. If you are unable to add all the events to a single event group, then you will need to create multiple event groups. Alternatively, you can use the `cuptiEventGroupSetsCreate` function to automatically create the event group(s) required for a set of events.

It's possible that all the requested events can't be collected in the single pass due to hardware or software limitations, one needs to replay the exact same set of GPU workloads multiple times. Number of passes can be queried using the API `cuptiEventGroupSetsCreate`. Profiling one event always takes single pass. Multiple passes might be required when we want to profile multiple events together. Code snippet showing how to query number of passes:

    CUpti_EventGroupSets *eventGroupSets = NULL;
    size_t eventIdArraySize = sizeof(CUpti_EventID) * numEvents;
    CUpti_EventID *eventIdArray = (CUpti_EventID *)malloc(sizeof(CUpti_EventID) * numEvents);
    // fill in event Ids
    cuptiEventGroupSetsCreate(context, eventIdArraySize, eventIdArray, &eventGroupSets);
    // number of passes required to collect all the events
    passes = eventGroupSets->numSets;

To begin counting a set of events, enable the event group or groups that contain those events by using the `cuptiEventGroupEnable` function. If your events are contained in multiple event groups, you may be unable to enable all of the event groups at the same time i.e. in the same pass. In this case, you can gather the events across multiple executions of the application or you can enable kernel replay. If you enable kernel replay using `cuptiEnableKernelReplayMode`, you will be able to enable any number of event groups and all the contained events will be collected.

Use the `cuptiEventGroupReadEvent` and/or `cuptiEventGroupReadAllEvents` functions to read the event values. When you are done collecting events, use the `cuptiEventGroupDisable` function to stop counting the events contained in an event group. The callback_event sample described on the samples page shows how to use these functions to create, enable, and disable event groups, and how to read event counts.

Note: For event collection mode `CUPTI_EVENT_COLLECTION_MODE_KERNEL`, event or metric collection may significantly change the overall performance characteristics of the application because all kernel executions that occur between the `cuptiEventGroupEnable` and `cuptiEventGroupDisable` calls are serialized on the GPU. This can be avoided by using mode `CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS`, and restricting profiling to events and metrics that can be collected in a single pass.
Note: All the events and metrics except NVLink metrics are collected at the context level, irrespective of the event collection mode. That is, events or metrics can be attributed to the context being profiled and values can be accurately collected, when multiple contexts are executing on the GPU. NVLink metrics are collected at device level for all event collection modes.

In a system with multiple GPUs, events can be collected simultaneously on all the GPUs; in other words, event profiling doesn't enforce any serialization of work across GPUs. The event_multi_gpu sample shows how to use the CUPTI event and CUDA APIs on such setups.

Note: Event APIs from the header `cupti_events.h` are not supported for devices with compute capability 7.5 and higher. It is advised to use the CUPTI Profiling API instead. Refer to the section Migration to the Profiling API.

#### 2.5.1. Collecting Kernel Execution Events

A common use of the event API is to count a set of events during the execution of a kernel (as demonstrated by the callback_event sample). The following code shows a typical callback used for this purpose. Assume that the callback was enabled only for a kernel launch using the CUDA runtime (i.e., by `cuptiEnableCallback(1, subscriber, CUPTI_CB_DOMAIN_RUNTIME_API, CUPTI_RUNTIME_TRACE_CBID_cudaLaunch_v3020)`. To simplify the presentation, error checking code has been removed.

    static void CUPTIAPI
    getEventValueCallback(void *userdata,
                          CUpti_CallbackDomain domain,
                          CUpti_CallbackId cbid,
                          const void *cbdata)
    {
      const CUpti_CallbackData *cbData =
                    (CUpti_CallbackData *)cbdata;

      if (cbData->callbackSite == CUPTI_API_ENTER) {
        cudaDeviceSynchronize();
        cuptiSetEventCollectionMode(cbInfo->context,
                                    CUPTI_EVENT_COLLECTION_MODE_KERNEL);
        cuptiEventGroupEnable(eventGroup);
      }

      if (cbData->callbackSite == CUPTI_API_EXIT) {
        cudaDeviceSynchronize();
        cuptiEventGroupReadEvent(eventGroup,
                                 CUPTI_EVENT_READ_FLAG_NONE,
                                 eventId,
                                 &bytesRead, &eventVal);

        cuptiEventGroupDisable(eventGroup);
      }
    }

Two synchronization points are used to ensure that events are counted only for the execution of the kernel. If the application contains other threads that launch kernels, then additional thread-level synchronization must also be introduced to ensure that those threads do not launch kernels while the callback is collecting events. When the cudaLaunch API is entered (that is, before the kernel is actually launched on the device), `cudaDeviceSynchronize` is used to wait until the GPU is idle. The event collection mode is set to `CUPTI_EVENT_COLLECTION_MODE_KERNEL` so that the event counters are automatically started and stopped just before and after the kernel executes. Then event collection is enabled with `cuptiEventGroupEnable`.

When the cudaLaunch API is exited (that is, after the kernel is queued for execution on the GPU) another `cudaDeviceSynchronize` is used to cause the CPU thread to wait for the kernel to finish execution. Finally, the event counts are read with `cuptiEventGroupReadEvent`.

#### 2.5.2. Sampling Events

The event API can also be used to sample event values while a kernel or kernels are executing (as demonstrated by the event_sampling sample). The sample shows one possible way to perform the sampling. The event collection mode is set to `CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS` so that the event counters run continuously. Two threads are used in event_sampling: one thread schedules the kernels and memcpys that perform the computation, while another thread wakes up periodically to sample an event counter. In this sample, there is no correlation of the event samples with what is happening on the GPU. To get some coarse correlation, you can use `cuptiDeviceGetTimestamp` to collect the GPU timestamp at the time of the sample and also at other interesting points in your application.

### 2.6. CUPTI Metric API

The CUPTI Metric API allows you to collect application metrics calculated from one or more event values. The following terminology is used by the metric API.

Metric
  A characteristic of an application that is calculated from one or more event values.
Metric ID
  Each metric is assigned a unique identifier. A named metric will represent the same characteristic on all device types. But the named metric may have different IDs on different device families. Use `cuptiMetricGetIdFromName` to get the ID for a named metric on a particular device.
Metric Category
  Each metric is placed in one of the categories defined by `CUpti_MetricCategory`. The category indicates the general type of the characteristic measured by the metric.
Metric Property
  Each metric is calculated from input values. These input values can be events or properties of the device or system. The available properties are defined by `CUpti_MetricPropertyID`.
Metric Value
  Each metric has a value that represents one of the kinds defined by `CUpti_MetricValueKind`. For each value kind, there is a corresponding member of the `CUpti_MetricValue` union that is used to hold the metric's value.

The tables included in this section list the metrics available for each device, as determined by the device's compute capability. You can also determine the metrics available on a device using the `cuptiDeviceEnumMetrics` function. The cupti_query sample described on the samples page shows how to use this function. You can also enumerate all the CUPTI metrics available on any device using the `cuptiEnumMetrics` function.

CUPTI provides two functions for calculating a metric value. `cuptiMetricGetValue2` can be used to calculate a metric value when the device is not available. All required event values and metric properties must be provided by the caller. `cuptiMetricGetValue` can be used to calculate a metric value when the device is available (as a CUdevice object). All required event values must be provided by the caller, but CUPTI will determine the appropriate property values from the CUdevice object.

Configuring and calculating metric values requires the following steps. First, determine the name of the metric that you want to collect, and then use the `cuptiMetricGetIdFromName` to get the metric ID. Use `cuptiMetricEnumEvents` to get the events required to calculate the metric, and follow instructions in the CUPTI Event API section to create the event groups for those events. When creating event groups in this manner, it is important to use the result of `cuptiMetricGetRequiredEventGroupSets` to properly group together events that must be collected in the same pass to ensure proper metric calculation.

Alternatively, you can use the `cuptiMetricCreateEventGroupSets` function to automatically create the event group(s) required for metrics' events. When using this function, events will be grouped as required to most accurately calculate the metric; as a result, it is not necessary to use `cuptiMetricGetRequiredEventGroupSets`.

If you are using `cuptiMetricGetValue2`, then you must also collect the required metric property values using `cuptiMetricEnumProperties`.

Collect event counts as described in the CUPTI Event API section, and then use either `cuptiMetricGetValue` or `cuptiMetricGetValue2` to calculate the metric value from the collected event and property values. The callback_metric sample described on the samples page shows how to use the functions to calculate event values and calculate a metric using `cuptiMetricGetValue`. Note that as shown in the example, you should collect event counts from all domain instances, and normalize the counts to get the most accurate metric values. It is necessary to normalize the event counts because the number of event counter instances varies by device and by the event being counted.

For example, a device might have 8 multiprocessors but only have event counters for 4 of the multiprocessors, and might have 3 memory units and only have events counters for one memory unit. When calculating a metric that requires a multiprocessor event and a memory unit event, the 4 multiprocessor counters should be summed and multiplied by 2 to normalize the event count across the entire device. Similarly, the one memory unit counter should be multiplied by 3 to normalize the event count across the entire device. The normalized values can then be passed to `cuptiMetricGetValue` or `cuptiMetricGetValue2` to calculate the metric value.

As described, the normalization assumes the kernel executes a sufficient number of blocks to completely load the device. If the kernel has only a small number of blocks, normalizing across the entire device may skew the result.

It's possible that all the requested metrics can't be collected in the single pass due to hardware or software limitations, one needs to replay the exact same set of GPU workloads multiple times. Number of passes can be queried using the API `cuptiMetricCreateEventGroupSets`. Profiling a single metric can also take multiple passes depending on the number and type of events it is calculated from. Code snippet showing how to query number of passes:

    CUpti_EventGroupSets *eventGroupSets = NULL;
    size_t metricIdArraySize = sizeof(CUpti_MetricID) * numMetrics;
    CUpti_MetricID metricIdArray = (CUpti_MetricID *)malloc(sizeof(CUpti_MetricID) * numMetrics);
    // fill in metric Ids
    cuptiMetricCreateEventGroupSets(context, metricIdArraySize, metricIdArray, &eventGroupSets);
    // number of passes required to collect all the metrics
    passes = eventGroupSets->numSets;

Note: Metric APIs from the header `cupti_metrics.h` are not supported for devices with compute capability 7.5 and higher. It is advised to use the CUPTI Profiling API instead. Refer to the section Migration to the Profiling API.

#### 2.6.1. Metrics Reference

This section contains detailed descriptions of the metrics that can be collected by the CUPTI. A scope value of "Single-context" indicates that the metric can only be accurately collected when a single context (CUDA or graphics) is executing on the GPU. A scope value of "Multi-context" indicates that the metric can be accurately collected when multiple contexts are executing on the GPU. A scope value of "Device" indicates that the metric will be collected at device level, that is, it will include values for all the contexts executing on the GPU.

##### 2.6.1.1. Metrics for Capability 3.x

Devices with compute capability 3.x implement the metrics shown in the following table. Note that for some metrics, the "Multi-context" scope is supported only for specific devices. Such metrics are marked with "Multi-context*" under the "Scope" column. Refer to the note at the bottom of the table.

Table 1. Capability 3.x Metrics
Metric Name | Description | Scope
--- | --- | ---
achieved_occupancy | Ratio of the average active warps per active cycle to the maximum number of warps supported on a multiprocessor | Multi-context
alu_fu_utilization | The utilization level of the multiprocessor function units that execute integer and floating-point arithmetic instructions on a scale of 0 to 10 | Multi-context
atomic_replay_overhead | Average number of replays due to atomic and reduction bank conflicts for each instruction executed | Multi-context
atomic_throughput | Global memory atomic and reduction throughput | Multi-context
atomic_transactions | Global memory atomic and reduction transactions | Multi-context
atomic_transactions_per_request | Average number of global memory atomic and reduction transactions performed for each atomic and reduction instruction | Multi-context
branch_efficiency | Ratio of non-divergent branches to total branches expressed as percentage. This is available for compute capability 3.0. | Multi-context
cf_executed | Number of executed control-flow instructions | Multi-context
cf_fu_utilization | The utilization level of the multiprocessor function units that execute control-flow instructions on a scale of 0 to 10 | Multi-context
cf_issued | Number of issued control-flow instructions | Multi-context
dram_read_throughput | Device memory read throughput. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
dram_read_transactions | Device memory read transactions. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
dram_utilization | The utilization level of the device memory relative to the peak utilization on a scale of 0 to 10 | Multi-context*
dram_write_throughput | Device memory write throughput. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
dram_write_transactions | Device memory write transactions. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
ecc_throughput | ECC throughput from L2 to DRAM. This is available for compute capability 3.5 and 3.7. | Multi-context*
ecc_transactions | Number of ECC transactions between L2 and DRAM. This is available for compute capability 3.5 and 3.7. | Multi-context*
eligible_warps_per_cycle | Average number of warps that are eligible to issue per active cycle | Multi-context
flop_count_dp | Number of double-precision floating-point operations executed by non-predicated threads (add, multiply and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. | Multi-context
flop_count_dp_add | Number of double-precision floating-point add operations executed by non-predicated threads | Multi-context
flop_count_dp_fma | Number of double-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_dp_mul | Number of double-precision floating-point multiply operations executed by non-predicated threads | Multi-context
flop_count_sp | Number of single-precision floating-point operations executed by non-predicated threads (add, multiply and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. The count does not include special operations. | Multi-context
flop_count_sp_add | Number of single-precision floating-point add operations executed by non-predicated threads | Multi-context
flop_count_sp_fma | Number of single-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_sp_mul | Number of single-precision floating-point multiply operations executed by non-predicated threads | Multi-context
flop_count_sp_special | Number of single-precision floating-point special operations executed by non-predicated threads | Multi-context
flop_dp_efficiency | Ratio of achieved to peak double-precision floating-point operations | Multi-context
flop_sp_efficiency | Ratio of achieved to peak single-precision floating-point operations | Multi-context
gld_efficiency | Ratio of requested global memory load throughput to required global memory load throughput expressed as percentage | Multi-context*
gld_requested_throughput | Requested global memory load throughput | Multi-context
gld_throughput | Global memory load throughput | Multi-context*
gld_transactions | Number of global memory load transactions | Multi-context*
gld_transactions_per_request | Average number of global memory load transactions performed for each global memory load | Multi-context*
global_cache_replay_overhead | Average number of replays due to global memory cache misses for each instruction executed | Multi-context
global_replay_overhead | Average number of replays due to global memory cache misses | Multi-context
gst_efficiency | Ratio of requested global memory store throughput to required global memory store throughput expressed as percentage | Multi-context*
gst_requested_throughput | Requested global memory store throughput | Multi-context
gst_throughput | Global memory store throughput | Multi-context*
gst_transactions | Number of global memory store transactions | Multi-context*
gst_transactions_per_request | Average number of global memory store transactions performed for each global memory store | Multi-context*
inst_bit_convert | Number of bit-conversion instructions executed by non-predicated threads | Multi-context
inst_compute_ld_st | Number of compute load/store instructions executed by non-predicated threads | Multi-context
inst_control | Number of control-flow instructions executed by non-predicated threads (jump, branch, etc.) | Multi-context
inst_executed | The number of instructions executed | Multi-context
inst_fp_32 | Number of single-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_64 | Number of double-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_integer | Number of integer instructions executed by non-predicated threads | Multi-context
inst_inter_thread_communication | Number of inter-thread communication instructions executed by non-predicated threads | Multi-context
inst_issued | The number of instructions issued | Multi-context
inst_misc | Number of miscellaneous instructions executed by non-predicated threads | Multi-context
inst_per_warp | Average number of instructions executed by each warp | Multi-context
inst_replay_overhead | Average number of replays for each instruction executed | Multi-context
ipc | Instructions executed per cycle | Multi-context
ipc_instance | Instructions executed per cycle for a single multiprocessor | Multi-context
issue_slot_utilization | Percentage of issue slots that issued at least one instruction, averaged across all cycles | Multi-context
issue_slots | The number of issue slots used | Multi-context
issued_ipc | Instructions issued per cycle | Multi-context
l1_cache_global_hit_rate | Hit rate in L1 cache for global loads | Multi-context*
l1_cache_local_hit_rate | Hit rate in L1 cache for local loads and stores | Multi-context*
l1_shared_utilization | The utilization level of the L1/shared memory relative to peak utilization on a scale of 0 to 10. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_atomic_throughput | Memory read throughput seen at L2 cache for atomic and reduction requests | Multi-context*
l2_atomic_transactions | Memory read transactions seen at L2 cache for atomic and reduction requests | Multi-context*
l2_l1_read_hit_rate | Hit rate at L2 cache for all read requests from L1 cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_l1_read_throughput | Memory read throughput seen at L2 cache for read requests from L1 cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_l1_read_transactions | Memory read transactions seen at L2 cache for all read requests from L1 cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_l1_write_throughput | Memory write throughput seen at L2 cache for write requests from L1 cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_l1_write_transactions | Memory write transactions seen at L2 cache for all write requests from L1 cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_read_throughput | Memory read throughput seen at L2 cache for all read requests | Multi-context*
l2_read_transactions | Memory read transactions seen at L2 cache for all read requests | Multi-context*
l2_tex_read_transactions | Memory read transactions seen at L2 cache for read requests from the texture cache | Multi-context*
l2_tex_read_hit_rate | Hit rate at L2 cache for all read requests from texture cache. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
l2_tex_read_throughput | Memory read throughput seen at L2 cache for read requests from the texture cache | Multi-context*
l2_utilization | The utilization level of the L2 cache relative to the peak utilization on a scale of 0 to 10 | Multi-context*
l2_write_throughput | Memory write throughput seen at L2 cache for all write requests | Multi-context*
l2_write_transactions | Memory write transactions seen at L2 cache for all write requests | Multi-context*
ldst_executed | Number of executed local, global, shared and texture memory load and store instructions | Multi-context
ldst_fu_utilization | The utilization level of the multiprocessor function units that execute global, local and shared memory instructions on a scale of 0 to 10 | Multi-context
ldst_issued | Number of issued local, global, shared and texture memory load and store instructions | Multi-context
local_load_throughput | Local memory load throughput | Multi-context*
local_load_transactions | Number of local memory load transactions | Multi-context*
local_load_transactions_per_request | Average number of local memory load transactions performed for each local memory load | Multi-context*
local_memory_overhead | Ratio of local memory traffic to total memory traffic between the L1 and L2 caches expressed as percentage. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
local_replay_overhead | Average number of replays due to local memory accesses for each instruction executed | Multi-context
local_store_throughput | Local memory store throughput | Multi-context*
local_store_transactions | Number of local memory store transactions | Multi-context*
local_store_transactions_per_request | Average number of local memory store transactions performed for each local memory store | Multi-context*
nc_cache_global_hit_rate | Hit rate in non coherent cache for global loads | Multi-context*
nc_gld_efficiency | Ratio of requested non coherent global memory load throughput to required non coherent global memory load throughput expressed as percentage | Multi-context*
nc_gld_requested_throughput | Requested throughput for global memory loaded via non-coherent cache | Multi-context
nc_gld_throughput | Non coherent global memory load throughput | Multi-context*
nc_l2_read_throughput | Memory read throughput for non coherent global read requests seen at L2 cache | Multi-context*
nc_l2_read_transactions | Memory read transactions seen at L2 cache for non coherent global read requests | Multi-context*
shared_efficiency | Ratio of requested shared memory throughput to required shared memory throughput expressed as percentage | Multi-context*
shared_load_throughput | Shared memory load throughput | Multi-context*
shared_load_transactions | Number of shared memory load transactions | Multi-context*
shared_load_transactions_per_request | Average number of shared memory load transactions performed for each shared memory load | Multi-context*
shared_replay_overhead | Average number of replays due to shared memory conflicts for each instruction executed | Multi-context
shared_store_throughput | Shared memory store throughput | Multi-context*
shared_store_transactions | Number of shared memory store transactions | Multi-context*
shared_store_transactions_per_request | Average number of shared memory store transactions performed for each shared memory store | Multi-context*
sm_efficiency | The percentage of time at least one warp is active on a multiprocessor averaged over all multiprocessors on the GPU | Multi-context*
sm_efficiency_instance | The percentage of time at least one warp is active on a specific multiprocessor | Multi-context*
stall_constant_memory_dependency | Percentage of stalls occurring because of immediate constant cache miss. This is available for compute capability 3.2, 3.5 and 3.7. | Multi-context
stall_exec_dependency | Percentage of stalls occurring because an input required by the instruction is not yet available | Multi-context
stall_inst_fetch | Percentage of stalls occurring because the next assembly instruction has not yet been fetched | Multi-context
stall_memory_dependency | Percentage of stalls occurring because a memory operation cannot be performed due to the required resources not being available or fully utilized, or because too many requests of a given type are outstanding. | Multi-context
stall_memory_throttle | Percentage of stalls occurring because of memory throttle. | Multi-context
stall_not_selected | Percentage of stalls occurring because warp was not selected. | Multi-context
stall_other | Percentage of stalls occurring due to miscellaneous reasons | Multi-context
stall_pipe_busy | Percentage of stalls occurring because a compute operation cannot be performed because the compute pipeline is busy. This is available for compute capability 3.2, 3.5 and 3.7. | Multi-context
stall_sync | Percentage of stalls occurring because the warp is blocked at a __syncthreads() call | Multi-context
stall_texture | Percentage of stalls occurring because the texture sub-system is fully utilized or has too many outstanding requests | Multi-context
sysmem_read_throughput | System memory read throughput. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
sysmem_read_transactions | System memory read transactions. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
sysmem_read_utilization | The read utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context
sysmem_utilization | The utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
sysmem_write_throughput | System memory write throughput. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
sysmem_write_transactions | System memory write transactions. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context*
sysmem_write_utilization | The write utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 3.0, 3.5 and 3.7. | Multi-context
tex_cache_hit_rate | Texture cache hit rate | Multi-context*
tex_cache_throughput | Texture cache throughput | Multi-context*
tex_cache_transactions | Texture cache read transactions | Multi-context*
tex_fu_utilization | The utilization level of the multiprocessor function units that execute texture instructions on a scale of 0 to 10 | Multi-context
tex_utilization | The utilization level of the texture cache relative to the peak utilization on a scale of 0 to 10 | Multi-context*
warp_execution_efficiency | Ratio of the average active threads per warp to the maximum number of threads per warp supported on a multiprocessor expressed as percentage | Multi-context
warp_nonpred_execution_efficiency | Ratio of the average active threads per warp executing non-predicated instructions to the maximum number of threads per warp supported on a multiprocessor expressed as percentage | Multi-context

* The "Multi-context" scope for this metric is supported only for devices with compute capability 3.0, 3.5, and 3.7.

##### 2.6.1.2. Metrics for Capability 5.x

Devices with compute capability 5.x implement the metrics shown in the following table. Note that for some metrics, the "Multi-context" scope is supported only for specific devices. Such metrics are marked with "Multi-context*" under the "Scope" column. Refer to the note at the bottom of the table.

Table 2. Capability 5.x Metrics
Metric Name | Description | Scope
--- | --- | ---
achieved_occupancy | Ratio of the average active warps per active cycle to the maximum number of warps supported on a multiprocessor | Multi-context
atomic_transactions | Global memory atomic and reduction transactions | Multi-context
atomic_transactions_per_request | Average number of global memory atomic and reduction transactions performed for each atomic and reduction instruction | Multi-context
branch_efficiency | Ratio of non-divergent branches to total branches expressed as percentage | Multi-context
cf_executed | Number of executed control-flow instructions | Multi-context
cf_fu_utilization | The utilization level of the multiprocessor function units that execute control-flow instructions on a scale of 0 to 10 | Multi-context
cf_issued | Number of issued control-flow instructions | Multi-context
double_precision_fu_utilization | The utilization level of the multiprocessor function units that execute double-precision floating-point instructions on a scale of 0 to 10 | Multi-context
dram_read_bytes | Total bytes read from DRAM to L2 cache. This is available for compute capability 5.0 and 5.2. | Multi-context*
dram_read_throughput | Device memory read throughput. This is available for compute capability 5.0 and 5.2. | Multi-context*
dram_read_transactions | Device memory read transactions. This is available for compute capability 5.0 and 5.2. | Multi-context*
dram_utilization | The utilization level of the device memory relative to the peak utilization on a scale of 0 to 10 | Multi-context*
dram_write_bytes | Total bytes written from L2 cache to DRAM. This is available for compute capability 5.0 and 5.2. | Multi-context*
dram_write_throughput | Device memory write throughput. This is available for compute capability 5.0 and 5.2. | Multi-context*
dram_write_transactions | Device memory write transactions. This is available for compute capability 5.0 and 5.2. | Multi-context*
ecc_throughput | ECC throughput from L2 to DRAM. This is available for compute capability 5.0 and 5.2. | Multi-context*
ecc_transactions | Number of ECC transactions between L2 and DRAM. This is available for compute capability 5.0 and 5.2. | Multi-context*
eligible_warps_per_cycle | Average number of warps that are eligible to issue per active cycle | Multi-context
flop_count_dp | Number of double-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. | Multi-context
flop_count_dp_add | Number of double-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_dp_fma | Number of double-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_dp_mul | Number of double-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_hp | Number of half-precision floating-point operations executed by non-predicated threads (add, multiply and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. This is available for compute capability 5.3. | Multi-context*
flop_count_hp_add | Number of half-precision floating-point add operations executed by non-predicated threads. This is available for compute capability 5.3. | Multi-context*
flop_count_hp_fma | Number of half-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. This is available for compute capability 5.3. | Multi-context*
flop_count_hp_mul | Number of half-precision floating-point multiply operations executed by non-predicated threads. This is available for compute capability 5.3. | Multi-context*
flop_count_sp | Number of single-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. The count does not include special operations. | Multi-context
flop_count_sp_add | Number of single-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_sp_fma | Number of single-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_sp_mul | Number of single-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_sp_special | Number of single-precision floating-point special operations executed by non-predicated threads. | Multi-context
flop_dp_efficiency | Ratio of achieved to peak double-precision floating-point operations | Multi-context
flop_hp_efficiency | Ratio of achieved to peak half-precision floating-point operations. This is available for compute capability 5.3. | Multi-context*
flop_sp_efficiency | Ratio of achieved to peak single-precision floating-point operations | Multi-context
gld_efficiency | Ratio of requested global memory load throughput to required global memory load throughput expressed as percentage. | Multi-context*
gld_requested_throughput | Requested global memory load throughput | Multi-context
gld_throughput | Global memory load throughput | Multi-context*
gld_transactions | Number of global memory load transactions | Multi-context*
gld_transactions_per_request | Average number of global memory load transactions performed for each global memory load. | Multi-context*
global_atomic_requests | Total number of global atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
global_hit_rate | Hit rate for global loads in unified l1/tex cache. Metric value maybe wrong if malloc is used in kernel. | Multi-context*
global_load_requests | Total number of global load requests from Multiprocessor | Multi-context
global_reduction_requests | Total number of global reduction requests from Multiprocessor | Multi-context
global_store_requests | Total number of global store requests from Multiprocessor. This does not include atomic requests. | Multi-context
gst_efficiency | Ratio of requested global memory store throughput to required global memory store throughput expressed as percentage. | Multi-context*
gst_requested_throughput | Requested global memory store throughput | Multi-context
gst_throughput | Global memory store throughput | Multi-context*
gst_transactions | Number of global memory store transactions | Multi-context*
gst_transactions_per_request | Average number of global memory store transactions performed for each global memory store | Multi-context*
half_precision_fu_utilization | The utilization level of the multiprocessor function units that execute 16 bit floating-point instructions and integer instructions on a scale of 0 to 10. This is available for compute capability 5.3. | Multi-context*
inst_bit_convert | Number of bit-conversion instructions executed by non-predicated threads | Multi-context
inst_compute_ld_st | Number of compute load/store instructions executed by non-predicated threads | Multi-context
inst_control | Number of control-flow instructions executed by non-predicated threads (jump, branch, etc.) | Multi-context
inst_executed | The number of instructions executed | Multi-context
inst_executed_global_atomics | Warp level instructions for global atom and atom cas | Multi-context
inst_executed_global_loads | Warp level instructions for global loads | Multi-context
inst_executed_global_reductions | Warp level instructions for global reductions | Multi-context
inst_executed_global_stores | Warp level instructions for global stores | Multi-context
inst_executed_local_loads | Warp level instructions for local loads | Multi-context
inst_executed_local_stores | Warp level instructions for local stores | Multi-context
inst_executed_shared_atomics | Warp level shared instructions for atom and atom CAS | Multi-context
inst_executed_shared_loads | Warp level instructions for shared loads | Multi-context
inst_executed_shared_stores | Warp level instructions for shared stores | Multi-context
inst_executed_surface_atomics | Warp level instructions for surface atom and atom cas | Multi-context
inst_executed_surface_loads | Warp level instructions for surface loads | Multi-context
inst_executed_surface_reductions | Warp level instructions for surface reductions | Multi-context
inst_executed_surface_stores | Warp level instructions for surface stores | Multi-context
inst_executed_tex_ops | Warp level instructions for texture | Multi-context
inst_fp_16 | Number of half-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) This is available for compute capability 5.3. | Multi-context*
inst_fp_32 | Number of single-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_64 | Number of double-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_integer | Number of integer instructions executed by non-predicated threads | Multi-context
inst_inter_thread_communication | Number of inter-thread communication instructions executed by non-predicated threads | Multi-context
inst_issued | The number of instructions issued | Multi-context
inst_misc | Number of miscellaneous instructions executed by non-predicated threads | Multi-context
inst_per_warp | Average number of instructions executed by each warp | Multi-context
inst_replay_overhead | Average number of replays for each instruction executed | Multi-context
ipc | Instructions executed per cycle | Multi-context
issue_slot_utilization | Percentage of issue slots that issued at least one instruction, averaged across all cycles | Multi-context
issue_slots | The number of issue slots used | Multi-context
issued_ipc | Instructions issued per cycle | Multi-context
l2_atomic_throughput | Memory read throughput seen at L2 cache for atomic and reduction requests | Multi-context
l2_atomic_transactions | Memory read transactions seen at L2 cache for atomic and reduction requests | Multi-context*
l2_global_atomic_store_bytes | Bytes written to L2 from Unified cache for global atomics (ATOM and ATOM CAS) | Multi-context*
l2_global_load_bytes | Bytes read from L2 for misses in Unified Cache for global loads | Multi-context*
l2_global_reduction_bytes | Bytes written to L2 from Unified cache for global reductions | Multi-context*
l2_local_global_store_bytes | Bytes written to L2 from Unified Cache for local and global stores. This does not include global atomics. | Multi-context*
l2_local_load_bytes | Bytes read from L2 for misses in Unified Cache for local loads | Multi-context*
l2_read_throughput | Memory read throughput seen at L2 cache for all read requests | Multi-context*
l2_read_transactions | Memory read transactions seen at L2 cache for all read requests | Multi-context*
l2_surface_atomic_store_bytes | Bytes transferred between Unified Cache and L2 for surface atomics (ATOM and ATOM CAS) | Multi-context*
l2_surface_load_bytes | Bytes read from L2 for misses in Unified Cache for surface loads | Multi-context*
l2_surface_reduction_bytes | Bytes written to L2 from Unified Cache for surface reductions | Multi-context*
l2_surface_store_bytes | Bytes written to L2 from Unified Cache for surface stores. This does not include surface atomics. | Multi-context*
l2_tex_hit_rate | Hit rate at L2 cache for all requests from texture cache | Multi-context*
l2_tex_read_hit_rate | Hit rate at L2 cache for all read requests from texture cache. This is available for compute capability 5.0 and 5.2. | Multi-context*
l2_tex_read_throughput | Memory read throughput seen at L2 cache for read requests from the texture cache | Multi-context*
l2_tex_read_transactions | Memory read transactions seen at L2 cache for read requests from the texture cache | Multi-context*
l2_tex_write_hit_rate | Hit Rate at L2 cache for all write requests from texture cache. This is available for compute capability 5.0 and 5.2. | Multi-context*
l2_tex_write_throughput | Memory write throughput seen at L2 cache for write requests from the texture cache | Multi-context*
l2_tex_write_transactions | Memory write transactions seen at L2 cache for write requests from the texture cache | Multi-context*
l2_utilization | The utilization level of the L2 cache relative to the peak utilization on a scale of 0 to 10 | Multi-context*
l2_write_throughput | Memory write throughput seen at L2 cache for all write requests | Multi-context*
l2_write_transactions | Memory write transactions seen at L2 cache for all write requests | Multi-context*
ldst_executed | Number of executed local, global, shared and texture memory load and store instructions | Multi-context
ldst_fu_utilization | The utilization level of the multiprocessor function units that execute shared load, shared store and constant load instructions on a scale of 0 to 10 | Multi-context
ldst_issued | Number of issued local, global, shared and texture memory load and store instructions | Multi-context
local_hit_rate | Hit rate for local loads and stores | Multi-context*
local_load_requests | Total number of local load requests from Multiprocessor | Multi-context*
local_load_throughput | Local memory load throughput | Multi-context*
local_load_transactions | Number of local memory load transactions | Multi-context*
local_load_transactions_per_request | Average number of local memory load transactions performed for each local memory load | Multi-context*
local_memory_overhead | Ratio of local memory traffic to total memory traffic between the L1 and L2 caches expressed as percentage | Multi-context*
local_store_requests | Total number of local store requests from Multiprocessor | Multi-context*
local_store_throughput | Local memory store throughput | Multi-context*
local_store_transactions | Number of local memory store transactions | Multi-context*
local_store_transactions_per_request | Average number of local memory store transactions performed for each local memory store | Multi-context*
pcie_total_data_received | Total data bytes received through PCIe | Device
pcie_total_data_transmitted | Total data bytes transmitted through PCIe | Device
shared_efficiency | Ratio of requested shared memory throughput to required shared memory throughput expressed as percentage | Multi-context*
shared_load_throughput | Shared memory load throughput | Multi-context*
shared_load_transactions | Number of shared memory load transactions | Multi-context*
shared_load_transactions_per_request | Average number of shared memory load transactions performed for each shared memory load | Multi-context*
shared_store_throughput | Shared memory store throughput | Multi-context*
shared_store_transactions | Number of shared memory store transactions | Multi-context*
shared_store_transactions_per_request | Average number of shared memory store transactions performed for each shared memory store | Multi-context*
shared_utilization | The utilization level of the shared memory relative to peak utilization on a scale of 0 to 10 | Multi-context*
single_precision_fu_utilization | The utilization level of the multiprocessor function units that execute single-precision floating-point instructions and integer instructions on a scale of 0 to 10 | Multi-context
sm_efficiency | The percentage of time at least one warp is active on a specific multiprocessor | Multi-context*
special_fu_utilization | The utilization level of the multiprocessor function units that execute sin, cos, ex2, popc, flo, and similar instructions on a scale of 0 to 10 | Multi-context
stall_constant_memory_dependency | Percentage of stalls occurring because of immediate constant cache miss | Multi-context
stall_exec_dependency | Percentage of stalls occurring because an input required by the instruction is not yet available | Multi-context
stall_inst_fetch | Percentage of stalls occurring because the next assembly instruction has not yet been fetched | Multi-context
stall_memory_dependency | Percentage of stalls occurring because a memory operation cannot be performed due to the required resources not being available or fully utilized, or because too many requests of a given type are outstanding | Multi-context
stall_memory_throttle | Percentage of stalls occurring because of memory throttle | Multi-context
stall_not_selected | Percentage of stalls occurring because warp was not selected | Multi-context
stall_other | Percentage of stalls occurring due to miscellaneous reasons | Multi-context
stall_pipe_busy | Percentage of stalls occurring because a compute operation cannot be performed because the compute pipeline is busy | Multi-context
stall_sync | Percentage of stalls occurring because the warp is blocked at a __syncthreads() call | Multi-context
stall_texture | Percentage of stalls occurring because the texture sub-system is fully utilized or has too many outstanding requests | Multi-context
surface_atomic_requests | Total number of surface atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
surface_load_requests | Total number of surface load requests from Multiprocessor | Multi-context
surface_reduction_requests | Total number of surface reduction requests from Multiprocessor | Multi-context
surface_store_requests | Total number of surface store requests from Multiprocessor | Multi-context
sysmem_read_bytes | Number of bytes read from system memory | Multi-context*
sysmem_read_throughput | System memory read throughput | Multi-context*
sysmem_read_transactions | Number of system memory read transactions | Multi-context*
sysmem_read_utilization | The read utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 5.0 and 5.2. | Multi-context
sysmem_utilization | The utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 5.0 and 5.2. | Multi-context*
sysmem_write_bytes | Number of bytes written to system memory | Multi-context*
sysmem_write_throughput | System memory write throughput | Multi-context*
sysmem_write_transactions | Number of system memory write transactions | Multi-context*
sysmem_write_utilization | The write utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 5.0 and 5.2. | Multi-context*
tex_cache_hit_rate | Unified cache hit rate | Multi-context*
tex_cache_throughput | Unified cache throughput | Multi-context*
tex_cache_transactions | Unified cache read transactions | Multi-context*
tex_fu_utilization | The utilization level of the multiprocessor function units that execute global, local and texture memory instructions on a scale of 0 to 10 | Multi-context
tex_utilization | The utilization level of the unified cache relative to the peak utilization on a scale of 0 to 10 | Multi-context*
texture_load_requests | Total number of texture Load requests from Multiprocessor | Multi-context
warp_execution_efficiency | Ratio of the average active threads per warp to the maximum number of threads per warp supported on a multiprocessor | Multi-context
warp_nonpred_execution_efficiency | Ratio of the average active threads per warp executing non-predicated instructions to the maximum number of threads per warp supported on a multiprocessor | Multi-context

* The "Multi-context" scope for this metric is supported only for devices with compute capability 5.0 and 5.2.

##### 2.6.1.3. Metrics for Capability 6.x

Devices with compute capability 6.x implement the metrics shown in the following table.

Table 3. Capability 6.x Metrics
Metric Name | Description | Scope
--- | --- | ---
achieved_occupancy | Ratio of the average active warps per active cycle to the maximum number of warps supported on a multiprocessor | Multi-context
atomic_transactions | Global memory atomic and reduction transactions | Multi-context
atomic_transactions_per_request | Average number of global memory atomic and reduction transactions performed for each atomic and reduction instruction | Multi-context
branch_efficiency | Ratio of non-divergent branches to total branches expressed as percentage | Multi-context
cf_executed | Number of executed control-flow instructions | Multi-context
cf_fu_utilization | The utilization level of the multiprocessor function units that execute control-flow instructions on a scale of 0 to 10 | Multi-context
cf_issued | Number of issued control-flow instructions | Multi-context
double_precision_fu_utilization | The utilization level of the multiprocessor function units that execute double-precision floating-point instructions on a scale of 0 to 10 | Multi-context
dram_read_bytes | Total bytes read from DRAM to L2 cache | Multi-context
dram_read_throughput | Device memory read throughput. This is available for compute capability 6.0 and 6.1. | Multi-context
dram_read_transactions | Device memory read transactions. This is available for compute capability 6.0 and 6.1. | Multi-context
dram_utilization | The utilization level of the device memory relative to the peak utilization on a scale of 0 to 10 | Multi-context
dram_write_bytes | Total bytes written from L2 cache to DRAM | Multi-context
dram_write_throughput | Device memory write throughput. This is available for compute capability 6.0 and 6.1. | Multi-context
dram_write_transactions | Device memory write transactions. This is available for compute capability 6.0 and 6.1. | Multi-context
ecc_throughput | ECC throughput from L2 to DRAM. This is available for compute capability 6.1. | Multi-context
ecc_transactions | Number of ECC transactions between L2 and DRAM. This is available for compute capability 6.1. | Multi-context
eligible_warps_per_cycle | Average number of warps that are eligible to issue per active cycle | Multi-context
flop_count_dp | Number of double-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. | Multi-context
flop_count_dp_add | Number of double-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_dp_fma | Number of double-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_dp_mul | Number of double-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_hp | Number of half-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. | Multi-context
flop_count_hp_add | Number of half-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_hp_fma | Number of half-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_hp_mul | Number of half-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_sp | Number of single-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. The count does not include special operations. | Multi-context
flop_count_sp_add | Number of single-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_sp_fma | Number of single-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_sp_mul | Number of single-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_sp_special | Number of single-precision floating-point special operations executed by non-predicated threads. | Multi-context
flop_dp_efficiency | Ratio of achieved to peak double-precision floating-point operations | Multi-context
flop_hp_efficiency | Ratio of achieved to peak half-precision floating-point operations | Multi-context
flop_sp_efficiency | Ratio of achieved to peak single-precision floating-point operations | Multi-context
gld_efficiency | Ratio of requested global memory load throughput to required global memory load throughput expressed as percentage. | Multi-context
gld_requested_throughput | Requested global memory load throughput | Multi-context
gld_throughput | Global memory load throughput | Multi-context
gld_transactions | Number of global memory load transactions | Multi-context
gld_transactions_per_request | Average number of global memory load transactions performed for each global memory load. | Multi-context
global_atomic_requests | Total number of global atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
global_hit_rate | Hit rate for global loads in unified l1/tex cache. Metric value maybe wrong if malloc is used in kernel. | Multi-context
global_load_requests | Total number of global load requests from Multiprocessor | Multi-context
global_reduction_requests | Total number of global reduction requests from Multiprocessor | Multi-context
global_store_requests | Total number of global store requests from Multiprocessor. This does not include atomic requests. | Multi-context
gst_efficiency | Ratio of requested global memory store throughput to required global memory store throughput expressed as percentage. | Multi-context
gst_requested_throughput | Requested global memory store throughput | Multi-context
gst_throughput | Global memory store throughput | Multi-context
gst_transactions | Number of global memory store transactions | Multi-context
gst_transactions_per_request | Average number of global memory store transactions performed for each global memory store | Multi-context
half_precision_fu_utilization | The utilization level of the multiprocessor function units that execute 16 bit floating-point instructions on a scale of 0 to 10 | Multi-context
inst_bit_convert | Number of bit-conversion instructions executed by non-predicated threads | Multi-context
inst_compute_ld_st | Number of compute load/store instructions executed by non-predicated threads | Multi-context
inst_control | Number of control-flow instructions executed by non-predicated threads (jump, branch, etc.) | Multi-context
inst_executed | The number of instructions executed | Multi-context
inst_executed_global_atomics | Warp level instructions for global atom and atom cas | Multi-context
inst_executed_global_loads | Warp level instructions for global loads | Multi-context
inst_executed_global_reductions | Warp level instructions for global reductions | Multi-context
inst_executed_global_stores | Warp level instructions for global stores | Multi-context
inst_executed_local_loads | Warp level instructions for local loads | Multi-context
inst_executed_local_stores | Warp level instructions for local stores | Multi-context
inst_executed_shared_atomics | Warp level shared instructions for atom and atom CAS | Multi-context
inst_executed_shared_loads | Warp level instructions for shared loads | Multi-context
inst_executed_shared_stores | Warp level instructions for shared stores | Multi-context
inst_executed_surface_atomics | Warp level instructions for surface atom and atom cas | Multi-context
inst_executed_surface_loads | Warp level instructions for surface loads | Multi-context
inst_executed_surface_reductions | Warp level instructions for surface reductions | Multi-context
inst_executed_surface_stores | Warp level instructions for surface stores | Multi-context
inst_executed_tex_ops | Warp level instructions for texture | Multi-context
inst_fp_16 | Number of half-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_32 | Number of single-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_64 | Number of double-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_integer | Number of integer instructions executed by non-predicated threads | Multi-context
inst_inter_thread_communication | Number of inter-thread communication instructions executed by non-predicated threads | Multi-context
inst_issued | The number of instructions issued | Multi-context
inst_misc | Number of miscellaneous instructions executed by non-predicated threads | Multi-context
inst_per_warp | Average number of instructions executed by each warp | Multi-context
inst_replay_overhead | Average number of replays for each instruction executed | Multi-context
ipc | Instructions executed per cycle | Multi-context
issue_slot_utilization | Percentage of issue slots that issued at least one instruction, averaged across all cycles | Multi-context
issue_slots | The number of issue slots used | Multi-context
issued_ipc | Instructions issued per cycle | Multi-context
l2_atomic_throughput | Memory read throughput seen at L2 cache for atomic and reduction requests | Multi-context
l2_atomic_transactions | Memory read transactions seen at L2 cache for atomic and reduction requests | Multi-context
l2_global_atomic_store_bytes | Bytes written to L2 from Unified cache for global atomics (ATOM and ATOM CAS) | Multi-context
l2_global_load_bytes | Bytes read from L2 for misses in Unified Cache for global loads | Multi-context
l2_global_reduction_bytes | Bytes written to L2 from Unified cache for global reductions | Multi-context
l2_local_global_store_bytes | Bytes written to L2 from Unified Cache for local and global stores. This does not include global atomics. | Multi-context
l2_local_load_bytes | Bytes read from L2 for misses in Unified Cache for local loads | Multi-context
l2_read_throughput | Memory read throughput seen at L2 cache for all read requests | Multi-context
l2_read_transactions | Memory read transactions seen at L2 cache for all read requests | Multi-context
l2_surface_atomic_store_bytes | Bytes transferred between Unified Cache and L2 for surface atomics (ATOM and ATOM CAS) | Multi-context
l2_surface_load_bytes | Bytes read from L2 for misses in Unified Cache for surface loads | Multi-context
l2_surface_reduction_bytes | Bytes written to L2 from Unified Cache for surface reductions | Multi-context
l2_surface_store_bytes | Bytes written to L2 from Unified Cache for surface stores. This does not include surface atomics. | Multi-context
l2_tex_hit_rate | Hit rate at L2 cache for all requests from texture cache | Multi-context
l2_tex_read_hit_rate | Hit rate at L2 cache for all read requests from texture cache. This is available for compute capability 6.0 and 6.1. | Multi-context
l2_tex_read_throughput | Memory read throughput seen at L2 cache for read requests from the texture cache | Multi-context
l2_tex_read_transactions | Memory read transactions seen at L2 cache for read requests from the texture cache | Multi-context
l2_tex_write_hit_rate | Hit Rate at L2 cache for all write requests from texture cache. This is available for compute capability 6.0 and 6.1. | Multi-context
l2_tex_write_throughput | Memory write throughput seen at L2 cache for write requests from the texture cache | Multi-context
l2_tex_write_transactions | Memory write transactions seen at L2 cache for write requests from the texture cache | Multi-context
l2_utilization | The utilization level of the L2 cache relative to the peak utilization on a scale of 0 to 10 | Multi-context
l2_write_throughput | Memory write throughput seen at L2 cache for all write requests | Multi-context
l2_write_transactions | Memory write transactions seen at L2 cache for all write requests | Multi-context
ldst_executed | Number of executed local, global, shared and texture memory load and store instructions | Multi-context
ldst_fu_utilization | The utilization level of the multiprocessor function units that execute shared load, shared store and constant load instructions on a scale of 0 to 10 | Multi-context
ldst_issued | Number of issued local, global, shared and texture memory load and store instructions | Multi-context
local_hit_rate | Hit rate for local loads and stores | Multi-context
local_load_requests | Total number of local load requests from Multiprocessor | Multi-context
local_load_throughput | Local memory load throughput | Multi-context
local_load_transactions | Number of local memory load transactions | Multi-context
local_load_transactions_per_request | Average number of local memory load transactions performed for each local memory load | Multi-context
local_memory_overhead | Ratio of local memory traffic to total memory traffic between the L1 and L2 caches expressed as percentage | Multi-context
local_store_requests | Total number of local store requests from Multiprocessor | Multi-context
local_store_throughput | Local memory store throughput | Multi-context
local_store_transactions | Number of local memory store transactions | Multi-context
local_store_transactions_per_request | Average number of local memory store transactions performed for each local memory store | Multi-context
nvlink_overhead_data_received | Ratio of overhead data to the total data, received through NVLink. This is available for compute capability 6.0. | Device
nvlink_overhead_data_transmitted | Ratio of overhead data to the total data, transmitted through NVLink. This is available for compute capability 6.0. | Device
nvlink_receive_throughput | Number of bytes received per second through NVLinks. This is available for compute capability 6.0. | Device
nvlink_total_data_received | Total data bytes received through NVLinks including headers. This is available for compute capability 6.0. | Device
nvlink_total_data_transmitted | Total data bytes transmitted through NVLinks including headers. This is available for compute capability 6.0. | Device
nvlink_total_nratom_data_transmitted | Total non-reduction atomic data bytes transmitted through NVLinks. This is available for compute capability 6.0. | Device
nvlink_total_ratom_data_transmitted | Total reduction atomic data bytes transmitted through NVLinks This is available for compute capability 6.0. | Device
nvlink_total_response_data_received | Total response data bytes received through NVLink, response data includes data for read requests and result of non-reduction atomic requests. This is available for compute capability 6.0. | Device
nvlink_total_write_data_transmitted | Total write data bytes transmitted through NVLinks. This is available for compute capability 6.0. | Device
nvlink_transmit_throughput | Number of Bytes Transmitted per second through NVLinks. This is available for compute capability 6.0. | Device
nvlink_user_data_received | User data bytes received through NVLinks, doesn't include headers. This is available for compute capability 6.0. | Device
nvlink_user_data_transmitted | User data bytes transmitted through NVLinks, doesn't include headers. This is available for compute capability 6.0. | Device
nvlink_user_nratom_data_transmitted | Total non-reduction atomic user data bytes transmitted through NVLinks. This is available for compute capability 6.0. | Device
nvlink_user_ratom_data_transmitted | Total reduction atomic user data bytes transmitted through NVLinks. This is available for compute capability 6.0. | Device
nvlink_user_response_data_received | Total user response data bytes received through NVLink, response data includes data for read requests and result of non-reduction atomic requests. This is available for compute capability 6.0. | Device
nvlink_user_write_data_transmitted | User write data bytes transmitted through NVLinks. This is available for compute capability 6.0. | Device
pcie_total_data_received | Total data bytes received through PCIe | Device
pcie_total_data_transmitted | Total data bytes transmitted through PCIe | Device
shared_efficiency | Ratio of requested shared memory throughput to required shared memory throughput expressed as percentage | Multi-context
shared_load_throughput | Shared memory load throughput | Multi-context
shared_load_transactions | Number of shared memory load transactions | Multi-context
shared_load_transactions_per_request | Average number of shared memory load transactions performed for each shared memory load | Multi-context
shared_store_throughput | Shared memory store throughput | Multi-context
shared_store_transactions | Number of shared memory store transactions | Multi-context
shared_store_transactions_per_request | Average number of shared memory store transactions performed for each shared memory store | Multi-context
shared_utilization | The utilization level of the shared memory relative to peak utilization on a scale of 0 to 10 | Multi-context
single_precision_fu_utilization | The utilization level of the multiprocessor function units that execute single-precision floating-point instructions and integer instructions on a scale of 0 to 10 | Multi-context
sm_efficiency | The percentage of time at least one warp is active on a specific multiprocessor | Multi-context
special_fu_utilization | The utilization level of the multiprocessor function units that execute sin, cos, ex2, popc, flo, and similar instructions on a scale of 0 to 10 | Multi-context
stall_constant_memory_dependency | Percentage of stalls occurring because of immediate constant cache miss | Multi-context
stall_exec_dependency | Percentage of stalls occurring because an input required by the instruction is not yet available | Multi-context
stall_inst_fetch | Percentage of stalls occurring because the next assembly instruction has not yet been fetched | Multi-context
stall_memory_dependency | Percentage of stalls occurring because a memory operation cannot be performed due to the required resources not being available or fully utilized, or because too many requests of a given type are outstanding | Multi-context
stall_memory_throttle | Percentage of stalls occurring because of memory throttle | Multi-context
stall_not_selected | Percentage of stalls occurring because warp was not selected | Multi-context
stall_other | Percentage of stalls occurring due to miscellaneous reasons | Multi-context
stall_pipe_busy | Percentage of stalls occurring because a compute operation cannot be performed because the compute pipeline is busy | Multi-context
stall_sync | Percentage of stalls occurring because the warp is blocked at a __syncthreads() call | Multi-context
stall_texture | Percentage of stalls occurring because the texture sub-system is fully utilized or has too many outstanding requests | Multi-context
surface_atomic_requests | Total number of surface atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
surface_load_requests | Total number of surface load requests from Multiprocessor | Multi-context
surface_reduction_requests | Total number of surface reduction requests from Multiprocessor | Multi-context
surface_store_requests | Total number of surface store requests from Multiprocessor | Multi-context
sysmem_read_bytes | Number of bytes read from system memory | Multi-context
sysmem_read_throughput | System memory read throughput | Multi-context
sysmem_read_transactions | Number of system memory read transactions | Multi-context
sysmem_read_utilization | The read utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 6.0 and 6.1. | Multi-context
sysmem_utilization | The utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 6.0 and 6.1. | Multi-context
sysmem_write_bytes | Number of bytes written to system memory | Multi-context
sysmem_write_throughput | System memory write throughput | Multi-context
sysmem_write_transactions | Number of system memory write transactions | Multi-context
sysmem_write_utilization | The write utilization level of the system memory relative to the peak utilization on a scale of 0 to 10. This is available for compute capability 6.0 and 6.1. | Multi-context
tex_cache_hit_rate | Unified cache hit rate | Multi-context
tex_cache_throughput | Unified cache throughput | Multi-context
tex_cache_transactions | Unified cache read transactions | Multi-context
tex_fu_utilization | The utilization level of the multiprocessor function units that execute global, local and texture memory instructions on a scale of 0 to 10 | Multi-context
tex_utilization | The utilization level of the unified cache relative to the peak utilization on a scale of 0 to 10 | Multi-context
texture_load_requests | Total number of texture Load requests from Multiprocessor | Multi-context
unique_warps_launched | Number of warps launched. Value is unaffected by compute preemption. | Multi-context
warp_execution_efficiency | Ratio of the average active threads per warp to the maximum number of threads per warp supported on a multiprocessor | Multi-context
warp_nonpred_execution_efficiency | Ratio of the average active threads per warp executing non-predicated instructions to the maximum number of threads per warp supported on a multiprocessor | Multi-context

##### 2.6.1.4. Metrics for Capability 7.0

Devices with compute capability 7.0 implement the metrics shown in the following table.

Table 4. Capability 7.x (7.0 and 7.2) Metrics
Metric Name | Description | Scope
--- | --- | ---
achieved_occupancy | Ratio of the average active warps per active cycle to the maximum number of warps supported on a multiprocessor | Multi-context
atomic_transactions | Global memory atomic and reduction transactions | Multi-context
atomic_transactions_per_request | Average number of global memory atomic and reduction transactions performed for each atomic and reduction instruction | Multi-context
branch_efficiency | Ratio of branch instruction to sum of branch and divergent branch instruction | Multi-context
cf_executed | Number of executed control-flow instructions | Multi-context
cf_fu_utilization | The utilization level of the multiprocessor function units that execute control-flow instructions on a scale of 0 to 10 | Multi-context
cf_issued | Number of issued control-flow instructions | Multi-context
double_precision_fu_utilization | The utilization level of the multiprocessor function units that execute double-precision floating-point instructions on a scale of 0 to 10 | Multi-context
dram_read_bytes | Total bytes read from DRAM to L2 cache | Multi-context
dram_read_throughput | Device memory read throughput | Multi-context
dram_read_transactions | Device memory read transactions | Multi-context
dram_utilization | The utilization level of the device memory relative to the peak utilization on a scale of 0 to 10 | Multi-context
dram_write_bytes | Total bytes written from L2 cache to DRAM | Multi-context
dram_write_throughput | Device memory write throughput | Multi-context
dram_write_transactions | Device memory write transactions | Multi-context
eligible_warps_per_cycle | Average number of warps that are eligible to issue per active cycle | Multi-context
flop_count_dp | Number of double-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. | Multi-context
flop_count_dp_add | Number of double-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_dp_fma | Number of double-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_dp_mul | Number of double-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_hp | Number of half-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate contributes 2 or 4 to the count based on the number of inputs. | Multi-context
flop_count_hp_add | Number of half-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_hp_fma | Number of half-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate contributes 2 or 4 to the count based on the number of inputs. | Multi-context
flop_count_hp_mul | Number of half-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_sp | Number of single-precision floating-point operations executed by non-predicated threads (add, multiply, and multiply-accumulate). Each multiply-accumulate operation contributes 2 to the count. The count does not include special operations. | Multi-context
flop_count_sp_add | Number of single-precision floating-point add operations executed by non-predicated threads. | Multi-context
flop_count_sp_fma | Number of single-precision floating-point multiply-accumulate operations executed by non-predicated threads. Each multiply-accumulate operation contributes 1 to the count. | Multi-context
flop_count_sp_mul | Number of single-precision floating-point multiply operations executed by non-predicated threads. | Multi-context
flop_count_sp_special | Number of single-precision floating-point special operations executed by non-predicated threads. | Multi-context
flop_dp_efficiency | Ratio of achieved to peak double-precision floating-point operations | Multi-context
flop_hp_efficiency | Ratio of achieved to peak half-precision floating-point operations | Multi-context
flop_sp_efficiency | Ratio of achieved to peak single-precision floating-point operations | Multi-context
gld_efficiency | Ratio of requested global memory load throughput to required global memory load throughput expressed as percentage. | Multi-context
gld_requested_throughput | Requested global memory load throughput | Multi-context
gld_throughput | Global memory load throughput | Multi-context
gld_transactions | Number of global memory load transactions | Multi-context
gld_transactions_per_request | Average number of global memory load transactions performed for each global memory load. | Multi-context
global_atomic_requests | Total number of global atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
global_hit_rate | Hit rate for global load and store in unified l1/tex cache | Multi-context
global_load_requests | Total number of global load requests from Multiprocessor | Multi-context
global_reduction_requests | Total number of global reduction requests from Multiprocessor | Multi-context
global_store_requests | Total number of global store requests from Multiprocessor. This does not include atomic requests. | Multi-context
gst_efficiency | Ratio of requested global memory store throughput to required global memory store throughput expressed as percentage. | Multi-context
gst_requested_throughput | Requested global memory store throughput | Multi-context
gst_throughput | Global memory store throughput | Multi-context
gst_transactions | Number of global memory store transactions | Multi-context
gst_transactions_per_request | Average number of global memory store transactions performed for each global memory store | Multi-context
half_precision_fu_utilization | The utilization level of the multiprocessor function units that execute 16 bit floating-point instructions on a scale of 0 to 10. Note that this doesn't specify the utilization level of tensor core unit | Multi-context
inst_bit_convert | Number of bit-conversion instructions executed by non-predicated threads | Multi-context
inst_compute_ld_st | Number of compute load/store instructions executed by non-predicated threads | Multi-context
inst_control | Number of control-flow instructions executed by non-predicated threads (jump, branch, etc.) | Multi-context
inst_executed | The number of instructions executed | Multi-context
inst_executed_global_atomics | Warp level instructions for global atom and atom cas | Multi-context
inst_executed_global_loads | Warp level instructions for global loads | Multi-context
inst_executed_global_reductions | Warp level instructions for global reductions | Multi-context
inst_executed_global_stores | Warp level instructions for global stores | Multi-context
inst_executed_local_loads | Warp level instructions for local loads | Multi-context
inst_executed_local_stores | Warp level instructions for local stores | Multi-context
inst_executed_shared_atomics | Warp level shared instructions for atom and atom CAS | Multi-context
inst_executed_shared_loads | Warp level instructions for shared loads | Multi-context
inst_executed_shared_stores | Warp level instructions for shared stores | Multi-context
inst_executed_surface_atomics | Warp level instructions for surface atom and atom cas | Multi-context
inst_executed_surface_loads | Warp level instructions for surface loads | Multi-context
inst_executed_surface_reductions | Warp level instructions for surface reductions | Multi-context
inst_executed_surface_stores | Warp level instructions for surface stores | Multi-context
inst_executed_tex_ops | Warp level instructions for texture | Multi-context
inst_fp_16 | Number of half-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_32 | Number of single-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_fp_64 | Number of double-precision floating-point instructions executed by non-predicated threads (arithmetic, compare, etc.) | Multi-context
inst_integer | Number of integer instructions executed by non-predicated threads | Multi-context
inst_inter_thread_communication | Number of inter-thread communication instructions executed by non-predicated threads | Multi-context
inst_issued | The number of instructions issued | Multi-context
inst_misc | Number of miscellaneous instructions executed by non-predicated threads | Multi-context
inst_per_warp | Average number of instructions executed by each warp | Multi-context
inst_replay_overhead | Average number of replays for each instruction executed | Multi-context
ipc | Instructions executed per cycle | Multi-context
issue_slot_utilization | Percentage of issue slots that issued at least one instruction, averaged across all cycles | Multi-context
issue_slots | The number of issue slots used | Multi-context
issued_ipc | Instructions issued per cycle | Multi-context
l2_atomic_throughput | Memory read throughput seen at L2 cache for atomic and reduction requests | Multi-context
l2_atomic_transactions | Memory read transactions seen at L2 cache for atomic and reduction requests | Multi-context
l2_global_atomic_store_bytes | Bytes written to L2 from L1 for global atomics (ATOM and ATOM CAS) | Multi-context
l2_global_load_bytes | Bytes read from L2 for misses in L1 for global loads | Multi-context
l2_local_global_store_bytes | Bytes written to L2 from L1 for local and global stores. This does not include global atomics. | Multi-context
l2_local_load_bytes | Bytes read from L2 for misses in L1 for local loads | Multi-context
l2_read_throughput | Memory read throughput seen at L2 cache for all read requests | Multi-context
l2_read_transactions | Memory read transactions seen at L2 cache for all read requests | Multi-context
l2_surface_load_bytes | Bytes read from L2 for misses in L1 for surface loads | Multi-context
l2_surface_store_bytes | Bytes read from L2 for misses in L1 for surface stores | Multi-context
l2_tex_hit_rate | Hit rate at L2 cache for all requests from texture cache | Multi-context
l2_tex_read_hit_rate | Hit rate at L2 cache for all read requests from texture cache | Multi-context
l2_tex_read_throughput | Memory read throughput seen at L2 cache for read requests from the texture cache | Multi-context
l2_tex_read_transactions | Memory read transactions seen at L2 cache for read requests from the texture cache | Multi-context
l2_tex_write_hit_rate | Hit Rate at L2 cache for all write requests from texture cache | Multi-context
l2_tex_write_throughput | Memory write throughput seen at L2 cache for write requests from the texture cache | Multi-context
l2_tex_write_transactions | Memory write transactions seen at L2 cache for write requests from the texture cache | Multi-context
l2_utilization | The utilization level of the L2 cache relative to the peak utilization on a scale of 0 to 10 | Multi-context
l2_write_throughput | Memory write throughput seen at L2 cache for all write requests | Multi-context
l2_write_transactions | Memory write transactions seen at L2 cache for all write requests | Multi-context
ldst_executed | Number of executed local, global, shared and texture memory load and store instructions | Multi-context
ldst_fu_utilization | The utilization level of the multiprocessor function units that execute shared load, shared store and constant load instructions on a scale of 0 to 10 | Multi-context
ldst_issued | Number of issued local, global, shared and texture memory load and store instructions | Multi-context
local_hit_rate | Hit rate for local loads and stores | Multi-context
local_load_requests | Total number of local load requests from Multiprocessor | Multi-context
local_load_throughput | Local memory load throughput | Multi-context
local_load_transactions | Number of local memory load transactions | Multi-context
local_load_transactions_per_request | Average number of local memory load transactions performed for each local memory load | Multi-context
local_memory_overhead | Ratio of local memory traffic to total memory traffic between the L1 and L2 caches expressed as percentage | Multi-context
local_store_requests | Total number of local store requests from Multiprocessor | Multi-context
local_store_throughput | Local memory store throughput | Multi-context
local_store_transactions | Number of local memory store transactions | Multi-context
local_store_transactions_per_request | Average number of local memory store transactions performed for each local memory store | Multi-context
nvlink_overhead_data_received | Ratio of overhead data to the total data, received through NVLink. | Device
nvlink_overhead_data_transmitted | Ratio of overhead data to the total data, transmitted through NVLink. | Device
nvlink_receive_throughput | Number of bytes received per second through NVLinks. | Device
nvlink_total_data_received | Total data bytes received through NVLinks including headers. | Device
nvlink_total_data_transmitted | Total data bytes transmitted through NVLinks including headers. | Device
nvlink_total_nratom_data_transmitted | Total non-reduction atomic data bytes transmitted through NVLinks. | Device
nvlink_total_ratom_data_transmitted | Total reduction atomic data bytes transmitted through NVLinks. | Device
nvlink_total_response_data_received | Total response data bytes received through NVLink, response data includes data for read requests and result of non-reduction atomic requests. | Device
nvlink_total_write_data_transmitted | Total write data bytes transmitted through NVLinks. | Device
nvlink_transmit_throughput | Number of Bytes Transmitted per second through NVLinks. | Device
nvlink_user_data_received | User data bytes received through NVLinks, doesn't include headers. | Device
nvlink_user_data_transmitted | User data bytes transmitted through NVLinks, doesn't include headers. | Device
nvlink_user_nratom_data_transmitted | Total non-reduction atomic user data bytes transmitted through NVLinks. | Device
nvlink_user_ratom_data_transmitted | Total reduction atomic user data bytes transmitted through NVLinks. | Device
nvlink_user_response_data_received | Total user response data bytes received through NVLink, response data includes data for read requests and result of non-reduction atomic requests. | Device
nvlink_user_write_data_transmitted | User write data bytes transmitted through NVLinks. | Device
pcie_total_data_received | Total data bytes received through PCIe | Device
pcie_total_data_transmitted | Total data bytes transmitted through PCIe | Device
shared_efficiency | Ratio of requested shared memory throughput to required shared memory throughput expressed as percentage | Multi-context
shared_load_throughput | Shared memory load throughput | Multi-context
shared_load_transactions | Number of shared memory load transactions | Multi-context
shared_load_transactions_per_request | Average number of shared memory load transactions performed for each shared memory load | Multi-context
shared_store_throughput | Shared memory store throughput | Multi-context
shared_store_transactions | Number of shared memory store transactions | Multi-context
shared_store_transactions_per_request | Average number of shared memory store transactions performed for each shared memory store | Multi-context
shared_utilization | The utilization level of the shared memory relative to peak utilization on a scale of 0 to 10 | Multi-context
single_precision_fu_utilization | The utilization level of the multiprocessor function units that execute single-precision floating-point instructions on a scale of 0 to 10 | Multi-context
sm_efficiency | The percentage of time at least one warp is active on a specific multiprocessor | Multi-context
special_fu_utilization | The utilization level of the multiprocessor function units that execute sin, cos, ex2, popc, flo, and similar instructions on a scale of 0 to 10 | Multi-context
stall_constant_memory_dependency | Percentage of stalls occurring because of immediate constant cache miss | Multi-context
stall_exec_dependency | Percentage of stalls occurring because an input required by the instruction is not yet available | Multi-context
stall_inst_fetch | Percentage of stalls occurring because the next assembly instruction has not yet been fetched | Multi-context
stall_memory_dependency | Percentage of stalls occurring because a memory operation cannot be performed due to the required resources not being available or fully utilized, or because too many requests of a given type are outstanding | Multi-context
stall_memory_throttle | Percentage of stalls occurring because of memory throttle | Multi-context
stall_not_selected | Percentage of stalls occurring because warp was not selected | Multi-context
stall_other | Percentage of stalls occurring due to miscellaneous reasons | Multi-context
stall_pipe_busy | Percentage of stalls occurring because a compute operation cannot be performed because the compute pipeline is busy | Multi-context
stall_sleeping | Percentage of stalls occurring because warp was sleeping | Multi-context
stall_sync | Percentage of stalls occurring because the warp is blocked at a __syncthreads() call | Multi-context
stall_texture | Percentage of stalls occurring because the texture sub-system is fully utilized or has too many outstanding requests | Multi-context
surface_atomic_requests | Total number of surface atomic(Atom and Atom CAS) requests from Multiprocessor | Multi-context
surface_load_requests | Total number of surface load requests from Multiprocessor | Multi-context
surface_reduction_requests | Total number of surface reduction requests from Multiprocessor | Multi-context
surface_store_requests | Total number of surface store requests from Multiprocessor | Multi-context
sysmem_read_bytes | Number of bytes read from system memory | Multi-context
sysmem_read_throughput | System memory read throughput | Multi-context
sysmem_read_transactions | Number of system memory read transactions | Multi-context
sysmem_read_utilization | The read utilization level of the system memory relative to the peak utilization on a scale of 0 to 10 | Multi-context
sysmem_utilization | The utilization level of the system memory relative to the peak utilization on a scale of 0 to 10 | Multi-context
sysmem_write_bytes | Number of bytes written to system memory | Multi-context
sysmem_write_throughput | System memory write throughput | Multi-context
sysmem_write_transactions | Number of system memory write transactions | Multi-context
sysmem_write_utilization | The write utilization level of the system memory relative to the peak utilization on a scale of 0 to 10 | Multi-context
tensor_precision_fu_utilization | The utilization level of the multiprocessor function units that execute tensor core instructions on a scale of 0 to 10 | Multi-context
tensor_int_fu_utilization | The utilization level of the multiprocessor function units that execute tensor core int8 instructions on a scale of 0 to 10. This metric is only available for device with compute capability 7.2. | Multi-context
tex_cache_hit_rate | Unified cache hit rate | Multi-context
tex_cache_throughput | Unified cache to Multiprocessor read throughput | Multi-context
tex_cache_transactions | Unified cache to Multiprocessor read transactions | Multi-context
tex_fu_utilization | The utilization level of the multiprocessor function units that execute global, local and texture memory instructions on a scale of 0 to 10 | Multi-context
tex_utilization | The utilization level of the unified cache relative to the peak utilization on a scale of 0 to 10 | Multi-context
texture_load_requests | Total number of texture Load requests from Multiprocessor | Multi-context
warp_execution_efficiency | Ratio of the average active threads per warp to the maximum number of threads per warp supported on a multiprocessor | Multi-context
warp_nonpred_execution_efficiency | Ratio of the average active threads per warp executing non-predicated instructions to the maximum number of threads per warp supported on a multiprocessor | Multi-context

### 2.7. CUPTI Profiling API

Starting with CUDA 10.0, a new set of metric APIs are added for devices with compute capability 7.0 and higher. These APIs provide low and deterministic profiling overhead on the target system. These are supported on all CUDA supported platforms except Android, and are not supported under MPS (Multi-Process Service), Confidential Compute, or SLI configured systems. In order to determine whether a device is compatible with this API, a new function `cuptiProfilerDeviceSupported` is introduced in CUDA 11.5 which exposes overall Profiling API support and specific requirements for a given device. Profiling API must be initialized by calling `cuptiProfilerInitialize` before testing device support.

This section covers performance profiling Host and Target APIs for CUDA. Broadly profiling APIs are divided into following four sections:

- Enumeration (Host)
- Configuration (Host)
- Collection (Target)
- Evaluation (Host)

Host APIs provide a metric interface for enumeration, configuration and evaluation that doesn't require a compute(GPU) device, and can also run in an offline mode. In the samples section under extensions, profiler host utility covers the usage of host APIs. Target APIs are used for data collection of the metrics and requires a compute (GPU) device. Refer to samples auto_rangeProfiling and userrange_profiling for usage of profiling APIs.

The list of metrics has been overhauled from earlier generation metrics and event APIs, to support a standard naming convention based upon `unit__(subunit?)_(pipestage?)_quantity_qualifiers`

#### 2.7.1. Multi Pass Collection

NVIDIA GPU hardware has a limited number of counter registers and cannot collect all possible counters concurrently. There are also limitations on which counters can be collected together in a single pass. This is resolved by replaying the exact same set of GPU workloads multiple times, where each replay is termed a pass. On each pass, a different subset of requested counters are collected. Once all passes are collected, the data is available for evaluation. Certain metrics have many counters as inputs; adding a single metric may require many passes to collect. CUPTI APIs support multi pass collection through different collection attributes.

Sample cupti_metric_properties shows how to query number of passes required to collect a set of counters.

#### 2.7.2. Range Profiling

Each profiling session runs a series of replay passes, where each pass contains a sequence of ranges. Every metric enabled in the session's configuration is collected separately per unique range-stack in the pass. CUPTI supports auto and user defined ranges.

##### 2.7.2.1. Auto Range

In a session with auto range mode, ranges are defined around each kernel automatically with a unique name assigned to each range, while profiling is enabled. This mode is useful for tight metric collection around each kernel. A user can choose one of the supported replay modes, pseudo code for each is described below:

##### Kernel Replay

The replay logic (multiple pass, if needed) is done by CUPTI implicitly (opaque to the user), and usage of CUPTI replay API's `cuptiProfilerBeginPass` and `cuptiProfilerEndPass` will be a no-op in this mode. This mode is useful for collecting metrics around a kernel in tight control. Each kernel launch is synchronized to segregate its metrics into a separate range, and a CPU-GPU sync is made to ensure the profiled data is collected from GPU. Counter Collection can be enabled and disabled with `cuptiProfilerEnableProfiling` and `cuptiProfilerDisableProfiling`. Refer to the sample autorange_profiling

    /* Assume Inputs(counterDataImagePrefix and configImage) from configuration phase at host */
    void Collection(std::vector<uint8_t>& counterDataImagePrefix, std::vector<uint8_t>& configImage)
    {
    	CUpti_Profiler_Initialize_Params profilerInitializeParams = { CUpti_Profiler_Initialize_Params_STRUCT_SIZE };
    	cuptiProfilerInitialize(&profilerInitializeParams);

    	std::vector<uint8_t> counterDataImages;
    	std::vector<uint8_t> counterDataScratchBuffer;
    	CreateCounterDataImage(counterDataImages, counterDataScratchBuffer, counterDataImagePrefix);

    	CUpti_Profiler_BeginSession_Params beginSessionParams = { CUpti_Profiler_BeginSession_Params_STRUCT_SIZE };
    	CUpti_ProfilerRange profilerRange = CUPTI_AutoRange;
    	CUpti_ProfilerReplayMode profilerReplayMode = CUPTI_KernelReplay;

    	beginSessionParams.ctx = NULL;
    	beginSessionParams.counterDataImageSize = counterDataImage.size();
    	beginSessionParams.pCounterDataImage = &counterDataImage[0];
    	beginSessionParams.counterDataScratchBufferSize = counterDataScratchBuffer.size();
    	beginSessionParams.pCounterDataScratchBuffer = &counterDataScratchBuffer[0];
    	beginSessionParams.range = profilerRange;
    	beginSessionParams.replayMode = profilerReplayMode;
    	beginSessionParams.maxRangesPerPass = num_ranges;
    	beginSessionParams.maxLaunchesPerPass = num_ranges;

    	cuptiProfilerBeginSession(&beginSessionParams));

    	CUpti_Profiler_SetConfig_Params setConfigParams = { CUpti_Profiler_SetConfig_Params_STRUCT_SIZE };
    	setConfigParams.pConfig = &configImage[0];
    	setConfigParams.configSize = configImage.size();

    	cuptiProfilerSetConfig(&setConfigParams));

    	kernelA <<<grid, tids >>>(...);                  // KernelA not profiled

    	CUpti_Profiler_EnableProfiling_Params enableProfilingParams = { CUpti_Profiler_EnableProfiling_Params_STRUCT_SIZE };
    	cuptiProfilerEnableProfiling(&enableProfilingParams);
    	{

    		kernelB <<<grid, tids >>>(...);              // KernelB profiled and captured in an unique range.
    		kernelC <<<grid, tids >>>(...);              // KernelC profiled and captured in an unique range.
    		kernelD <<<grid, tids >>>(...);              // KernelD profiled and captured in an unique range.
    	}

    	CUpti_Profiler_DisableProfiling_Params disableProfilingParams = { CUpti_Profiler_DisableProfiling_Params_STRUCT_SIZE };
    	cuptiProfilerDisableProfiling(&disableProfilingParams);

    	kernelE <<<grid, tids >>>(...);                  // KernelE not profiled

    	CUpti_Profiler_UnsetConfig_Params unsetConfigParams = { CUpti_Profiler_UnsetConfig_Params_STRUCT_SIZE };
    	cuptiProfilerUnsetConfig(&unsetConfigParams);

    	CUpti_Profiler_EndSession_Params endSessionParams = { CUpti_Profiler_EndSession_Params_STRUCT_SIZE };
    	cuptiProfilerEndSession(&endSessionParams);
    }

##### User Replay

The replay (multiple passes, if needed) is done by the user using the replay API's `cuptiProfilerBeginPass` and `cuptiProfilerEndPass`. It is user responsibility to flush the counter data `cuptiProfilerFlushCounterData` before ending the session to ensure collection of metric data in CPU. Counter collection can be enabled and disabled with `cuptiProfilerEnableProfiling`/ `cuptiProfilerDisableProfiling`. Refer to the sample autorange_profiling

        /* Assume Inputs(counterDataImagePrefix and configImage) from configuration phase at host */

        void Collection(std::vector<uint8_t>& counterDataImagePrefix, std::vector<uint8_t>& configImage)
        {
            CUpti_Profiler_Initialize_Params profilerInitializeParams = {CUpti_Profiler_Initialize_Params_STRUCT_SIZE};
            cuptiProfilerInitialize(&profilerInitializeParams);

            std::vector<uint8_t> counterDataImages;
            std::vector<uint8_t> counterDataScratchBuffer;
            CreateCounterDataImage(counterDataImages, counterDataScratchBuffer, counterDataImagePrefix);

            CUpti_Profiler_BeginSession_Params beginSessionParams = {CUpti_Profiler_BeginSession_Params_STRUCT_SIZE};
            CUpti_ProfilerRange profilerRange = CUPTI_AutoRange;
            CUpti_ProfilerReplayMode profilerReplayMode = CUPTI_UserReplay;

            beginSessionParams.ctx = NULL;
            beginSessionParams.counterDataImageSize = counterDataImage.size();
            beginSessionParams.pCounterDataImage = &counterDataImage[0];
            beginSessionParams.counterDataScratchBufferSize = counterDataScratchBuffer.size();
            beginSessionParams.pCounterDataScratchBuffer = &counterDataScratchBuffer[0];
            beginSessionParams.range = profilerRange;
            beginSessionParams.replayMode = profilerReplayMode;
            beginSessionParams.maxRangesPerPass = num_ranges;
            beginSessionParams.maxLaunchesPerPass = num_ranges;

            cuptiProfilerBeginSession(&beginSessionParams));

            CUpti_Profiler_SetConfig_Params setConfigParams = {CUpti_Profiler_SetConfig_Params_STRUCT_SIZE};
            setConfigParams.pConfig = &configImage[0];
            setConfigParams.configSize = configImage.size();

            cuptiProfilerSetConfig(&setConfigParams));

            CUpti_Profiler_FlushCounterData_Params cuptiFlushCounterDataParams =        {CUpti_Profiler_FlushCounterData_Params_STRUCT_SIZE};

            CUpti_Profiler_EnableProfiling_Params enableProfilingParams =       {CUpti_Profiler_EnableProfiling_Params_STRUCT_SIZE};

            CUpti_Profiler_DisableProfiling_Params disableProfilingParams =         {CUpti_Profiler_DisableProfiling_Params_STRUCT_SIZE};

            kernelA<<<grid, tids>>>(...);                  // KernelA neither profiled, nor replayed

            CUpti_Profiler_BeginPass_Params beginPassParams = {CUpti_Profiler_BeginPass_Params_STRUCT_SIZE};
            CUpti_Profiler_EndPass_Params endPassParams = {CUpti_Profiler_EndPass_Params_STRUCT_SIZE};

            cuptiProfilerBeginPass(&beginPassParams);
            {
                kernelB<<<grid, tids>>>(...);              // KernelB replayed but not profiled

                cuptiProfilerEnableProfiling(&enableProfilingParams);

                kernelC<<<grid, tids>>>(...);              // KernelC profiled and captured in an unique range.
                kernelD<<<grid, tids>>>(...);              // KernelD profiled and captured in an unique range.

                cuptiProfilerDisableProfiling(&disableProfilingParams);
            }
            cuptiProfilerEndPass(&endPassParams);

            cuptiProfilerFlushCounterData(&cuptiFlushCounterDataParams);

            kernelE<<<grid, tids>>>(...);                  // KernelE not profiled

            CUpti_Profiler_UnsetConfig_Params unsetConfigParams = {CUpti_Profiler_UnsetConfig_Params_STRUCT_SIZE};
            cuptiProfilerUnsetConfig(&unsetConfigParams);

            CUpti_Profiler_EndSession_Params endSessionParams = {CUpti_Profiler_EndSession_Params_STRUCT_SIZE};
            cuptiProfilerEndSession(&endSessionParams);
        }

##### Application Replay

This replay mode is same as user replay, instead of in process replay, you can replay the whole process again. You will need to update the pass index while setting the config `cuptiProfilerSetConfig` and reload the intermediate counterDataImage on each pass.

##### 2.7.2.2. User Range

In a session with user range mode, ranges are defined by you, `cuptiProfilerPushRange` and `cuptiProfilerPopRange`. Kernel launches are concurrent within a range. This mode is useful for metric data collection around a specific section of code, instead of per-kernel metric collection. Kernel replay is not supported in user range mode. You own the responsibility of replay using `cuptiProfilerBeginPass` and `cuptiProfilerEndPass`.

##### User Replay

The replay (multiple passes, if needed) is done by the user using the replay API's `cuptiProfilerBeginPass` and `cuptiProfilerEndPass`. It is your responsibility to flush the counter data using `cuptiProfilerFlushCounterData` before ending the session. Counter collection can be enabled/disabled with `cuptiProfilerEnableProfiling` and `cuptiProfilerDisableProfiling`. Refer to the sample userrange_profiling

    >
        /* Assume Inputs(counterDataImagePrefix and configImage) from configuration phase at host */

        void Collection(std::vector<uint8_t>& counterDataImagePrefix, std::vector<uint8_t>& configImage)
        {
            CUpti_Profiler_Initialize_Params profilerInitializeParams = {CUpti_Profiler_Initialize_Params_STRUCT_SIZE};
            cuptiProfilerInitialize(&profilerInitializeParams);

            std::vector<uint8_t> counterDataImages;
            std::vector<uint8_t> counterDataScratchBuffer;
            CreateCounterDataImage(counterDataImages, counterDataScratchBuffer, counterDataImagePrefix);

            CUpti_Profiler_BeginSession_Params beginSessionParams = {CUpti_Profiler_BeginSession_Params_STRUCT_SIZE};
            CUpti_ProfilerRange profilerRange = CUPTI_UserRange;
            CUpti_ProfilerReplayMode profilerReplayMode = CUPTI_UserReplay;

            beginSessionParams.ctx = NULL;
            beginSessionParams.counterDataImageSize = counterDataImage.size();
            beginSessionParams.pCounterDataImage = &counterDataImage[0];
            beginSessionParams.counterDataScratchBufferSize = counterDataScratchBuffer.size();
            beginSessionParams.pCounterDataScratchBuffer = &counterDataScratchBuffer[0];
            beginSessionParams.range = profilerRange;
            beginSessionParams.replayMode = profilerReplayMode;
            beginSessionParams.maxRangesPerPass = num_ranges;
            beginSessionParams.maxLaunchesPerPass = num_ranges;

            cuptiProfilerBeginSession(&beginSessionParams));

            CUpti_Profiler_SetConfig_Params setConfigParams = {CUpti_Profiler_SetConfig_Params_STRUCT_SIZE};
            setConfigParams.pConfig = &configImage[0];
            setConfigParams.configSize = configImage.size();

            cuptiProfilerSetConfig(&setConfigParams));

            CUpti_Profiler_FlushCounterData_Params cuptiFlushCounterDataParams = {CUpti_Profiler_FlushCounterData_Params_STRUCT_SIZE};

            kernelA<<<grid, tids>>>(...);                  // KernelA neither profiled, nor replayed

            CUpti_Profiler_BeginPass_Params beginPassParams = {CUpti_Profiler_BeginPass_Params_STRUCT_SIZE};
            CUpti_Profiler_EndPass_Params endPassParams = {CUpti_Profiler_EndPass_Params_STRUCT_SIZE};

            cuptiProfilerBeginPass(&beginPassParams);
            {
                kernelB<<<grid, tids>>>(...);              // KernelB replayed but not profiled

                CUpti_Profiler_PushRange_Params enableProfilingParams = {CUpti_Profiler_PushRange_Params_STRUCT_SIZE};
                pushRangeParams.pRangeName = "RangeA";
                cuptiProfilerPushRange(&pushRangeParams);

                kernelC<<<grid, tids>>>(...);
                kernelD<<<grid, tids>>>(...);

                cuptiProfilerPopRange(&popRangeParams);     // Kernel C and Kernel D are captured in rangeA without any serialization introduced by profiler
            }
            cuptiProfilerEndPass(&endPassParams);
            cuptiProfilerFlushCounterData(&cuptiFlushCounterDataParams);

            kernelE<<<grid, tids>>>(...);                  // KernelE not Profiled

            CUpti_Profiler_UnsetConfig_Params unsetConfigParams = {CUpti_Profiler_UnsetConfig_Params_STRUCT_SIZE};
            cuptiProfilerUnsetConfig(&unsetConfigParams);

            CUpti_Profiler_EndSession_Params endSessionParams = {CUpti_Profiler_EndSession_Params_STRUCT_SIZE};
            cuptiProfilerEndSession(&endSessionParams);
        }

##### Application Replay

This replay mode is same as user replay, instead of in process replay, you can replay the whole process again. You will need to update the pass index while setting the config using the `cuptiProfilerSetConfig` API, and reload the intermediate counterDataImage on each pass.

#### 2.7.3. CUPTI Profiler Definitions

Definitions of glossary used in this section.

Counter:
  The number of occurrences of a specific event on the device.
Configuration Image:
  A Blob to configure the session for counters to be collected.
CounterData Image:
  A Blob which contains the values of collected counters
CounterData Prefix:
  A metadata header for CounterData Image
Device:
  A physical NVIDIA GPU.
Event:
  An event is a countable activity, action, or occurrence on device.
Metric:
  A high-level value derived from counter values.
Pass:
  A repeatable set of operations, with consistently labeled ranges.
Range:
  A labeled region of execution
Replay:
  Performing the repeatable set of operation.
Session:
  A profiling session where GPU resources needed for profiling are allocated. The profiler is in armed state at session boundaries, and power management may be disabled at session boundaries. Outside of a session, the GPU will return to its normal operating state.

#### 2.7.4. Differences from event and metric APIs

Here is the list of features which are supported by the event and metric APIs but these are not available with the Profiling API:

- Continuous mode or sampling of the metrics.
- Profiling API provides closest equivalent metrics for most of the events and metrics supported by the event and metric APIs. However, there are some events and metrics, for example NVLink performance metrics, for which there is no equivalent metrics in the Profiling API. Tables Metrics Mapping Table and Events Mapping Table can be referred to find the equivalent Perfworks metrics for compute capability 7.0.
- Per-instance metrics i.e. users can't collect metrics for each instance of the hardware units like SM, FB etc separately. However Profiling API provides sub-metrics which can be used to get the avg/sum/min/max across all instances of a hardware unit.

### 2.8. Perfworks Metric API

### Introduction:

The Perfworks Metric API supports the enumeration, configuration and evaluation of metrics. The binary outputs of the configuration phase are inputs to the CUPTI Range Profiling API. The output of Range Profiling is the CounterData, which is passed to the Derived Metrics Evaluation APIs.

GPU Metrics are generally presented as counts, ratios and percentages. The underlying values collected from hardware are raw counters (analogous to CUPTI events), but those details are hidden behind derived metric formulas.

The Metric APIs are split into two layers: Derived Metrics and Raw Metrics. Derived Metrics contains the list of named metrics and performs evaluation to numeric results, serving a similar purpose as the previous CUPTI Metric API. Most user interaction will be with derived metrics. Raw Metrics contains the list of raw counters and generates configuration file images analogous to the previous CUPTI Event API.

### Metric Enumeration

Metric Enumeration is the process of listing available counters and metrics.

Refer to file `List.cpp` used by the cupti_metric_properties sample.

Metrics are grouped into three types i.e. counters, ratios and throughput. Except ratios metric type each metrics have four type of sub-metrics also known as rollup metrics i.e. sum, avg, min, max.

For enumerating supported metrics for a chip, we need to calculate the scratch buffer needed for host operation and to initialize the Metric Evaluator.

- Call `NVPW_CUDA_MetricsEvaluator_CalculateScratchBufferSize` for calculating scratch buffer size required for allocating memory for host operations.
- Call `NVPW_CUDA_MetricsEvaluator_Initialize` for initializing the Metrics Evaluator which creates a NVPW_MetricsEvaluator object.

The outline for enumerating supported counter metrics for a chip:

- Call `NVPW_MetricsEvaluator_GetMetricNames` for NVPW_METRIC_TYPE_COUNTER metric type for listing all the counter metrics supported.
- Call `NVPW_MetricsEvaluator_GetSupportedSubmetrics` to list all the sub-metric supported for NVPW_METRIC_TYPE_COUNTER metric type.
- Call `NVPW_MetricsEvaluator_GetCounterProperties` to give description of the counter and the collection hardware unit.

Similarly, for enumerating ratio and throughput metrics we need to pass NVPW_METRIC_TYPE_RATIO and NVPW_METRIC_TYPE_THROUGHPUT as metric types to `NVPW_MetricsEvaluator_GetMetricNames` and `NVPW_MetricsEvaluator_GetSupportedSubmetrics`.

For more details about the metric properties call `NVPW_MetricsEvaluator_GetRatioMetricProperties` and `NVPW_MetricsEvaluator_GetThroughputMetricProperties` respectively.

### Configuration Workflow

Configuration is the process of specifying the metrics that will be collected and how those metrics should be collected. The inputs for this phase are the metric names and metric collection properties. The output for this phase is a ConfigImage and a CounterDataPrefix Image.

Refer to file `Metric.cpp` used by the userrange_profiling sample.

The outline for configuring metrics:

- As input, take a list of metric names.
- Before creating ConfigImage or CounterDataPrefixImage, we need a list of NVPA_RawMetricRequest for the metrics listed for collection.
  - We need to calculate the scratch buffer size required for the host operation and to initialize the Metric Evaluator like in the Enumeration phase.
  - For each metric, Call `NVPW_MetricsEvaluator_ConvertMetricNameToMetricEvalRequest` for creating a NVPW_MetricEvalRequest.
  - Call `NVPW_MetricsEvaluator_GetMetricRawDependencies` which takes the NVPW_MetricsEvaluator and NVPW_MetricEvalRequest as input, for getting raw dependencies for given metrics.
- Create an `NVPA_RawMetricRequest` with `keepInstances=true` and `isolated=true`
- Pass the `NVPA_RawMetricRequest` to `NVPW_RawMetricsConfig_AddMetrics` for the ConfigImage.
- Pass the `NVPA_RawMetricRequest` to `NVPW_CounterDataBuilder_AddMetrics` for the CounterDataPrefix.
- Generate binary configuration "images" (file format in memory):
  - ConfigImage from `NVPW_RawMetricsConfig_GetConfigImage`
  - CounterDataPrefix from `NVPW_CounterDataBuilder_GetCounterDataPrefix`

### Metric Evaluation

Metric Evaluation is the process of forming metrics from the counters stored in the CounterData image.

Refer to file `Eval.cpp` used by the userrange_profiling sample.

The outline for configuring metrics:

- As input, take the same list of metric names as used during configuration.
- As input, take a CounterDataImage collected on a target device.
- We need to calculate the scratch buffer size required for the host operation and to initialize the Metric Evaluator like in the Enumeration phase.
- Query the number of ranges collected via `NVPW_CounterData_GetNumRanges`.
- For each metric:
  - Call `NVPW_MetricsEvaluator_ConvertMetricNameToMetricEvalRequest` for creating NVPW_MetricEvalRequest
  - For each range:
    - Call `NVPW_Profiler_CounterData_GetRangeDescriptions` to retrieve the range's description, originally set by `cuptiProfilerPushRange`.
    - Call `NVPW_MetricsEvaluator_SetDeviceAttributes` to set the current range for evaluation on the NVPW_MetricEvalRequest.
    - Call `NVPW_MetricsEvaluator_EvaluateToGpuValues` to query an array of numeric values corresponding to each input metric.

#### 2.8.1. Derived metrics

#### Metrics Overview

The PerfWorks API comes with an advanced metrics calculation system, designed to help you determine what happened (counters and metrics), and how close the program reached to peak GPU performance (throughputs as a percentage). Every counter has associated peak rates in the database, to allow computing its throughput as a percentage.

Throughput metrics return the maximum percentage value of their constituent counters. Constituents can be programmatically queried via `NVPW_MetricsEvaluator_GetMetricNames` with NVPW_METRIC_TYPE_THROUGHPUT as metric types. These constituents have been carefully selected to represent the sections of the GPU pipeline that govern peak performance. While all counters can be converted to a %-of-peak, not all counters are suitable for peak-performance analysis; examples of unsuitable counters include qualified subsets of activity, and workload residency counters. Using throughput metrics ensures meaningful and actionable analysis.

Two types of peak rates are available for every counter: burst and sustained. Burst rate is the maximum rate reportable in a single clock cycle. Sustained rate is the maximum rate achievable over an infinitely long measurement period, for "typical" operations. For many counters, burst == sustained. Since the burst rate cannot be exceeded, percentages of burst rate will always be less than 100%. Percentages of sustained rate can occasionally exceed 100% in edge cases. Burst metrics are only supported with MetricsContext APIs and these will be deprecated in a future CUDA release. These metrics are not supported with NVPW_MetricsEvaluator APIs.

#### Metrics Entities

The Metrics layer has 3 major types of entities:

- Metrics : these are calculated quantities, with the following static properties:
  - Description string.
  - Dimensional Units : a list of ('name', exponent) in the style of dimensional analysis. Example string representation: `pixels / gpc_clk`.
  - Raw Metric dependencies : the list of raw metrics that must be collected, in order to evaluate the metric.
  - Every metric has the following sub-metrics built in.

    `.peak_sustained` | the peak sustained rate
    `.peak_sustained_active` | the peak sustained rate during unit active cycles
    `.peak_sustained_active.per_second` | the peak sustained rate during unit active cycles, per second *
    `.peak_sustained_elapsed` | the peak sustained rate during unit elapsed cycles
    `.peak_sustained_elapsed.per_second` | the peak sustained rate during unit elapsed cycles, per second *
    `.peak_sustained_region` | the peak sustained rate over a user-specified "range"
    `.peak_sustained_region.per_second` | the peak sustained rate over a user-specified "range", per second *
    `.peak_sustained_frame` | the peak sustained rate over a user-specified "frame"
    `.peak_sustained_frame.per_second` | the peak sustained rate over a user-specified "frame", per second *
    `.per_cycle_active` | the number of operations per unit active cycle
    `.per_cycle_elapsed` | the number of operations per unit elapsed cycle
    `.per_cycle_in_region` | the number of operations per user-specified "range" cycle
    `.per_cycle_in_frame` | the number of operations per user-specified "frame" cycle
    `.per_second` | the number of operations per second
    `.pct_of_peak_sustained_active` | % of peak sustained rate achieved during unit active cycles
    `.pct_of_peak_sustained_elapsed` | % of peak sustained rate achieved during unit elapsed cycles
    `.pct_of_peak_sustained_region` | % of peak sustained rate achieved over a user-specified "range" time
    `.pct_of_peak_sustained_frame` | % of peak sustained rate achieved over a user-specified "frame" time

    * sub-metrics added in CUPTI 11.3.
- Counters may be either a raw counter from the GPU, or a calculated counter value. Every counter has four sub-metrics under it, which are also called roll-ups:

  `.sum` | The sum of counter values across all unit instances.
  `.avg` | The average counter value across all unit instances.
  `.min` | The minimum counter value across all unit instances.
  `.max` | The maximum counter value across all unit instances.

- Ratios have three sub-metrics under it:

  `.pct` | The value expressed as a percentage.
  `.ratio` | The value expressed as a ratio.
  `.max_rate` | The ratio's maximum value.

- Throughputs indicate how close a portion of the GPU reached to peak rate. Every throughput has the following sub-metrics:

  `.pct_of_peak_sustained_active` | % of peak sustained rate achieved during unit active cycles
  `.pct_of_peak_sustained_elapsed` | % of peak sustained rate achieved during unit elapsed cycles
  `.pct_of_peak_sustained_region` | % of peak sustained rate achieved over a user-specified "range" time
  `.pct_of_peak_sustained_frame` | % of peak sustained rate achieved over a user-specified "frame" time

At the configuration step, you must specify metric names. Counters, ratios, and throughputs are not directly schedulable.

Note: Burst metrics are only supported with MetricsContext APIs.

From CUPTI 11.3 onwards, due to not being useful for performance optimization following counter sub-metrics are not present in MetricEvaluator APIs and are only supported with MetricsContext APIs:

`.peak_burst` | the peak burst rate
`.pct_of_peak_burst_active` | % of peak burst rate achieved during unit active cycles
`.pct_of_peak_burst_elapsed` | % of peak burst rate achieved during unit elapsed cycles
`.pct_of_peak_burst_region` | % of peak burst rate achieved over a user-specified "range"
`.pct_of_peak_burst_frame` | % of peak burst rate achieved over a user-specified "frame"

From CUPTI 11.3 onwards, due to not being useful for performance optimization following throughput sub-metrics are not present in MetricEvaluator APIs and are only supported with MetricsContext APIs:

`.pct_of_peak_burst_active` | % of peak burst rate achieved during unit active cycles
`.pct_of_peak_burst_elapsed` | % of peak burst rate achieved during unit elapsed cycles
`.pct_of_peak_burst_region` | % of peak burst rate achieved over a user-specified "range" time
`.pct_of_peak_burst_frame` | % of peak burst rate achieved over a user-specified "frame" time

#### Metrics Examples

    ## non-metric names -- *not* directly evaluable
    sm__inst_executed                   # counter
    smsp__average_warp_latency          # ratio
    sm__throughput                      # throughput

    ## a counter's four roll-ups as sub-metrics -- all evaluable
    sm__inst_executed.sum               # metric
    sm__inst_executed.avg               # metric
    sm__inst_executed.min               # metric
    sm__inst_executed.max               # metric

    ## all names below are metrics -- all evaluable
    l1tex__data_bank_conflicts_pipe_lsu.sum
    l1tex__data_bank_conflicts_pipe_lsu.sum.peak_burst
    l1tex__data_bank_conflicts_pipe_lsu.sum.peak_sustained
    l1tex__data_bank_conflicts_pipe_lsu.sum.per_cycle_active
    l1tex__data_bank_conflicts_pipe_lsu.sum.per_cycle_elapsed
    l1tex__data_bank_conflicts_pipe_lsu.sum.per_cycle_in_region
    l1tex__data_bank_conflicts_pipe_lsu.sum.per_cycle_in_frame
    l1tex__data_bank_conflicts_pipe_lsu.sum.per_second
    l1tex__data_bank_conflicts_pipe_lsu.sum.pct_of_peak_sustained_active
    l1tex__data_bank_conflicts_pipe_lsu.sum.pct_of_peak_sustained_elapsed
    l1tex__data_bank_conflicts_pipe_lsu.sum.pct_of_peak_sustained_region
    l1tex__data_bank_conflicts_pipe_lsu.sum.pct_of_peak_sustained_frame

#### Metrics Naming Conventions

Counters and metrics _generally_ obey the naming scheme:

- Unit-Level Counter : `unit__(subunit?)_(pipestage?)_quantity_(qualifiers?)`
- Interface Counter : `unit__(subunit?)_(pipestage?)_(interface)_quantity_(qualifiers?)`
- Unit Metric : `(counter_name).(rollup_metric)`
- Sub-Metric : `(counter_name).(rollup_metric).(submetric)`

where

- unit: A logical of physical unit of the GPU
- subunit: The subunit within the unit where the counter was measured. Sometimes this is a pipeline mode instead.
- pipestage: The pipeline stage within the subunit where the counter was measured.
- quantity: What is being measured. Generally matches the "dimensional units".
- qualifiers: Any additional predicates or filters applied to the counter. Often, an unqualified counter can be broken down into several qualified sub-components.
- interface: Of the form `sender2receiver`, where `sender` is the source-unit and `receiver` is the destination-unit.
- rollup_metric: One of sum,avg,min,max.
- submetric: refer to section Metric Entities

Components are not always present. Most top-level counters have no qualifiers. Subunit and pipestage may be absent where irrelevant, or there may be many subunit specifiers for detailed counters.

#### Cycle Metrics

Counters using the term `cycles` in the name report the number of cycles in the unit's clock domain. Unit-level cycle metrics include:

- `unit__cycles_elapsed` : The number of cycles within a range. The cycles' DimUnits are specific to the unit's clock domain.
- `unit__cycles_active` : The number of cycles where the unit was processing data.
- `unit__cycles_stalled` : The number of cycles where the unit was unable to process new data because its output interface was blocked.
- `unit__cycles_idle` : The number of cycles where the unit was idle.

Interface-level cycle counters are often (not always) available in the following variations:

- `unit__(interface)_active` : Cycles where data was transferred from source-unit to destination-unit.
- `unit__(interface)_stalled` : Cycles where the source-unit had data, but the destination-unit was unable to accept data.

#### 2.8.2. Raw Metrics

The raw metrics layer contains a list of low-level GPU counters, and the "scheduling" logic needed to program the hardware. The binary output files (ConfigImage and CounterDataPrefix) can be generated offline, stored on disk, and used on any compatible GPU. They do not need to be generated on a machine where a GPU is available.

Refer to Metrics Configuration to see where Raw Metrics fit into the overall data flow of the profiler.

#### 2.8.3. Metrics Mapping Table

The table below lists the CUPTI metrics for devices with compute capability 7.0. For each CUPTI metric the closest equivalent Perfworks metric or formula is given. If no equivalent Perfworks metric is available the column is left blank. Note that there can be some difference in the metric values between the CUPTI metric and the Perfworks metrics.

Table 5. Metrics Mapping Table from CUPTI to Perfworks for Compute Capability 7.0
CUPTI Metric | Perfworks Metric or Formula
--- | ---
achieved_occupancy | sm__warps_active.avg.pct_of_peak_sustained_active
atomic_transactions | l1tex__t_set_accesses_pipe_lsu_mem_global_op_atom.sum + l1tex__t_set_accesses_pipe_lsu_mem_global_op_red.sum
atomic_transactions_per_request | (l1tex__t_sectors_pipe_lsu_mem_global_op_atom.sum + l1tex__t_sectors_pipe_lsu_mem_global_op_red.sum) / (l1tex__t_requests_pipe_lsu_mem_global_op_atom.sum + l1tex__t_requests_pipe_lsu_mem_global_op_red.sum)
branch_efficiency | smsp__sass_average_branch_targets_threads_uniform.pct
cf_executed | smsp__inst_executed_pipe_cbu.sum + smsp__inst_executed_pipe_adu.sum
cf_fu_utilization |
cf_issued |
double_precision_fu_utilization | smsp__inst_executed_pipe_fp64.avg.pct_of_peak_sustained_active
dram_read_bytes | dram__bytes_read.sum
dram_read_throughput | dram__bytes_read.sum.per_second
dram_read_transactions | dram__sectors_read.sum
dram_utilization | dram__throughput.avg.pct_of_peak_sustained_elapsed
dram_write_bytes | dram__bytes_write.sum
dram_write_throughput | dram__bytes_write.sum.per_second
dram_write_transactions | dram__sectors_write.sum
eligible_warps_per_cycle | smsp__warps_eligible.sum.per_cycle_active
flop_count_dp | smsp__sass_thread_inst_executed_op_dadd_pred_on.sum + smsp__sass_thread_inst_executed_op_dmul_pred_on.sum + smsp__sass_thread_inst_executed_op_dfma_pred_on.sum * 2
flop_count_dp_add | smsp__sass_thread_inst_executed_op_dadd_pred_on.sum
flop_count_dp_fma | smsp__sass_thread_inst_executed_op_dfma_pred_on.sum
flop_count_dp_mul | smsp__sass_thread_inst_executed_op_dmul_pred_on.sum
flop_count_hp | smsp__sass_thread_inst_executed_op_hadd_pred_on.sum + smsp__sass_thread_inst_executed_op_hmul_pred_on.sum + smsp__sass_thread_inst_executed_op_hfma_pred_on.sum * 2
flop_count_hp_add | smsp__sass_thread_inst_executed_op_hadd_pred_on.sum
flop_count_hp_fma | smsp__sass_thread_inst_executed_op_hfma_pred_on.sum
flop_count_hp_mul | smsp__sass_thread_inst_executed_op_hmul_pred_on.sum
flop_count_sp | smsp__sass_thread_inst_executed_op_fadd_pred_on.sum + smsp__sass_thread_inst_executed_op_fmul_pred_on.sum + smsp__sass_thread_inst_executed_op_ffma_pred_on.sum * 2
flop_count_sp_add | smsp__sass_thread_inst_executed_op_fadd_pred_on.sum
flop_count_sp_fma | smsp__sass_thread_inst_executed_op_ffma_pred_on.sum
flop_count_sp_mul | smsp__sass_thread_inst_executed_op_fmul_pred_on.sum
flop_count_sp_special |
flop_dp_efficiency | smsp__sass_thread_inst_executed_ops_dadd_dmul_dfma_pred_on.avg.pct_of_peak_sustained_elapsed
flop_hp_efficiency | smsp__sass_thread_inst_executed_ops_hadd_hmul_hfma_pred_on.avg.pct_of_peak_sustained_elapsed
flop_sp_efficiency | smsp__sass_thread_inst_executed_ops_fadd_fmul_ffma_pred_on.avg.pct_of_peak_sustained_elapsed
gld_efficiency | smsp__sass_average_data_bytes_per_sector_mem_global_op_ld.pct
gld_requested_throughput |
gld_throughput | l1tex__t_bytes_pipe_lsu_mem_global_op_ld.sum.per_second
gld_transactions | l1tex__t_sectors_pipe_lsu_mem_global_op_ld.sum
gld_transactions_per_request | l1tex__average_t_sectors_per_request_pipe_lsu_mem_global_op_ld.ratio
global_atomic_requests | l1tex__t_requests_pipe_lsu_mem_global_op_atom.sum
global_hit_rate | l1tex__t_sectors_pipe_lsu_mem_global_op_{op}_lookup_hit.sum / l1tex__t_sectors_pipe_lsu_mem_global_op_{op}.sum
global_load_requests | l1tex__t_requests_pipe_lsu_mem_global_op_ld.sum
global_reduction_requests | l1tex__t_requests_pipe_lsu_mem_global_op_red.sum
global_store_requests | l1tex__t_requests_pipe_lsu_mem_global_op_st.sum
gst_efficiency | smsp__sass_average_data_bytes_per_sector_mem_global_op_st.pct
gst_requested_throughput |
gst_throughput | l1tex__t_bytes_pipe_lsu_mem_global_op_st.sum.per_second
gst_transactions | l1tex__t_bytes_pipe_lsu_mem_global_op_st.sum
gst_transactions_per_request | l1tex__average_t_sectors_per_request_pipe_lsu_mem_global_op_st.ratio
half_precision_fu_utilization | smsp__inst_executed_pipe_fp16.avg.pct_of_peak_sustained_active
inst_bit_convert | smsp__sass_thread_inst_executed_op_conversion_pred_on.sum
inst_compute_ld_st | smsp__sass_thread_inst_executed_op_memory_pred_on.sum
inst_control | smsp__sass_thread_inst_executed_op_control_pred_on.sum
inst_executed | smsp__inst_executed.sum
inst_executed_global_atomics | smsp__sass_inst_executed_op_global_atom.sum
inst_executed_global_loads | smsp__inst_executed_op_global_ld.sum
inst_executed_global_reductions | smsp__inst_executed_op_global_red.sum
inst_executed_global_stores | smsp__inst_executed_op_global_st.sum
inst_executed_local_loads | smsp__inst_executed_op_local_ld.sum
inst_executed_local_stores | smsp__inst_executed_op_local_st.sum
inst_executed_shared_atomics | smsp__inst_executed_op_shared_atom.sum + smsp__inst_executed_op_shared_atom_dot_alu.sum + smsp__inst_executed_op_shared_atom_dot_cas.sum
inst_executed_shared_loads | smsp__inst_executed_op_shared_ld.sum
inst_executed_shared_stores | smsp__inst_executed_op_shared_st.sum
inst_executed_surface_atomics | smsp__inst_executed_op_surface_atom.sum
inst_executed_surface_loads | smsp__inst_executed_op_surface_ld.sum + smsp__inst_executed_op_shared_atom_dot_alu.sum + smsp__inst_executed_op_shared_atom_dot_cas.sum
inst_executed_surface_reductions | smsp__inst_executed_op_surface_red.sum
inst_executed_surface_stores | smsp__inst_executed_op_surface_st.sum
inst_executed_tex_ops | smsp__inst_executed_op_texture.sum
inst_fp_16 | smsp__sass_thread_inst_executed_op_fp16_pred_on.sum
inst_fp_32 | smsp__sass_thread_inst_executed_op_fp32_pred_on.sum
inst_fp_64 | smsp__sass_thread_inst_executed_op_fp64_pred_on.sum
inst_integer | smsp__sass_thread_inst_executed_op_integer_pred_on.sum
inst_inter_thread_communication | smsp__sass_thread_inst_executed_op_inter_thread_communication_pred_on.sum
inst_issued | smsp__inst_issued.sum
inst_misc | smsp__sass_thread_inst_executed_op_misc_pred_on.sum
inst_per_warp | smsp__average_inst_executed_per_warp.ratio
inst_replay_overhead |
ipc | smsp__inst_executed.avg.per_cycle_active
issue_slot_utilization | smsp__issue_active.avg.pct_of_peak_sustained_active
issue_slots | smsp__inst_issued.sum
issued_ipc | smsp__inst_issued.avg.per_cycle_active
l1_sm_lg_utilization | l1tex__lsu_writeback_active.avg.pct_of_peak_sustained_active
l2_atomic_throughput | lts__t_sectors_srcunit_l1_op_atom.sum.per_second
l2_atomic_transactions | lts__t_sectors_srcunit_l1_op_atom.sum
l2_global_atomic_store_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_lsu_mem_global_op_atom.sum
l2_global_load_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_lsu_mem_global_op_ld.sum
l2_local_global_store_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_lsu_mem_local_op_st.sum + lts__t_bytes_equiv_l1sectormiss_pipe_lsu_mem_global_op_st.sum
l2_local_load_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_lsu_mem_local_op_ld.sum
l2_read_throughput | lts__t_sectors_op_read.sum.per_second
l2_read_transactions | lts__t_sectors_op_read.sum
l2_surface_load_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_tex_mem_surface_op_ld.sum
l2_surface_store_bytes | lts__t_bytes_equiv_l1sectormiss_pipe_tex_mem_surface_op_st.sum
l2_tex_hit_rate | lts__t_sector_hit_rate.pct
l2_tex_read_hit_rate | lts__t_sector_op_read_hit_rate.pct
l2_tex_read_throughput | lts__t_sectors_srcunit_tex_op_read.sum.per_second
l2_tex_read_transactions | lts__t_sectors_srcunit_tex_op_read.sum
l2_tex_write_hit_rate | lts__t_sector_op_write_hit_rate.pct
l2_tex_write_throughput | lts__t_sectors_srcunit_tex_op_read.sum.per_second
l2_tex_write_transactions | lts__t_sectors_srcunit_tex_op_read.sum
l2_utilization | lts__t_sectors.avg.pct_of_peak_sustained_elapsed
l2_write_throughput | lts__t_sectors_op_write.sum.per_second
l2_write_transactions | lts__t_sectors_op_write.sum
ldst_executed |
ldst_fu_utilization | smsp__inst_executed_pipe_lsu.avg.pct_of_peak_sustained_active
ldst_issued |
local_hit_rate |
local_load_requests | l1tex__t_requests_pipe_lsu_mem_local_op_ld.sum
local_load_throughput | l1tex__t_bytes_pipe_lsu_mem_local_op_ld.sum.per_second
local_load_transactions | l1tex__t_sectors_pipe_lsu_mem_local_op_ld.sum
local_load_transactions_per_request | l1tex__average_t_sectors_per_request_pipe_lsu_mem_local_op_ld.ratio
local_memory_overhead |
local_store_requests | l1tex__t_requests_pipe_lsu_mem_local_op_st.sum
local_store_throughput | l1tex__t_sectors_pipe_lsu_mem_local_op_st.sum.per_second
local_store_transactions | l1tex__t_sectors_pipe_lsu_mem_local_op_st.sum
local_store_transactions_per_request | l1tex__average_t_sectors_per_request_pipe_lsu_mem_local_op_st.ratio
nvlink_data_receive_efficiency |
nvlink_data_transmission_efficiency |
nvlink_overhead_data_received |
nvlink_overhead_data_transmitted |
nvlink_receive_throughput |
nvlink_total_data_received |
nvlink_total_data_transmitted |
nvlink_total_nratom_data_transmitted |
nvlink_total_ratom_data_transmitted |
nvlink_total_response_data_received |
nvlink_total_write_data_transmitted |
nvlink_transmit_throughput |
nvlink_user_data_received |
nvlink_user_data_transmitted |
nvlink_user_nratom_data_transmitted |
nvlink_user_ratom_data_transmitted |
nvlink_user_response_data_received |
nvlink_user_write_data_transmitted |
pcie_total_data_received | pcie__read_bytes.sum
pcie_total_data_transmitted | pcie__write_bytes.sum
shared_efficiency | smsp__sass_average_data_bytes_per_wavefront_mem_shared.pct
shared_load_throughput | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_ld.sum.per_second
shared_load_transactions | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_ld.sum
shared_load_transactions_per_request |
shared_store_throughput | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_st.sum.per_second
shared_store_transactions | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_st.sum
shared_store_transactions_per_request |
shared_utilization | l1tex__data_pipe_lsu_wavefronts_mem_shared.avg.pct_of_peak_sustained_elapsed
single_precision_fu_utilization | smsp__pipe_fma_cycles_active.avg.pct_of_peak_sustained_active
sm_efficiency | smsp__cycles_active.avg.pct_of_peak_sustained_elapsed
sm_tex_utilization | l1tex__texin_sm2tex_req_cycles_active.avg.pct_of_peak_sustained_elapsed
special_fu_utilization | smsp__inst_executed_pipe_xu.avg.pct_of_peak_sustained_active
stall_constant_memory_dependency | smsp__warp_issue_stalled_imc_miss_per_warp_active.pct
stall_exec_dependency | smsp__warp_issue_stalled_short_scoreboard_per_warp_active.pct + smsp__warp_issue_stalled_wait_per_warp_active.pct
stall_inst_fetch | smsp__warp_issue_stalled_no_instruction_per_warp_active.pct
stall_memory_dependency | smsp__warp_issue_stalled_long_scoreboard_per_warp_active.pct
stall_memory_throttle | smsp__warp_issue_stalled_drain_per_warp_active.pct + smsp__warp_issue_stalled_lg_throttle_per_warp_active.pct
stall_not_selected | smsp__warp_issue_stalled_not_selected_per_warp_active.pct
stall_other | smsp__warp_issue_stalled_misc_per_warp_active.pct + smsp__warp_issue_stalled_dispatch_stall_per_warp_active.pct
stall_pipe_busy | smsp__warp_issue_stalled_mio_throttle_per_warp_active.pct + smsp__warp_issue_stalled_math_pipe_throttle_per_warp_active.pct
stall_sleeping | smsp__warp_issue_stalled_sleeping_per_warp_active.pct
stall_sync | smsp__warp_issue_stalled_membar_per_warp_active.pct + smsp__warp_issue_stalled_barrier_per_warp_active.pct
stall_texture | smsp__warp_issue_stalled_tex_throttle_per_warp_active.pct
surface_atomic_requests | l1tex__t_requests_pipe_tex_mem_surface_op_atom.sum
surface_load_requests | l1tex__t_requests_pipe_tex_mem_surface_op_ld.sum
surface_reduction_requests | l1tex__t_requests_pipe_tex_mem_surface_op_red.sum
surface_store_requests | l1tex__t_requests_pipe_tex_mem_surface_op_st.sum
sysmem_read_bytes | lts__t_sectors_aperture_sysmem_op_read* 32
sysmem_read_throughput | lts__t_sectors_aperture_sysmem_op_read.sum.per_second
sysmem_read_transactions | lts__t_sectors_aperture_sysmem_op_read.sum
sysmem_read_utilization |
sysmem_utilization |
sysmem_write_bytes | lts__t_sectors_aperture_sysmem_op_write * 32
sysmem_write_throughput | lts__t_sectors_aperture_sysmem_op_write.sum.per_second
sysmem_write_transactions | lts__t_sectors_aperture_sysmem_op_write.sum
sysmem_write_utilization |
tensor_precision_fu_utilization | sm__pipe_tensor_cycles_active.avg.pct_of_peak_sustained_active
tex_cache_hit_rate | l1tex__t_sector_hit_rate.pct
tex_cache_throughput |
tex_cache_transactions | l1tex__lsu_writeback_active.avg.pct_of_peak_sustained_active + l1tex__tex_writeback_active.avg.pct_of_peak_sustained_active
tex_fu_utilization | smsp__inst_executed_pipe_tex.avg.pct_of_peak_sustained_active
tex_sm_tex_utilization | l1tex__f_tex2sm_cycles_active.avg.pct_of_peak_sustained_elapsed
tex_sm_utilization | sm__mio2rf_writeback_active.avg.pct_of_peak_sustained_elapsed
tex_utilization |
texture_load_requests | l1tex__t_requests_pipe_tex_mem_texture.sum
warp_execution_efficiency | smsp__thread_inst_executed_per_inst_executed.ratio
warp_nonpred_execution_efficiency | smsp__thread_inst_executed_per_inst_executed.pct

#### 2.8.4. Events Mapping Table

The table below lists the CUPTI events for devices with compute capability 7.0. For each CUPTI event the closest equivalent Perfworks metric or formula is given. If no equivalent Perfworks metric is available the column is left blank. Note that there can be some difference in the values between the CUPTI event and the Perfworks metrics.

Table 6. Events Mapping Table from CUPTI events to Perfworks metrics for Compute Capability 7.0
CUPTI Event | Perfworks Metric or Formula
--- | ---
active_cycles | sm__cycles_active.sum
active_cycles_pm | sm__cycles_active.sum
active_cycles_sys | sys__cycles_active.sum
active_warps | sm__warps_active.sum
active_warps_pm | sm__warps_active.sum
atom_count | smsp__inst_executed_op_generic_atom_dot_alu.sum
elapsed_cycles_pm | sm__cycles_elapsed.sum
elapsed_cycles_sm | sm__cycles_elapsed.sum
elapsed_cycles_sys | sys__cycles_elapsed.sum
fb_subp0_read_sectors | dram__sectors_read.sum
fb_subp1_read_sectors | dram__sectors_read.sum
fb_subp0_write_sectors | dram__sectors_write.sum
fb_subp1_write_sectors | dram__sectors_write.sum
global_atom_cas | smsp__inst_executed_op_generic_atom_dot_cas.sum
gred_count | smsp__inst_executed_op_global_red.sum
inst_executed | sm__inst_executed.sum
inst_executed_fma_pipe_s0 | smsp__inst_executed_pipe_fma.sum
inst_executed_fma_pipe_s1 | smsp__inst_executed_pipe_fma.sum
inst_executed_fma_pipe_s2 | smsp__inst_executed_pipe_fma.sum
inst_executed_fma_pipe_s3 | smsp__inst_executed_pipe_fma.sum
inst_executed_fp16_pipe_s0 | smsp__inst_executed_pipe_fp16.sum
inst_executed_fp16_pipe_s1 | smsp__inst_executed_pipe_fp16.sum
inst_executed_fp16_pipe_s2 | smsp__inst_executed_pipe_fp16.sum
inst_executed_fp16_pipe_s3 | smsp__inst_executed_pipe_fp16.sum
inst_executed_fp64_pipe_s0 | smsp__inst_executed_pipe_fp64.sum
inst_executed_fp64_pipe_s1 | smsp__inst_executed_pipe_fp64.sum
inst_executed_fp64_pipe_s2 | smsp__inst_executed_pipe_fp64.sum
inst_executed_fp64_pipe_s3 | smsp__inst_executed_pipe_fp64.sum
inst_issued1 | sm__inst_issued.sum
l2_subp0_read_sector_misses | lts__t_sectors_op_read_lookup_miss.sum
l2_subp1_read_sector_misses | lts__t_sectors_op_read_lookup_miss.sum
l2_subp0_read_sysmem_sector_queries | lts__t_sectors_aperture_sysmem_op_read.sum
l2_subp1_read_sysmem_sector_queries | lts__t_sectors_aperture_sysmem_op_read.sum
l2_subp0_read_tex_hit_sectors | lts__t_sectors_srcunit_tex_op_read_lookup_hit.sum
l2_subp1_read_tex_hit_sectors | lts__t_sectors_srcunit_tex_op_read_lookup_hit.sum
l2_subp0_read_tex_sector_queries | lts__t_sectors_srcunit_tex_op_read.sum
l2_subp1_read_tex_sector_queries | lts__t_sectors_srcunit_tex_op_read.sum
l2_subp0_total_read_sector_queries | lts__t_sectors_op_read.sum + lts__t_sectors_op_atom.sum + lts__t_sectors_op_red.sum
l2_subp1_total_read_sector_queries | lts__t_sectors_op_read.sum + lts__t_sectors_op_atom.sum + lts__t_sectors_op_red.sum
l2_subp0_total_write_sector_queries | lts__t_sectors_op_write.sum + lts__t_sectors_op_atom.sum + lts__t_sectors_op_red.sum
l2_subp1_total_write_sector_queries | lts__t_sectors_op_write.sum + lts__t_sectors_op_atom.sum + lts__t_sectors_op_red.sum
l2_subp0_write_sector_misses | lts__t_sectors_op_write_lookup_miss.sum
l2_subp1_write_sector_misses | lts__t_sectors_op_write_lookup_miss.sum
l2_subp0_write_sysmem_sector_queries | lts__t_sectors_aperture_sysmem_op_write.sum
l2_subp1_write_sysmem_sector_queries | lts__t_sectors_aperture_sysmem_op_write.sum
l2_subp0_write_tex_hit_sectors | lts__t_sectors_srcunit_tex_op_write_lookup_hit.sum
l2_subp1_write_tex_hit_sectors | lts__t_sectors_srcunit_tex_op_write_lookup_hit.sum
l2_subp0_write_tex_sector_queries | lts__t_sectors_srcunit_tex_op_write.sum
l2_subp1_write_tex_sector_queries | lts__t_sectors_srcunit_tex_op_write.sum
not_predicated_off_thread_inst_executed | smsp__thread_inst_executed_pred_on.sum
pcie_rx_active_pulse |
pcie_tx_active_pulse |
prof_trigger_00 |
prof_trigger_01 |
prof_trigger_02 |
prof_trigger_03 |
prof_trigger_04 |
prof_trigger_05 |
prof_trigger_06 |
prof_trigger_07 |
inst_issued0 | smsp__issue_inst0.sum
sm_cta_launched | sm__ctas_launched.sum
shared_load | smsp__inst_executed_op_shared_ld.sum
shared_store | smsp__inst_executed_op_shared_st.sum
generic_load | smsp__inst_executed_op_generic_ld.sum
generic_store | smsp__inst_executed_op_generic_st.sum
global_load | smsp__inst_executed_op_global_ld.sum
global_store | smsp__inst_executed_op_global_st.sum
local_load | smsp__inst_executed_op_local_ld.sum
local_store | smsp__inst_executed_op_local_st.sum
shared_atom | smsp__inst_executed_op_shared_atom.sum
shared_atom_cas | smsp__inst_executed_op_shared_atom_dot_cas.sum
shared_ld_bank_conflict | l1tex__data_bank_conflicts_pipe_lsu_mem_shared_op_ld.sum
shared_st_bank_conflict | l1tex__data_bank_conflicts_pipe_lsu_mem_shared_op_st.sum
shared_ld_transactions | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_ld.sum
shared_st_transactions | l1tex__data_pipe_lsu_wavefronts_mem_shared_op_st.sum
tensor_pipe_active_cycles_s0 | smsp__pipe_tensor_cycles_active.sum
tensor_pipe_active_cycles_s1 | smsp__pipe_tensor_cycles_active.sum
tensor_pipe_active_cycles_s2 | smsp__pipe_tensor_cycles_active.sum
tensor_pipe_active_cycles_s3 | smsp__pipe_tensor_cycles_active.sum
thread_inst_executed | smsp__thread_inst_executed.sum
warps_launched | smsp__warps_launched.sum

### 2.9. Migration to the Profiling API

The CUPTI event APIs from the header `cupti_events.h` and metric APIs from the header `cupti_metrics.h` will be deprecated in a future CUDA release. The NVIDIA Volta platform is the last architecture on which these APIs are supported. These are being replaced by the Profiling API in the header `cupti_profiler_target.h` and Perfworks Metric API in the headers `nvperf_host.h` and `nvperf_target.h`. These provide low and deterministic profiling overhead on the target system. These APIs also have other significant enhancements such as:

- Range Profiling
- Improved metrics
- Lower overhead for PC Sampling

GPU architectures supported by different CUPTI APIs are listed at the table. Both the event and metric APIs and the profiling APIs are supported for Volta. This is to enable transition of code to the profiling APIs. But one cannot mix the usage of the event and metric APIs and the profiling APIs.

The Profiling APIs are supported on all CUDA supported platforms except Android.

It is important to note that for support of future GPU architectures and feature improvements (such as performance overhead reduction and additional performance metrics), users should use the Profiling APIs. There are few features which are not supported by Profiling APIs, refer to the section for differences from event and metric APIs.

However note that there are no changes to the CUPTI Activity and Callback APIs and these will continue to be supported for the current and future GPU architectures.

### 2.10. CUPTI PC Sampling API

A new set of CUPTI APIs for PC sampling data collection are provided in the header file `cupti_pcsampling.h` which support continuous mode data collection without serializing kernel execution and have a lower runtime overhead. Along with these a utility library is provided in the header file `cupti_pcsampling_util.h` which has APIs for GPU assembly to CUDA-C source correlation and for reading and writing the PC sampling data from/to files.

The PC Sampling APIs are supported on all CUDA supported platforms. These are supported on Volta and later GPU architectures, i.e. devices with compute capability 7.0 and higher.

Overview of Features:

- Two sampling modes – Continuous (concurrent kernels) or Serialized (one kernel at a time)​.
- Option to select stall reasons to collect.​
- Ability to collect GPU PC sampling data for entire application duration or for specific CPU code ranges (defined by start and stop APIs).​
- API to flush GPU PC sampling data.​
- APIs to support Offline and Runtime correlation of GPU PC samples to CUDA C source lines and GPU assembly instructions​.

Samples are provided to demonstrate how to write the injection library to collect the PC sampling information, and how to parse the generated files using the utility APIs to print the stall reasons counter values and associate those with the GPU assembly instructions and CUDA-C source code. Refer to the samples pc_sampling_continuous, pc_sampling_utility and pc_sampling_start_stop.

Note: PC Sampling APIs from the header `cupti_activity.h` would be referred as PC Sampling Activity APIs and APIs from the header `cupti_pcsampling.h` would be referred as PC Sampling APIs.

#### 2.10.1. Configuration Attributes

The following table lists the PC sampling configuration attributes which can be set using the `cuptiPCSamplingSetConfigurationAttribute()` API.

Table 7. PC Sampling Configuration Attributes
Configuration Attribute | Description | Default Value | Comparison of PC Sampling APIs with CUPTI PC Sampling Activity APIs | Guideline to Tune Configuration Option
--- | --- | --- | --- | ---
Collection mode | PC Sampling collection mode - Continuous or Kernel Serialized | Continuous | Continuous mode is new. Kernel Serialized mode is equivalent to the kernel level functionality provided by the CUPTI PC sampling Activity APIs. |
Sampling period | Sampling period for PC Sampling. Valid values for the sampling periods are between 5 to 31 both inclusive. This will set the sampling period to (2^samplingPeriod) cycles. e.g. for sampling period = 5 to 31, cycles = 32, 64, 128,..., 2^31 | CUPTI defined value is based on number of SMs | Dropped current support for 5 levels(MIN, LOW, MID, HIGH, MAX) for sampling period. The new "sampling period" is equivalent to the "samplingPeriod2" field in CUpti_ActivityPCSamplingConfig. | Low sampling period means a high sampling frequency which can result in dropping of samples. Very high sampling period can cause low sampling frequency and no sample generation.
Stall reason | Stall reasons to collect Input is a pointer to an array of the stall reason indexes to collect. | All stall reasons will be collected | With the CUPTI PC sampling Activity APIs there is no option to select which stall reasons to collect. Also the list of supported stall reasons has changed. |
Scratch buffer size | Size of SW buffer for raw PC counter data downloaded from HW buffer. Approximately it takes 16 Bytes (and some fixed size memory) to accommodate one PC with one stall reason e.g. 1 PC with 1 stall reason = 32 Bytes 1 PC with 2 stall reason = 48 Bytes 1 PC with 4 stall reason = 96 Bytes | 1 MB (which can accommodate approximately 5500 PCs with all stall reasons) | New | Clients can choose scratch buffer size as per memory budget. Very small scratch buffer size can cause runtime overhead as more iterations would be required to accommodate and process more PC samples
Hardware buffer size | Size of HW buffer in bytes. If sampling period is too less, HW buffer can overflow and drop PC data | 512 MB | New | Device accessible buffer for samples. Less hardware buffer size with low sampling periods, can cause overflow and dropping of PC data. High hardware buffer size can impact application execution due to lower amount of device memory being available
Enable start/stop control | Control over PC Sampling data collection range. 1 - Allows user to start and stop PC Sampling using APIs | 0 (disabled) | New |

#### 2.10.2. Stall Reasons Mapping Table

The table below lists the stall reasons mapping from PC Sampling Activity APIs to PC Sampling APIs. Note: Stall reasons with suffix _not_issued represents latency samples. These samples indicate that no instruction was issued in that cycle from the warp scheduler from where the warp was sampled.

Table 8. Stall Reasons Mapping Table from PC Sampling Activity APIs to PC Sampling APIs
PC Sampling Activity API Stall Reasons (common prefix: CUPTI_ACTIVITY_PC_SAMPLING_STALL_) | PC Sampling API Stall Reasons (common prefix: smsp__pcsamp_warps_issue_stalled_)
--- | ---
NONE | selected selected_not_issued
INST_FETCH | branch_resolving branch_resolving_not_issued no_instructions no_instructions_not_issued
EXEC_DEPENDENCY | short_scoreboard short_scoreboard_not_issued wait wait_not_issued
MEMORY_DEPENDENCY | long_scoreboard long_scoreboard_not_issued
TEXTURE | tex_throttle tex_throttle_not_issued
SYNC | barrier barrier_not_issued membar membar_not_issued
CONSTANT_MEMORY_DEPENDENCY | imc_miss imc_miss_not_issued
PIPE_BUSY | mio_throttle mio_throttle_not_issued math_pipe_throttle math_pipe_throttle_not_issued
MEMORY_THROTTLE | drain drain_not_issued lg_throttle lg_throttle_not_issued
NOT_SELECTED | not_selected not_selected_not_issued
OTHER | misc misc_not_issued dispatch_stall dispatch_stall_not_issued
SLEEPING | sleeping sleeping_not_issued

#### 2.10.3. Data Structure Mapping Table

The table below lists the data structure mapping from PC Sampling Activity APIs to PC Sampling APIs.

Table 9. Data structure Mapping Table from PC Sampling Activity APIs to PC Sampling APIs
PC Sampling Activity API structures | PC Sampling API structures
--- | ---
CUpti_ActivityPCSamplingConfig | CUpti_PCSamplingConfigurationInfo
CUpti_ActivityPCSamplingStallReason | CUpti_PCSamplingStallReason Refer Stall Reasons Mapping Table
CUpti_ActivityPCSampling3 | CUpti_PCSamplingPCData
CUpti_ActivityPCSamplingRecordInfo | CUpti_PCSamplingData

#### 2.10.4. Data flushing

CUPTI clients can periodically flush GPU PC sampling data using the API `cuptiPCSamplingGetData()`. Besides periodic flushing of GPU PC sampling data, CUPTI clients need to also flush the GPU PC sampling data at the following points to maintain the uniqueness of PCs:

- For continuous collection mode CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS - after each module load-unload-load sequence.
- For serialized collection mode CUPTI_PC_SAMPLING_COLLECTION_MODE_KERNEL_SERIALIZED - after completion of each kernel.
- For range profiling using the configuration option CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL - at the end of the range i.e. after `cuptiPCSamplingStop()` API.

If application is profiled in the continuous collection mode with range profiling disabled, and there is no module unload, CUPTI clients can collect data in two ways:

- By using `cuptiPCSamplingGetData()` API periodically.
- By using `cuptiPCSamplingDisable()` on application exit and reading GPU PC sampling data from sampling data buffer passed during configuration.

Note: In case, `cuptiPCSamplingGetData()` API is not called periodically, the sampling data buffer passed during configuration should be big enough to hold the data for all the PCs.
Note: Field `remainingNumPcs` of the struct `CUpti_PCSamplingData` helps in identifying the number of PC records available with CUPTI. User can adjust the periodic flush interval based on it. Further user need to ensure that all remaining records can be accommodated in the sampling data buffer passed during configuration before disabling the PC sampling.

#### 2.10.5. SASS Source Correlation

Building SASS source correlation for a PC can be split into two parts:

- Correlation of a PC to a SASS instruction - PC to SASS correlation is done during PC sampling at run time and the SASS data is available in the PC record. Fields `cubinCrc`, `pcOffset` and `functionName` in the PC record help in correlatation of a PC with a SASS instruction. You can extract cubins from the application executable or library using the `cuobjdump` utility by executing the command `cuobjdump -xelf all exe/lib`. The cuobjump utility version should match with the CUDA Toolkit version used to build the CUDA application executable or library files. You can find the cubinCrc for extracted cubins using the `cuptiGetCubinCrc()` API. With the help of cubinCrc you can find out the cubin to which a PC belongs. The cubin can be disassembled using the `nvdisasm` utility that comes with the CUDA toolkit.
- Correlation of a SASS instruction to a CUDA source line - Correlation of GPU PC samples to CUDA C source lines can be done offline as well as at runtime with the help of the `cuptiGetSassToSourceCorrelation()` API.

JIT compiled cubins - In case of JIT compiled cubins, it is not possible to extract the cubin from the executable or library. For this case one can subscribe to one of the `CUPTI_CBID_RESOURCE_MODULE_LOADED` or `CUPTI_CBID_RESOURCE_MODULE_UNLOAD_STARTING` or `CUPTI_CBID_RESOURCE_MODULE_PROFILED` callbacks. It returns a `CUpti_ModuleResourceData` structure having the CUDA binary. This binary can be stored in a file and can be used for offline CUDA C source correlation.

#### 2.10.6. API Usage

Here is a pseudo code which shows how to collect the PC sampling data for specific CPU code ranges:

    void Collection()
    {
        // Select collection mode
        CUpti_PCSamplingConfigurationInfoParams pcSamplingConfigurationInfoParams = {};

        CUpti_PCSamplingConfigurationInfo collectionMode = {};
        collectionMode.attributeData.collectionModeData.collectionMode = CUPTI_PC_SAMPLING_COLLECTION_MODE_CONTINUOUS;

        pcSamplingConfigurationInfoParams.numAttributes = 1;
        pcSamplingConfigurationInfoParams.pPCSamplingConfigurationInfo = &collectionMode;
        cuptiPCSamplingSetConfigurationAttribute(&pcSamplingConfigurationInfoParams);

        // Select stall reasons to collect
        {
            // Get number of supported stall reasons
            cuptiPCSamplingGetNumStallReasons();
            // Get number of supported stall reason names and corresponding indexes
            cuptiPCSamplingGetStallReasons();
            // Set selected stall reasons
            cuptiPCSamplingSetConfigurationAttribute();
        }

        // Select code range using start/stop APIs
        // Opt-in for start and stop PC Sampling using APIs cuptiPCSamplingStart and cuptiPCSamplingStop
        CUpti_PCSamplingConfigurationInfo enableStartStop = {};
        enableStartStop.attributeType = CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_ENABLE_START_STOP_CONTROL;
        enableStartStop.attributeData.enableStartStopControlData.enableStartStopControl = true;

        pcSamplingConfigurationInfoParams.numAttributes = 1;
        pcSamplingConfigurationInfoParams.pPCSamplingConfigurationInfo = &enableStartStop;
        cuptiPCSamplingSetConfigurationAttribute(&pcSamplingConfigurationInfoParams);

        // Enable PC Sampling
        cuptiPCSamplingEnable();

        kernelA <<<blocks, threads, 0, s0>>>(...);                  // KernelA is not sampled

        // Start PC sampling collection
        cuptiPCSamplingStart();
        {
            // KernelB and KernelC might run concurrently since 'continuous' sampling collection mode is selected
            kernelB <<<blocks, threads, 0, s0>>>(...);              // KernelB is sampled
            kernelC <<<blocks, threads, 0, s1>>>(...);              // KernelC is sampled
        }
        // Stop PC sampling collection
        cuptiPCSamplingStop();
        // Flush PC sampling data
        cuptiPCSamplingGetData();

        kernelD <<<blocks, threads, 0, s0>>>(...);                  // KernelD is not sampled

        // Start PC sampling collection
        cuptiPCSamplingStart();
        {
            kernelE <<<blocks, threads, 0, s0>>>(...);              // KernelE is sampled
        }
        // Stop PC sampling collection
        cuptiPCSamplingStop();
        // Flush PC sampling data
        cuptiPCSamplingGetData();

        // Disable PC Sampling
        cuptiPCSamplingDisable();
    }

#### 2.10.7. Limitations

Known limitations and issues:

- In the serial mode, PC Sampling APIs do not provide information for correlation of PC sampling data for a kernel to the CUDA kernel launch API. This is supported by the PC Sampling activity APIs. For continuous mode, this cannot be supported due to hardware limitations.
- PC Sampling APIs don't support simultaneous sampling of multiple CUDA contexts on a GPU. However, simultaneous sampling of single CUDA context per GPU is supported. Before enabling and configuring the PC sampling on a different CUDA context on the same GPU, PC sampling needs to be disabled on the other context.

### 2.11. CUPTI Checkpoint API

Starting with CUDA 11.5, CUPTI ships with a new library to assist tool developers who wish to replay kernels under direct control, such as tools using the Profiling API User Replay mode. This new Checkpoint library provides support for automatically saving and restoring device state for many common uses.

A device checkpoint is a managed copy of device functional state - including values in memory, along with some (but not all) other user visible state of the device. When a checkpoint is saved, this state is saved to internal buffers, preferentially using free device, then host, and finally filesystem space to save the data. The user tool maintains a handle to a checkpoint, and is able to restore the checkpoint with a single call, restoring the state so a kernel may be re-executed and expect to have the same device state as when the checkpoint was saved.

Once saved, a checkpoint may be restored any time including after multiple kernels have been launched, though currently there are limitations on which user calls (CUDA or driver API calls) have been validated to work between a `Save` and `Restore`. It currently is known safe to launch multiple kernels on a context and to do memcpy calls before restoring a checkpoint. Future versions of CUPTI will extend this to support additional API calls between a `Save` and `Restore`.

Checkpoints may be saved during injected kernel launch callbacks or directly coded into a target application.

Certain APIs are known to not work with the version of the `Checkpoint` API shipped with CUPTI 11.5, including Stream Capture mode.

#### 2.11.1. Usage

There is one header for the library, `cupti_checkpoint.h`, which needs to be included, and libcheckpoint needs to be linked in to the application or injection library. Though the checkpoint library doesn't depend on cupti, the error codes returned by the API are shared with cupti, so linking libcupti in is needed in order to translate the return codes to string representations.

The Checkpoint API follows a similar design to other CUPTI APIs. API behavior is controlled through a structure, `CUpti_Checkpoint`, which is initialized by a tool or application, then passed to `cuptiCheckpointSave`. If the call is successful, the structure saves a handle to a checkpoint. At this point, the application may make a series of calls which modify device state (kernels which update memory, memcopies, etc), and when the device state should be restored, the tool can use the same structure in calls to `cuptiCheckpointRestore`, and finally a call to `cuptiCheckpointFree` to release the resources used by the checkpoint object.

Multiple checkpoints may be saved at the same time. If multiple checkpoints exist, they operate entirely independently - each checkpoint consumes the full resources needed to restore the device state at the point it was saved. Order of operations between multiple checkpoints is not enforced by the API - while a common use for multiple checkpoints may be a nested pattern, it is also possible to interleave checkpoint operations.

Between a `cuptiCheckpointSave` and `cuptiCheckpointRestore`, any number of standard kernel launches (or equivalent API calls such as `cuLaunchKernel`) or memcpy calls may be made. Additionally, any host (cpu) side calls may be made that do not affect device state. It is possible that other CUDA or driver API calls may be made, but have not been validated with the 11.5 release.

Several options exist in the `CUpti_Checkpoint` structure. They must be set prior to the initial `cuptiCheckpointSave` using that structure. Any further changes to the structure are ignored until after a call to `cuptiCheckpointFree`, at which point the structure can be re-configured and re-used.

Important per-checkpoint options:

- `structSize` - must be set to the value of `CUpti_Checkpoint_STRUCT_SIZE`
- `ctx` - if NULL, the checkpoint will be of the default CUDA context, otherwise, specifies which context
- `reserveDeviceMB` - Restrict a checkpoint save from using at least this much device memory
- `reserveHostMB` - Restrict a checkpoint save from using at least this much host memory
- `allowOverwrite` - It is normally an error to call Save using an existing checkpoint handle (one which has not been Freed). When set, this option allows the Save operation to be called multiple times on a handle. Note that when using this option, the `CUpti_Checkpoint` options are not re-read on any subsequent Save. To read new options, the handle must be passed to `cuptiCheckpointFree` prior to the `cuptiCheckpointSave` call.
- `optimizations` - Bitmask of options for checkpoint behavior
  - `CUPTI_CHECKPOINT_OPT_TRANSFER` - Normally when restoring a checkpoint, all existing device memory at the time of the save is restored. This optimization adds a test to see whether a block of memory has changed before restoring it and caches the results for subsequent calls to Restore. Use of this option requires that all Restore calls be done at the same point in an application for a given checkpoint. As the optimization may be computationally expensive, it is most useful when there is a significant amount of data that can be skipped and there will be several calls to Restore the checkpoint.

#### 2.11.2. Restrictions

Checkpoints API calls may not be made during a stream capture. They also may not be inserted into a graph. Beyond kernel launches (cuLaunchKernel, standard kernel<<<>>> launches, etc) and memcpy calls, the remaining CUDA and driver API calls have not been validated within a Checkpoint `Save` and `Restore` region. Any other CUDA or driver API calls (example - device malloc or free) may work, or may cause undetermined behavior. Additional APIs will be validated to work with the Checkpoint API in future releases.

The Checkpoint API does not have visibility into which API calls have been made between `cuptiCheckpointSave` and `cuptiCheckpointRestore` calls, and may not be able to correctly detect error cases if unsupported calls have been made. In this case it is possible that device state may only be partially restored by `cuptiCheckpointRestore`, which may casue functionally incorrect behavior in subsequent device calls.

The Checkpoint API only restores functionally visible device state, not performance critical state. Some performance characteristics, such as state of the caches, will not be saved by a checkpoint, and saving or restoring a checkpoint may change the occupancy and alter performance for subsequent device calls.

The Checkpoint API makes no attempt to restore host (non-device) state, beyond freeing the resources it internally uses during a call to `cuptiCheckpointFree`.

The Checkpoint API by default uses device memory, host memory, and finally the filesystem to back up the device state. It is possible that addition of a `cuptiCheckpointSave` causes a later device allocation to fail due to the increased device memory usage. (Similarly, host memory is also used, and may be affected by a checkpoint). To allow the user to guarantee a certain amount of device or host memory remains available for later use, `reserveDeviceMB` and `reserveHostMB` fields in the `CUpti_Checkpoint` struct may be set. Use of these fields will guarantee that the device or host memory will leave that much memory free during a `cuptiCheckpointSave` call, but may cause the Checkpoint API call performance to degrade due to increased use of slower storage spaces.

#### 2.11.3. Examples

The Checkpoint API does not require any other CUPTI calls. A simple use case could be to compare the output of three different implementations of a kernel. Pseudocode for this could look like:

    CUpti_Checkpoint cp = { CUpti_Checkpoint_STRUCT_SIZE };

    int kernel = 0;
    do
    {
      if (kernel == 0)
        cuptiCheckpointSave(&cp);
      else
        cuptiCheckpointRestore(&cp);

      if (kernel == 0)
        kernel_1<<<>>>(...);
      else if (kernel == 1)
        kernel_2<<<>>>(...);
      else if (kernel == 2)
        kernel_3<<<>>>(...);
    } while (kernel++ < 3);

    cuptiCheckpointFree(&cp);

In this example, even if any of the kernels modify their own input data, the subsequent passes through the loop will still run correctly - the modified input data would be restored by each call to `cuptiCheckpointRestore` before the next kernel runs. This is particularly useful when a programmer does not know the exact state of the device prior to a kernel call - the Checkpoint API ensures that all needed data is saved and restored, which would not otherwise be practical or perhaps even possible in some complex cases.
Another possible use case could be for fuzzing - randomly modifying input to a kernel, and ensuring it performs as expected. Instead of manually restoring device state to a known good point, the Checkpoint API and initialize a good state, and the fuzzer can modify only what is needed.

    CUpti_Checkpoint cp = { CUpti_Checkpoint_STRUCT_SIZE };

    int i = 0;
    do
    {
      if (i == 0)
        cuptiCheckpointSave(&cp);
      else
        cuptiCheckpointRestore(&cp);

      setup_test<<<>>>(i, ...);

      kernel<<<>>>(...);

      validate_result<<<>>>(i, ...);
    } while (i++ < num_tests);

    cuptiCheckpointFree(&cp);

Finally, the Checkpoint API is very useful for the User Replay mode of the CUPTI Profiling API. The User Replay mode can be very desireable as it allows kernels to run concurrently, which Kernel Replay mode does not, and only replays parts of the application which are within a performance region, unlike Applicatin Replay mode. However, in this mode, a kernel potentially needs to be launched multiple times in order to gather all requested metrics. This is complicated when the kernel may modify some of its own input data, and without the Checkpoint API, would require the tool developer to handle restoring any modified input data manually. It is difficult for a tool to automatically know whether any data needs to be restored before each iteration, or even what the existing state of the device is. Using the Checkpoint API, the tool can guarantee that input data will be restored each pass.

    CUpti_Checkpoint cp = { CUpti_Checkpoint_STRUCT_SIZE };

    // Pseudocode - assume all Profiling API structures are already initialized correctly
    cuptiProfilerBeginSession(&beginSessionParams);
    cuptiProfilerSetConfig(&setConfigParams);
    int numPasses = 0;
    bool lastPass = false;
    do
    {
      if (numPasses == 0)
        cuptiCheckpointSave(&cp);
      else
        cuptiCheckpointRestore(&cp);

      cuptiProfilerBeginPass(&beginPassParams);
      cuptiProfilerEnableProfiling(&enableProfilingParams);
      cuptiProfilerPushRange(&pushRangeParams);

      // Kernel launch on N separate streams - will be profiled while running concurrently
      kernel<<<..., stream0>>>(...);
      kernel<<<..., stream1>>>(...);
      ...
      kernel<<<..., streamN>>>(...);

      cudaStreamSynchronize(stream0);
      cudaStreamSynchronize(stream1);
      ...
      cudaStreamSynchronize(streamN);

      cuptiProfilerPopRange(&popRangeParams);
      cuptiProfilerDisableProfiling(&disableProfilingParams);
      lastPass = cuptiProfilerEndPass(&endPassParams);
    } while (lastPass == false);
    cuptiProfilerFlushCounterData(&flushCounterDataParams);
    cuptiProfilerUnsetConfig(&unsetConfigParams);
    cuptiProfilerEndSession(&endSessionParams);

In this example, the Profiler range will span all concurrently running kernels, which may modify their own input data - each pass through the loop will restore the initial values.

### 2.12. CUPTI overhead

CUPTI incurs overhead when used for tracing or profiling of the CUDA application. Overhead can vary significantly from one application to another. It largely depends on the density of the CUDA activities in the application; lesser the CUDA activities, less the CUPTI overhead. In general overhead of tracing i.e. activity APIs is much lesser than the profiling i.e. event and metric APIs.

#### 2.12.1. Tracing Overhead

One of the goal of the tracing APIs is to provide a non-invasive collection of the timing information of the CUDA activities. Tracing is a low-overhead mechanism for collecting fine-grained runtime information.

##### 2.12.1.1. Execution overhead

Factors affecting the execution overhead under tracing are:

- Serial kernel trace enabled using the activity kind `CUPTI_ACTIVITY_KIND_KERNEL` can significantly change the overall performance characteristics of the application because all kernel executions are serialized on the GPU. For applications which use only a single CUDA stream and therefore cannot have concurrent kernel execution, this mode can be useful as it usually (not always) incurs less profiling overhead compared to the concurrent kernel mode.
- Concurrent kernel trace enabled using the activity kind `CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL` doesn't affect the concurrency of the kernels in the application. In this mode, CUPTI instruments the kernel code to collect the timing information. A single instrumentation code is generated at the time of loading the CUDA module and applied to each kernel during the kernel execution. Instrumentation code generation overhead is attributed as `CUPTI_ACTIVITY_OVERHEAD_CUPTI_INSTRUMENTATION` in the activity record `CUpti_ActivityOverhead`.
- Due to the code instrumentation, concurrent kernel mode can add significant runtime overhead if used on kernels that execute a large number of blocks and that have short execution durations.

##### 2.12.1.2. Memory overhead

CUPTI allocates device and pinned system memory for storing the tracing information:

- Static memory allocation: CUPTI allocates 3 buffers of 3 MB each in the pinned system memory for each CUDA context by default during the context creation phase. This is used for storing the concurrent kernel, serial kernel, memcopy and memset tracing information and these buffers are sufficient for storing information for about 300K such activities. The number of buffers is controlled using the attribute `CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_PRE_ALLOCATE_VALUE` and the size of the buffer is determined by the attribute `CUPTI_ACTIVITY_ATTR_DEVICE_BUFFER_SIZE`. User can change the buffer size at any time during the profiling session, but this setting takes effect only for new buffer allocations. It is recommended to adjust the buffer size before the creation of any CUDA context to make sure that all the pre-allocated buffers are of the adjusted size.
- Dynamic memory allocation: Once profiling buffers to store the tracing information are exhausted, CUPTI allocates another buffer of the same size. Note that memory footprint will not always scale with the kernel, memcopy, memset count because CUPTI reuses the buffer after processing all the records in the buffer. For applications with a high density of these activities CUPTI may allocate more buffers.

All of the CUPTI allocated memory associated with a context is freed when the context is destroyed. Memory allocation overhead is attributed as `CUPTI_ACTIVITY_OVERHEAD_CUPTI_RESOURCE` in the activity record `CUpti_ActivityOverhead`. If there are no CUDA contexts created then CUPTI will not allocate corresponding buffers.
CUPTI allocates memory to store unique kernel names, NVTX ranges, CUDA module cubin:

- Kernel trace: For kernel tracing enabled using the activity kind `CUPTI_ACTIVITY_KIND_KERNEL` or `CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL` CUPTI allocates memory to store the kernel name in the records. It is recommended to not free the memory allocated for the kernel name in the kernel activity record as the kernel name memory space might be common across all kernel records having the same kernel name.
- NVTX ranges: For NVTX enabled using the activity kind `CUPTI_ACTIVITY_KIND_MARKER` CUPTI allocates memory to store the range name in the records. It is recommended to not free the memory allocated for the NVTX range name in the marker activity record as the NVTX range name memory space will be common across all NVTX range records having the same name.
- CUDA module cubin: CUPTI stores the data related to the modules loaded by the application i.e. the cubin image. All of the CUPTI allocated memory associated with the cubin image of the module is freed when the module is unloaded.

#### 2.12.2. Profiling Overhead

Events and metrics collection using CUPTI incurs runtime overhead. This overhead depends on the number and type of events and metrics selected. Since each metric is computed from one or more events, metric overhead depends on the number and type of underlying events. The overhead includes time spent in configuration of hardware events and reading of hardware event values.

Factors affecting the execution overhead under profiling are:

- Overhead is less for hardware provided events and metrics.
  - For event and metric APIs, events which are collected using the collection method `CUPTI_EVENT_COLLECTION_METHOD_PM` or `CUPTI_EVENT_COLLECTION_METHOD_SM` fall in this category.
  - For Profiling APIs, metrics which don't have string "sass" in the name fall in this category.
- Software instrumented events and metrics are expensive as CUPTI needs to instrument the kernel to collect these. Further these events and metrics cannot be combined with any other event or metric in the same pass as otherwise instrumented code will also contribute to the event value.
  - For event and metric APIs, the collection method `CUPTI_EVENT_COLLECTION_METHOD_INSTRUMENTED` fall in this cateogry.
  - For Profiling APIs, metrics which have string "sass" in the name fall in this category.
- In the serial mode, profiling may significantly change the overall performance characteristics of the application because all kernel executions are serialized on the GPU. This is done to enable tight event or metric collection around each kernel.
  - For event and metric APIs, the collection mode `CUPTI_EVENT_COLLECTION_MODE_KERNEL`, serializes all kernel executions on the GPU that occur between the APIs `cuptiEventGroupEnable` and `cuptiEventGroupDisable`. On the other hand, kernel concurrency can be maintained by using the collection mode `CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS` and restricting profiling to events and metrics that can be collected in a single pass.
  - For Profiling APIs, auto range mode serializes all kernel executions on the GPU. On the other hand, kernel concurrency can be maintained by using the user range mode.
- When all the requested events or metrics cannot be collected in the single pass due to hardware or software limitations, one needs to replay the exact same set of GPU workloads multiple times. This can be achieved at the kernel granularity by replaying kernel multiple times or by launching the entire application multiple times. CUPTI provides support for kernel replay only. Application replay can be done by the CUPTI client.
- When kernel replay is used the overhead to save and restore kernel state for each replay pass depends on the amount of device memory used by the kernel. Application replay is expected to perform better than kernel replay for the case when the size of device memory used by the kernel is high.

### 2.13. Samples

The CUPTI installation includes several samples that demonstrate the use of the CUPTI APIs. These samples can be referred to for the usage of different APIs supported by CUPTI. The samples are:

Activity API

activity_trace_async
  This sample shows how to collect a trace of CPU and GPU activity using the new asynchronous activity buffer APIs.
callback_timestamp
  This sample shows how to use the callback API to record a trace of API start and stop times.
cuda_graphs_trace
  This sample shows how to collect the trace of CUDA graphs and correlate the graph node launch to the node creation API using CUPTI callbacks.
cuda_memory_trace
  This sample shows how to collect the trace of CUDA memory operations. The sample also traces CUDA memory operations done via default memory pool.
cupti_correlation
  This sample shows how to do the correlation between CUDA APIs and corresponding GPU activities.
cupti_external_correlation
  This sample shows how to do the correlation of CUDA API activity records with external APIs.
cupti_finalize
  This sample shows how to use API `cuptiFinalize()` to dynamically detach and attach CUPTI.
cupti_nvtx
  This sample shows how to receive NVTX callbacks and collect NVTX records in CUPTI.
cupti_trace_injection
  This sample shows how to build an injection library using the CUPTI activity and callback APIs. It can be used to trace CUDA APIs and GPU activities for any CUDA application. It does not require the CUDA application to be modified.
nvlink_bandwidth
  This sample shows how to collect NVLink topology and NVLink throughput metrics in continuous mode.
openacc_trace
  This sample shows how to use CUPTI APIs for OpenACC data collection.
pc_sampling
  This sample shows how to collect PC Sampling profiling information for a kernel using the PC Sampling Activity APIs.
sass_source_map
  This sample shows how to generate CUpti_ActivityInstructionExecution records and how to map SASS assembly instructions to CUDA C source.
unified_memory
  This sample shows how to collect information about page transfers for unified memory.

Event and Metric APIs

callback_event
  This sample shows how to use both the callback and event APIs to record the events that occur during the execution of a simple kernel. The sample shows the required ordering for synchronization, and for event group enabling, disabling, and reading.
callback_metric
  This sample shows how to use both the callback and metric APIs to record the metric's events during the execution of a simple kernel, and then use those events to calculate the metric value.
cupti_query
  This sample shows how to query CUDA-enabled devices for their event domains, events, and metrics.
event_multi_gpu
  This sample shows how to use the CUPTI event and CUDA APIs to sample events on a setup with multiple GPUs. The sample shows the required ordering for synchronization, and for event group enabling, disabling, and reading.
event_sampling
  This sample shows how to use the event APIs to sample events using a separate host thread.

Profiling API

extensions
  This includes utilities used in some of the samples.
autorange_profiling
  This sample shows how to use profiling APIs to collect metrics in autorange mode.
callback_profiling
  This sample shows how to use callback and profiling APIs to collect the metrics during the execution of a kernel. It shows how to use different phases of profiling i.e. enumeration, configuration, collection and evaluation in the appropriate callbacks.
concurrent_profiling
  This sample shows how to use the profiling API to record metrics from concurrent kernels launched in two different ways - using multiple streams on a single device, and using multiple threads with multiple devices.
cupti_metric_properties
  This sample shows how to query various properties of metrics using the Profiling APIs. The sample shows collection method (hardware or software) and number of passes required to collect a list of metrics.
nested_range_profiling
  This sample shows how to profile nested ranges using the Profiling APIs.
profiling_injection
  This sample for Linux systems shows how to build an injection library which can automatically enable CUPTI's Profiling API using Auto Ranges with Kernel Replay mode. It can attach to an application which was not instrumented using CUPTI and profile any kernel launches.
userrange_profiling
  This sample shows how to use profiling APIs to collect metrics in user specified range mode.

PC Sampling API

pc_sampling_continuous
  This injection sample shows how to collect PC Sampling profiling information using the PC Sampling APIs. A perl script libpc_sampling_continuous.pl is provided to run the CUDA application with different PC sampling options. Use the command './libpc_sampling_continuous.pl --help' to list all the options. The CUDA application code does not need to be modified. Refer the README.txt file shipped with the sample for instructions to build and use the injection library.
pc_sampling_start_stop
  This sample shows how to collect PC Sampling profiling information for kernels within a range using the PC Sampling start/stop APIs.
pc_sampling_utility
  This utility takes the pc sampling data file generated by the pc_sampling_continuous injection library as input. It prints the stall reason counter values at the GPU assembly instruction level. It also does GPU assembly to CUDA-C source correlation and shows the CUDA-C source file name and line number. Refer the README.txt file shipped with the sample for instructions to build and run the utility.

Checkpoint API

checkpoint_kernels
  This sample shows how to use the Checkpoint API to restore device memory, allowing a kernel to be replayed, even if it modifies its input data.