# CUPTI Profiling API

## Data Structures
struct | CUpti_Profiler_BeginPass_Params
| Params for cuptiProfilerBeginPass. More...
struct | CUpti_Profiler_BeginSession_Params
| Params for cuptiProfilerBeginSession. More...
struct | CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params
| Params for cuptiProfilerCounterDataImageCalculateScratchBufferSize. More...
struct | CUpti_Profiler_CounterDataImage_CalculateSize_Params
| Params for cuptiProfilerCounterDataImageCalculateSize. More...
struct | CUpti_Profiler_CounterDataImage_Initialize_Params
| Params for cuptiProfilerCounterDataImageInitialize. More...
struct | CUpti_Profiler_CounterDataImage_InitializeScratchBuffer_Params
| Params for cuptiProfilerCounterDataImageInitializeScratchBuffer. More...
struct | CUpti_Profiler_CounterDataImageOptions
| Input parameter to define the counterDataImage. More...
struct | CUpti_Profiler_DeInitialize_Params
| Default parameter for cuptiProfilerDeInitialize. More...
struct | CUpti_Profiler_DeviceSupported_Params
| Params for cuptiProfilerDeviceSupported. More...
struct | CUpti_Profiler_DisableProfiling_Params
| Params for cuptiProfilerDisableProfiling. More...
struct | CUpti_Profiler_EnableProfiling_Params
| Params for cuptiProfilerEnableProfiling. More...
struct | CUpti_Profiler_EndPass_Params
| Params for cuptiProfilerEndPass. More...
struct | CUpti_Profiler_EndSession_Params
| Params for cuptiProfilerEndSession. More...
struct | CUpti_Profiler_FlushCounterData_Params
| Params for cuptiProfilerFlushCounterData. More...
struct | CUpti_Profiler_GetCounterAvailability_Params
| Params for cuptiProfilerGetCounterAvailability. More...
struct | CUpti_Profiler_Initialize_Params
| Default parameter for cuptiProfilerInitialize. More...
struct | CUpti_Profiler_IsPassCollected_Params
| Params for cuptiProfilerIsPassCollected. More...
struct | CUpti_Profiler_SetConfig_Params
| Params for cuptiProfilerSetConfig. More...
struct | CUpti_Profiler_UnsetConfig_Params
| Params for cuptiProfilerUnsetConfig. More...
## Enumerations
enum | CUpti_Profiler_API { CUPTI_PROFILER_RANGE_PROFILING = 0, CUPTI_PROFILER_PC_SAMPLING, CUPTI_PROFILER_SASS_METRICS }
| Profiler API types. More...
enum | CUpti_Profiler_Support_Level { CUPTI_PROFILER_CONFIGURATION_UNKNOWN = 0, CUPTI_PROFILER_CONFIGURATION_UNSUPPORTED, CUPTI_PROFILER_CONFIGURATION_DISABLED, CUPTI_PROFILER_CONFIGURATION_SUPPORTED }
| Generic support level enum for CUPTI. More...
enum | CUpti_ProfilerRange { CUPTI_Range_INVALID, CUPTI_AutoRange, CUPTI_UserRange, CUPTI_Range_COUNT }
| Profiler range attribute. More...
enum | CUpti_ProfilerReplayMode { CUPTI_Replay_INVALID, CUPTI_ApplicationReplay, CUPTI_KernelReplay, CUPTI_UserReplay, CUPTI_Replay_COUNT }
| Profiler replay attribute. More...
## Functions
CUptiResult | cuptiProfilerBeginPass (CUpti_Profiler_BeginPass_Params *pParams)
| Replay API: used for multipass collection.
CUptiResult | cuptiProfilerBeginSession (CUpti_Profiler_BeginSession_Params *pParams)
| Begin profiling session sets up the profiling on the device.
CUptiResult | cuptiProfilerCounterDataImageCalculateScratchBufferSize (CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params *pParams)
| A temporary storage for CounterData image needed for internal operations.
CUptiResult | cuptiProfilerCounterDataImageCalculateSize (CUpti_Profiler_CounterDataImage_CalculateSize_Params *pParams)
| A CounterData image allocates space for values for each counter for each range.
CUptiResult | cuptiProfilerDeInitialize (CUpti_Profiler_DeInitialize_Params *pParams)
| DeInitializes the profiler interface.
CUptiResult | cuptiProfilerDeviceSupported (CUpti_Profiler_DeviceSupported_Params *pParams)
| Query device compatibility with Profiling API.
CUptiResult | cuptiProfilerDisableProfiling (CUpti_Profiler_DisableProfiling_Params *pParams)
| Disable Profiling.
CUptiResult | cuptiProfilerEnableProfiling (CUpti_Profiler_EnableProfiling_Params *pParams)
| Enables Profiling.
CUptiResult | cuptiProfilerEndPass (CUpti_Profiler_EndPass_Params *pParams)
| Replay API: used for multipass collection.
CUptiResult | cuptiProfilerEndSession (CUpti_Profiler_EndSession_Params *pParams)
| Ends profiling session.
CUptiResult | cuptiProfilerFlushCounterData (CUpti_Profiler_FlushCounterData_Params *pParams)
| Decode all the submitted passes.
CUptiResult | cuptiProfilerGetCounterAvailability (CUpti_Profiler_GetCounterAvailability_Params *pParams)
| Query counter availibility.
CUptiResult | cuptiProfilerInitialize (CUpti_Profiler_Initialize_Params *pParams)
| Initializes the profiler interface.
CUptiResult | cuptiProfilerIsPassCollected (CUpti_Profiler_IsPassCollected_Params *pParams)
| Asynchronous call to query if the submitted pass to GPU is collected.
CUptiResult | cuptiProfilerPopRange (CUpti_Profiler_PopRange_Params *pParams)
| Range API's : Pop user range.
CUptiResult | cuptiProfilerPushRange (CUpti_Profiler_PushRange_Params *pParams)
| Range API's : Push user range.
CUptiResult | cuptiProfilerSetConfig (CUpti_Profiler_SetConfig_Params *pParams)
| Set metrics configuration to be profiled.
CUptiResult | cuptiProfilerUnsetConfig (CUpti_Profiler_UnsetConfig_Params *pParams)
| Unset metrics configuration profiled.

## Detailed Description

Functions, types, and enums that implement the CUPTI Profiling API.

## Enumeration Type Documentation

enum CUpti_Profiler_API

Enumerator:

  CUPTI_PROFILER_RANGE_PROFILING | CUPTI APIs for range based profiling (cuptiProfiler*).
  CUPTI_PROFILER_PC_SAMPLING | CUPTI APIs collecting pc sampling data (cuptiPcSampling*).
  CUPTI_PROFILER_SASS_METRICS | CUPTI APIs collecting SASS metrics data (cuptiSassMetrics*).

enum CUpti_Profiler_Support_Level

Enumerator:

  CUPTI_PROFILER_CONFIGURATION_UNKNOWN | Configuration support level unknown - either detection code errored out before setting this value, or unable to determine it.
  CUPTI_PROFILER_CONFIGURATION_UNSUPPORTED | Profiling is unavailable. For specific feature fields, this means that the current configuration of this feature does not work with profiling. For instance, SLI-enabled devices do not support profiling, and this value would be returned for SLI on an SLI-enabled device.
  CUPTI_PROFILER_CONFIGURATION_DISABLED | Profiling would be available for this configuration, but was disabled by the system.
  CUPTI_PROFILER_CONFIGURATION_SUPPORTED | Profiling is supported. For specific feature fields, this means that the current configuration of this feature works with profiling. For instance, SLI-enabled devices do not support profiling, and this value would only be returned for devices which are not SLI-enabled.

enum CUpti_ProfilerRange

A metric enabled in the session's configuration is collected separately per unique range-stack in the pass. This is an attribute to collect metrics around each kernel in a profiling session or in an user defined range.

Enumerator:

  CUPTI_Range_INVALID | Invalid value
  CUPTI_AutoRange | Ranges are auto defined around each kernel in a profiling session
  CUPTI_UserRange | A range in which metric data to be collected is defined by the user
  CUPTI_Range_COUNT | Range count

enum CUpti_ProfilerReplayMode

For metrics which require multipass collection, a replay of the GPU kernel(s) is required. This is an attribute which specify how the replay of the kernel(s) to be measured is done.

Enumerator:

  CUPTI_Replay_INVALID | Invalid Value
  CUPTI_ApplicationReplay | Replay is done by CUPTI user around the process
  CUPTI_KernelReplay | Replay is done around kernel implicitly by CUPTI
  CUPTI_UserReplay | Replay is done by CUPTI user within a process
  CUPTI_Replay_COUNT | Replay count

## Function Documentation

CUptiResult cuptiProfilerBeginPass | ( | CUpti_Profiler_BeginPass_Params * | pParams | ) |

These APIs are used if user chooses to replay by itself CUPTI_UserReplay or CUPTI_ApplicationReplay for multipass collection of the metrics configurations. It's a no-op in case of CUPTI_KernelReplay.

CUptiResult cuptiProfilerBeginSession | ( | CUpti_Profiler_BeginSession_Params * | pParams | ) |

Although, it doesn't start the profiling but GPU resources needed for profiling are allocated. Outside of a session, the GPU will return to its normal operating state.

CUptiResult cuptiProfilerCounterDataImageCalculateScratchBufferSize | ( | CUpti_Profiler_CounterDataImage_CalculateScratchBufferSize_Params * | pParams | ) |

Use these APIs to calculate the allocation size and initialize counterData image scratch buffer.

CUptiResult cuptiProfilerCounterDataImageCalculateSize | ( | CUpti_Profiler_CounterDataImage_CalculateSize_Params * | pParams | ) |

User borne the resposibility of managing the counterDataImage allocations. CounterDataPrefix contains meta data about the metrics that will be stored in counterDataImage. Use these APIs to calculate the allocation size and initialize counterData image.

CUptiResult cuptiProfilerDeviceSupported | ( | CUpti_Profiler_DeviceSupported_Params * | pParams | ) |

Use this call to determine whether a compute device and configuration are compatible with the Profiling API. If the configuration does not support profiling, one of several flags will indicate why.

CUptiResult cuptiProfilerDisableProfiling | ( | CUpti_Profiler_DisableProfiling_Params * | pParams | ) |

In CUPTI_AutoRange, these APIs are used to enable/disable profiling for the kernels to be executed in a profiling session.

CUptiResult cuptiProfilerEnableProfiling | ( | CUpti_Profiler_EnableProfiling_Params * | pParams | ) |

In CUPTI_AutoRange, these APIs are used to enable/disable profiling for the kernels to be executed in a profiling session.

CUptiResult cuptiProfilerEndPass | ( | CUpti_Profiler_EndPass_Params * | pParams | ) |

These APIs are used if user chooses to replay by itself CUPTI_UserReplay or CUPTI_ApplicationReplay for multipass collection of the metrics configurations. Its a no-op in case of CUPTI_KernelReplay. Returns information for next pass.

CUptiResult cuptiProfilerEndSession | ( | CUpti_Profiler_EndSession_Params * | pParams | ) |

Frees up the GPU resources acquired for profiling. Outside of a session, the GPU will return to it's normal operating state.

CUptiResult cuptiProfilerFlushCounterData | ( | CUpti_Profiler_FlushCounterData_Params * | pParams | ) |

Flush Counter data API to ensure every pass is decoded into the counterDataImage passed at beginSession. This will cause the CPU/GPU sync to collect all the undecoded pass.

CUptiResult cuptiProfilerGetCounterAvailability | ( | CUpti_Profiler_GetCounterAvailability_Params * | pParams | ) |

Use this API to query counter availability information in a buffer which can be used to filter unavailable raw metrics on host. Note: This API may fail, if any profiling or sampling session is active on the specified context or its device.

CUptiResult cuptiProfilerInitialize | ( | CUpti_Profiler_Initialize_Params * | pParams | ) |

Loads the required libraries in the process address space. Sets up the hooks with the CUDA driver.

CUptiResult cuptiProfilerPopRange | ( | CUpti_Profiler_PopRange_Params * | pParams | ) |

Counter data is collected per unique range-stack. Identified by a string label passsed by the user. It's an invalid operation in case of CUPTI_AutoRange.

CUptiResult cuptiProfilerPushRange | ( | CUpti_Profiler_PushRange_Params * | pParams | ) |

Counter data is collected per unique range-stack. Identified by a string label passsed by the user. It's an invalid operation in case of CUPTI_AutoRange.

CUptiResult cuptiProfilerSetConfig | ( | CUpti_Profiler_SetConfig_Params * | pParams | ) |

Use these APIs to set the config to profile in a session. It can be used for advanced cases such as where multiple configurations are collected into a single CounterData Image on the need basis, without restarting the session.