# CUPTI Event API

## Data Structures
struct | CUpti_EventGroupSet
| A set of event groups. More...
struct | CUpti_EventGroupSets
| A set of event group sets. More...
## Defines
#define | CUPTI_EVENT_INVALID ((uint64_t)0xFFFFFFFFFFFFFFFEULL)
| The value that indicates the event value is invalid.
#define | CUPTI_EVENT_OVERFLOW ((uint64_t)0xFFFFFFFFFFFFFFFFULL)
| The overflow value for a CUPTI event.
## Typedefs
typedef uint32_t | CUpti_EventDomainID
| ID for an event domain.
typedef void * | CUpti_EventGroup
| A group of events.
typedef uint32_t | CUpti_EventID
| ID for an event.
typedef void(* | CUpti_KernelReplayUpdateFunc )(const char *kernelName, int numReplaysDone, void *customData)
| Function type for getting updates on kernel replay.
## Enumerations
enum | CUpti_DeviceAttribute { CUPTI_DEVICE_ATTR_MAX_EVENT_ID = 1, CUPTI_DEVICE_ATTR_MAX_EVENT_DOMAIN_ID = 2, CUPTI_DEVICE_ATTR_GLOBAL_MEMORY_BANDWIDTH = 3, CUPTI_DEVICE_ATTR_INSTRUCTION_PER_CYCLE = 4, CUPTI_DEVICE_ATTR_INSTRUCTION_THROUGHPUT_SINGLE_PRECISION = 5, CUPTI_DEVICE_ATTR_MAX_FRAME_BUFFERS = 6, CUPTI_DEVICE_ATTR_PCIE_LINK_RATE = 7, CUPTI_DEVICE_ATTR_PCIE_LINK_WIDTH = 8, CUPTI_DEVICE_ATTR_PCIE_GEN = 9, CUPTI_DEVICE_ATTR_DEVICE_CLASS = 10, CUPTI_DEVICE_ATTR_FLOP_SP_PER_CYCLE = 11, CUPTI_DEVICE_ATTR_FLOP_DP_PER_CYCLE = 12, CUPTI_DEVICE_ATTR_MAX_L2_UNITS = 13, CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_SHARED = 14, CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_L1 = 15, CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_EQUAL = 16, CUPTI_DEVICE_ATTR_FLOP_HP_PER_CYCLE = 17, CUPTI_DEVICE_ATTR_NVLINK_PRESENT = 18, CUPTI_DEVICE_ATTR_GPU_CPU_NVLINK_BW = 19, CUPTI_DEVICE_ATTR_NVSWITCH_PRESENT = 20 }
| Device attributes. More...
enum | CUpti_DeviceAttributeDeviceClass
| Device class. More...
enum | CUpti_EventAttribute { CUPTI_EVENT_ATTR_NAME = 0, CUPTI_EVENT_ATTR_SHORT_DESCRIPTION = 1, CUPTI_EVENT_ATTR_LONG_DESCRIPTION = 2, CUPTI_EVENT_ATTR_CATEGORY = 3, CUPTI_EVENT_ATTR_PROFILING_SCOPE = 5 }
| Event attributes. More...
enum | CUpti_EventCategory { CUPTI_EVENT_CATEGORY_INSTRUCTION = 0, CUPTI_EVENT_CATEGORY_MEMORY = 1, CUPTI_EVENT_CATEGORY_CACHE = 2, CUPTI_EVENT_CATEGORY_PROFILE_TRIGGER = 3, CUPTI_EVENT_CATEGORY_SYSTEM = 4 }
| An event category. More...
enum | CUpti_EventCollectionMethod { CUPTI_EVENT_COLLECTION_METHOD_PM = 0, CUPTI_EVENT_COLLECTION_METHOD_SM = 1, CUPTI_EVENT_COLLECTION_METHOD_INSTRUMENTED = 2, CUPTI_EVENT_COLLECTION_METHOD_NVLINK_TC = 3 }
| The collection method used for an event. More...
enum | CUpti_EventCollectionMode { CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS = 0, CUPTI_EVENT_COLLECTION_MODE_KERNEL = 1 }
| Event collection modes. More...
enum | CUpti_EventDomainAttribute { CUPTI_EVENT_DOMAIN_ATTR_NAME = 0, CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT = 1, CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT = 3, CUPTI_EVENT_DOMAIN_ATTR_COLLECTION_METHOD = 4 }
| Event domain attributes. More...
enum | CUpti_EventGroupAttribute { CUPTI_EVENT_GROUP_ATTR_EVENT_DOMAIN_ID = 0, CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES = 1, CUPTI_EVENT_GROUP_ATTR_USER_DATA = 2, CUPTI_EVENT_GROUP_ATTR_NUM_EVENTS = 3, CUPTI_EVENT_GROUP_ATTR_EVENTS = 4, CUPTI_EVENT_GROUP_ATTR_INSTANCE_COUNT = 5, CUPTI_EVENT_GROUP_ATTR_PROFILING_SCOPE = 6 }
| Event group attributes. More...
enum | CUpti_EventProfilingScope { CUPTI_EVENT_PROFILING_SCOPE_CONTEXT = 0, CUPTI_EVENT_PROFILING_SCOPE_DEVICE = 1, CUPTI_EVENT_PROFILING_SCOPE_BOTH = 2 }
| Profiling scope for event. More...
enum | CUpti_ReadEventFlags { CUPTI_EVENT_READ_FLAG_NONE = 0 }
| Flags for cuptiEventGroupReadEvent an cuptiEventGroupReadAllEvents. More...
## Functions
CUptiResult | cuptiDeviceEnumEventDomains (CUdevice device, size_t *arraySizeBytes, CUpti_EventDomainID *domainArray)
| Get the event domains for a device.
CUptiResult | cuptiDeviceGetAttribute (CUdevice device, CUpti_DeviceAttribute attrib, size_t *valueSize, void *value)
| Read a device attribute.
CUptiResult | cuptiDeviceGetEventDomainAttribute (CUdevice device, CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t *valueSize, void *value)
| Read an event domain attribute.
CUptiResult | cuptiDeviceGetNumEventDomains (CUdevice device, uint32_t *numDomains)
| Get the number of domains for a device.
CUptiResult | cuptiDisableKernelReplayMode (CUcontext context)
| Disable kernel replay mode.
CUptiResult | cuptiEnableKernelReplayMode (CUcontext context)
| Enable kernel replay mode.
CUptiResult | cuptiEnumEventDomains (size_t *arraySizeBytes, CUpti_EventDomainID *domainArray)
| Get the event domains available on any device.
CUptiResult | cuptiEventDomainEnumEvents (CUpti_EventDomainID eventDomain, size_t *arraySizeBytes, CUpti_EventID *eventArray)
| Get the events in a domain.
CUptiResult | cuptiEventDomainGetAttribute (CUpti_EventDomainID eventDomain, CUpti_EventDomainAttribute attrib, size_t *valueSize, void *value)
| Read an event domain attribute.
CUptiResult | cuptiEventDomainGetNumEvents (CUpti_EventDomainID eventDomain, uint32_t *numEvents)
| Get number of events in a domain.
CUptiResult | cuptiEventGetAttribute (CUpti_EventID event, CUpti_EventAttribute attrib, size_t *valueSize, void *value)
| Get an event attribute.
CUptiResult | cuptiEventGetIdFromName (CUdevice device, const char *eventName, CUpti_EventID *event)
| Find an event by name.
CUptiResult | cuptiEventGroupAddEvent (CUpti_EventGroup eventGroup, CUpti_EventID event)
| Add an event to an event group.
CUptiResult | cuptiEventGroupCreate (CUcontext context, CUpti_EventGroup *eventGroup, uint32_t flags)
| Create a new event group for a context.
CUptiResult | cuptiEventGroupDestroy (CUpti_EventGroup eventGroup)
| Destroy an event group.
CUptiResult | cuptiEventGroupDisable (CUpti_EventGroup eventGroup)
| Disable an event group.
CUptiResult | cuptiEventGroupEnable (CUpti_EventGroup eventGroup)
| Enable an event group.
CUptiResult | cuptiEventGroupGetAttribute (CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t *valueSize, void *value)
| Read an event group attribute.
CUptiResult | cuptiEventGroupReadAllEvents (CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, size_t *eventValueBufferSizeBytes, uint64_t *eventValueBuffer, size_t *eventIdArraySizeBytes, CUpti_EventID *eventIdArray, size_t *numEventIdsRead)
| Read the values for all the events in an event group.
CUptiResult | cuptiEventGroupReadEvent (CUpti_EventGroup eventGroup, CUpti_ReadEventFlags flags, CUpti_EventID event, size_t *eventValueBufferSizeBytes, uint64_t *eventValueBuffer)
| Read the value for an event in an event group.
CUptiResult | cuptiEventGroupRemoveAllEvents (CUpti_EventGroup eventGroup)
| Remove all events from an event group.
CUptiResult | cuptiEventGroupRemoveEvent (CUpti_EventGroup eventGroup, CUpti_EventID event)
| Remove an event from an event group.
CUptiResult | cuptiEventGroupResetAllEvents (CUpti_EventGroup eventGroup)
| Zero all the event counts in an event group.
CUptiResult | cuptiEventGroupSetAttribute (CUpti_EventGroup eventGroup, CUpti_EventGroupAttribute attrib, size_t valueSize, void *value)
| Write an event group attribute.
CUptiResult | cuptiEventGroupSetDisable (CUpti_EventGroupSet *eventGroupSet)
| Disable an event group set.
CUptiResult | cuptiEventGroupSetEnable (CUpti_EventGroupSet *eventGroupSet)
| Enable an event group set.
CUptiResult | cuptiEventGroupSetsCreate (CUcontext context, size_t eventIdArraySizeBytes, CUpti_EventID *eventIdArray, CUpti_EventGroupSets **eventGroupPasses)
| For a set of events, get the grouping that indicates the number of passes and the event groups necessary to collect the events.
CUptiResult | cuptiEventGroupSetsDestroy (CUpti_EventGroupSets *eventGroupSets)
| Destroy a event group sets object.
CUptiResult | cuptiGetNumEventDomains (uint32_t *numDomains)
| Get the number of event domains available on any device.
CUptiResult | cuptiKernelReplaySubscribeUpdate (CUpti_KernelReplayUpdateFunc updateFunc, void *customData)
| Subscribe to kernel replay updates.
CUptiResult | cuptiSetEventCollectionMode (CUcontext context, CUpti_EventCollectionMode mode)
| Set the event collection mode.

## Detailed Description

Functions, types, and enums that implement the CUPTI Event API.

Note:
  CUPTI event API from the header cupti_events.h are not supported on devices with compute capability 7.5 and higher (i.e. Turing and later GPU architectures). These API will be deprecated in a future CUDA release. These are replaced by Profiling API in the header cupti_profiler_target.h and Perfworks metrics API in the headers nvperf_host.h and nvperf_target.h which are supported on devices with compute capability 7.0 and higher (i.e. Volta and later GPU architectures).

## Define Documentation

#define CUPTI_EVENT_OVERFLOW ((uint64_t)0xFFFFFFFFFFFFFFFFULL)

The CUPTI event value that indicates an overflow.

## Typedef Documentation

typedef uint32_t CUpti_EventDomainID

ID for an event domain. An event domain represents a group of related events. A device may have multiple instances of a domain, indicating that the device can simultaneously record multiple instances of each event within that domain.

typedef void* CUpti_EventGroup

An event group is a collection of events that are managed together. All events in an event group must belong to the same domain.

typedef uint32_t CUpti_EventID

An event represents a countable activity, action, or occurrence on the device.

typedef void( * CUpti_KernelReplayUpdateFunc)(const char *kernelName, int numReplaysDone, void *customData)

Parameters:

  | kernelName | The mangled kernel name
  | numReplaysDone | Number of replays done so far
  | customData | Pointer of any custom data passed in when subscribing

## Enumeration Type Documentation

enum CUpti_DeviceAttribute

CUPTI device attributes. These attributes can be read using cuptiDeviceGetAttribute.

Enumerator:

  CUPTI_DEVICE_ATTR_MAX_EVENT_ID | Number of event IDs for a device. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_MAX_EVENT_DOMAIN_ID | Number of event domain IDs for a device. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_GLOBAL_MEMORY_BANDWIDTH | Get global memory bandwidth in Kbytes/sec. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_INSTRUCTION_PER_CYCLE | Get theoretical maximum number of instructions per cycle. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_INSTRUCTION_THROUGHPUT_SINGLE_PRECISION | Get theoretical maximum number of single precision instructions that can be executed per second. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_FRAME_BUFFERS | Get number of frame buffers for device. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_LINK_RATE | Get PCIE link rate in Mega bits/sec for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_LINK_WIDTH | Get PCIE link width for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_PCIE_GEN | Get PCIE generation for device. Return 0 if bus-type is non-PCIE. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_DEVICE_CLASS | Get the class for the device. Value is a CUpti_DeviceAttributeDeviceClass.
  CUPTI_DEVICE_ATTR_FLOP_SP_PER_CYCLE | Get the peak single precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_FLOP_DP_PER_CYCLE | Get the peak double precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_L2_UNITS | Get number of L2 units. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_SHARED | Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_SHARED preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_L1 | Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_L1 preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_MAX_SHARED_MEMORY_CACHE_CONFIG_PREFER_EQUAL | Get the maximum shared memory for the CU_FUNC_CACHE_PREFER_EQUAL preference. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_FLOP_HP_PER_CYCLE | Get the peak half precision flop per cycle. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_NVLINK_PRESENT | Check if Nvlink is connected to device. Returns 1, if at least one Nvlink is connected to the device, returns 0 otherwise. Value is a uint32_t.
  CUPTI_DEVICE_ATTR_GPU_CPU_NVLINK_BW | Check if Nvlink is present between GPU and CPU. Returns Bandwidth, in Bytes/sec, if Nvlink is present, returns 0 otherwise. Value is a uint64_t.
  CUPTI_DEVICE_ATTR_NVSWITCH_PRESENT | Check if NVSwitch is present in the underlying topology. Returns 1, if present, returns 0 otherwise. Value is a uint32_t.

enum CUpti_DeviceAttributeDeviceClass

Enumeration of device classes for device attribute CUPTI_DEVICE_ATTR_DEVICE_CLASS.

enum CUpti_EventAttribute

Event attributes. These attributes can be read using cuptiEventGetAttribute.

Enumerator:

  CUPTI_EVENT_ATTR_NAME | Event name. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_SHORT_DESCRIPTION | Short description of event. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_LONG_DESCRIPTION | Long description of event. Value is a null terminated const c-string.
  CUPTI_EVENT_ATTR_CATEGORY | Category of event. Value is CUpti_EventCategory.
  CUPTI_EVENT_ATTR_PROFILING_SCOPE | Profiling scope of the events. It can be either device or context or both. Value is a CUpti_EventProfilingScope.

enum CUpti_EventCategory

Each event is assigned to a category that represents the general type of the event. A event's category is accessed using cuptiEventGetAttribute and the CUPTI_EVENT_ATTR_CATEGORY attribute.

Enumerator:

  CUPTI_EVENT_CATEGORY_INSTRUCTION | An instruction related event.
  CUPTI_EVENT_CATEGORY_MEMORY | A memory related event.
  CUPTI_EVENT_CATEGORY_CACHE | A cache related event.
  CUPTI_EVENT_CATEGORY_PROFILE_TRIGGER | A profile-trigger event.
  CUPTI_EVENT_CATEGORY_SYSTEM | A system event.

enum CUpti_EventCollectionMethod

The collection method indicates how an event is collected.

Enumerator:

  CUPTI_EVENT_COLLECTION_METHOD_PM | Event is collected using a hardware global performance monitor.
  CUPTI_EVENT_COLLECTION_METHOD_SM | Event is collected using a hardware SM performance monitor.
  CUPTI_EVENT_COLLECTION_METHOD_INSTRUMENTED | Event is collected using software instrumentation.
  CUPTI_EVENT_COLLECTION_METHOD_NVLINK_TC | Event is collected using NvLink throughput counter method.

enum CUpti_EventCollectionMode

The event collection mode determines the period over which the events within the enabled event groups will be collected.

Enumerator:

  CUPTI_EVENT_COLLECTION_MODE_CONTINUOUS | Events are collected for the entire duration between the cuptiEventGroupEnable and cuptiEventGroupDisable calls. Event values are reset when the events are read. For CUDA toolkit v6.0 and older this was the default mode.
  CUPTI_EVENT_COLLECTION_MODE_KERNEL | Events are collected only for the durations of kernel executions that occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls. Event collection begins when a kernel execution begins, and stops when kernel execution completes. Event values are reset to zero when each kernel execution begins. If multiple kernel executions occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls then the event values must be read after each kernel launch if those events need to be associated with the specific kernel launch. Note that collection in this mode may significantly change the overall performance characteristics of the application because kernel executions that occur between the cuptiEventGroupEnable and cuptiEventGroupDisable calls are serialized on the GPU. This is the default mode from CUDA toolkit v6.5

enum CUpti_EventDomainAttribute

Event domain attributes. Except where noted, all the attributes can be read using either cuptiDeviceGetEventDomainAttribute or cuptiEventDomainGetAttribute.

Enumerator:

  CUPTI_EVENT_DOMAIN_ATTR_NAME | Event domain name. Value is a null terminated const c-string.
  CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT | Number of instances of the domain for which event counts will be collected. The domain may have additional instances that cannot be profiled (see CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT). Can be read only with cuptiDeviceGetEventDomainAttribute. Value is a uint32_t.
  CUPTI_EVENT_DOMAIN_ATTR_TOTAL_INSTANCE_COUNT | Total number of instances of the domain, including instances that cannot be profiled. Use CUPTI_EVENT_DOMAIN_ATTR_INSTANCE_COUNT to get the number of instances that can be profiled. Can be read only with cuptiDeviceGetEventDomainAttribute. Value is a uint32_t.
  CUPTI_EVENT_DOMAIN_ATTR_COLLECTION_METHOD | Collection method used for events contained in the event domain. Value is a CUpti_EventCollectionMethod.

enum CUpti_EventGroupAttribute

Event group attributes. These attributes can be read using cuptiEventGroupGetAttribute. Attributes marked [rw] can also be written using cuptiEventGroupSetAttribute.

Enumerator:

  CUPTI_EVENT_GROUP_ATTR_EVENT_DOMAIN_ID | The domain to which the event group is bound. This attribute is set when the first event is added to the group. Value is a CUpti_EventDomainID.
  CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES | [rw] Profile all the instances of the domain for this eventgroup. This feature can be used to get load balancing across all instances of a domain. Value is an integer.
  CUPTI_EVENT_GROUP_ATTR_USER_DATA | [rw] Reserved for user data.
  CUPTI_EVENT_GROUP_ATTR_NUM_EVENTS | Number of events in the group. Value is a uint32_t.
  CUPTI_EVENT_GROUP_ATTR_EVENTS | Enumerates events in the group. Value is a pointer to buffer of size sizeof(CUpti_EventID) * num_of_events in the eventgroup. num_of_events can be queried using CUPTI_EVENT_GROUP_ATTR_NUM_EVENTS.
  CUPTI_EVENT_GROUP_ATTR_INSTANCE_COUNT | Number of instances of the domain bound to this event group that will be counted. Value is a uint32_t.
  CUPTI_EVENT_GROUP_ATTR_PROFILING_SCOPE | Event group scope can be set to CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT for an eventGroup, before adding any event. Sets the scope of eventgroup as CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT when the scope of the events that will be added is CUPTI_EVENT_PROFILING_SCOPE_BOTH. If profiling scope of event is either CUPTI_EVENT_PROFILING_SCOPE_DEVICE or CUPTI_EVENT_PROFILING_SCOPE_CONTEXT then setting this attribute will not affect the default scope. It is not allowed to add events of different scope to same eventgroup. Value is a uint32_t.

enum CUpti_EventProfilingScope

Profiling scope of event indicates if the event can be collected at context scope or device scope or both i.e. it can be collected at any of context or device scope.

Enumerator:

  CUPTI_EVENT_PROFILING_SCOPE_CONTEXT | Event is collected at context scope.
  CUPTI_EVENT_PROFILING_SCOPE_DEVICE | Event is collected at device scope.
  CUPTI_EVENT_PROFILING_SCOPE_BOTH | Event can be collected at device or context scope. The scope can be set using cuptiEventGroupSetAttribute API.

enum CUpti_ReadEventFlags

Flags for cuptiEventGroupReadEvent an cuptiEventGroupReadAllEvents.

Enumerator:

  CUPTI_EVENT_READ_FLAG_NONE | No flags.

## Function Documentation

CUptiResult cuptiDeviceEnumEventDomains | ( | CUdevice | device,
|  | size_t * | arraySizeBytes,
|  | CUpti_EventDomainID * | domainArray |
| ) |  |  |

Returns the event domains IDs in `domainArray` for a device. The size of the `domainArray` buffer is given by `*arraySizeBytes`. The size of the `domainArray` buffer must be at least `numdomains` * sizeof(CUpti_EventDomainID) or else all domains will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `domainArray`.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | device | The CUDA device
  | arraySizeBytes | The size of `domainArray` in bytes, and returns the number of bytes written to `domainArray`
  | domainArray | Returns the IDs of the event domains for the device

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_DEVICE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `arraySizeBytes` or `domainArray` are NULL

CUptiResult cuptiDeviceGetAttribute | ( | CUdevice | device,
|  | CUpti_DeviceAttribute | attrib,
|  | size_t * | valueSize,
|  | void * | value |
| ) |  |  |

Read a device attribute and return it in `*value`.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | device | The CUDA device
  | attrib | The attribute to read
  | valueSize | Size of buffer pointed by the value, and returns the number of bytes written to `value`
  | value | Returns the value of the attribute

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_DEVICE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not a device attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiDeviceGetEventDomainAttribute | ( | CUdevice | device,
|  | CUpti_EventDomainID | eventDomain,
|  | CUpti_EventDomainAttribute | attrib,
|  | size_t * | valueSize,
|  | void * | value |
| ) |  |  |

Returns an event domain attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | device | The CUDA device
  | eventDomain | ID of the event domain
  | attrib | The event domain attribute to read
  | valueSize | The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  | value | Returns the attribute's value

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_DEVICE |
  | CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not an event domain attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiDeviceGetNumEventDomains | ( | CUdevice | device,
|  | uint32_t * | numDomains |
| ) |  |  |

Returns the number of domains in `numDomains` for a device.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | device | The CUDA device
  | numDomains | Returns the number of domains

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_DEVICE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `numDomains` is NULL

CUptiResult cuptiDisableKernelReplayMode | ( | CUcontext | context | ) |

Set profiling mode for the context to non-replay (default) mode. Event collection mode will be set to CUPTI_EVENT_COLLECTION_MODE_KERNEL. All previously enabled event groups and event group sets will be disabled.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | context | The context

Return values:

  | CUPTI_SUCCESS |

CUptiResult cuptiEnableKernelReplayMode | ( | CUcontext | context | ) |

Set profiling mode for the context to replay mode. In this mode, any number of events can be collected in one run of the kernel. The event collection mode will automatically switch to CUPTI_EVENT_COLLECTION_MODE_KERNEL. In this mode, cuptiSetEventCollectionMode will return CUPTI_ERROR_INVALID_OPERATION.

Note:
  Kernels might take longer to run if many events are enabled.

  Thread-safety: this function is thread safe.

Parameters:

  | context | The context

Return values:

  | CUPTI_SUCCESS |

CUptiResult cuptiEnumEventDomains | ( | size_t * | arraySizeBytes,
|  | CUpti_EventDomainID * | domainArray |
| ) |  |  |

Returns all the event domains available on any CUDA-capable device. Event domain IDs are returned in `domainArray`. The size of the `domainArray` buffer is given by `*arraySizeBytes`. The size of the `domainArray` buffer must be at least `numDomains` * sizeof(CUpti_EventDomainID) or all domains will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `domainArray`.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | arraySizeBytes | The size of `domainArray` in bytes, and returns the number of bytes written to `domainArray`
  | domainArray | Returns all the event domains

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_INVALID_PARAMETER | if `arraySizeBytes` or `domainArray` are NULL

CUptiResult cuptiEventDomainEnumEvents | ( | CUpti_EventDomainID | eventDomain,
|  | size_t * | arraySizeBytes,
|  | CUpti_EventID * | eventArray |
| ) |  |  |

Returns the event IDs in `eventArray` for a domain. The size of the `eventArray` buffer is given by `*arraySizeBytes`. The size of the `eventArray` buffer must be at least `numdomainevents` * sizeof(CUpti_EventID) or else all events will not be returned. The value returned in `*arraySizeBytes` contains the number of bytes returned in `eventArray`.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventDomain | ID of the event domain
  | arraySizeBytes | The size of `eventArray` in bytes, and returns the number of bytes written to `eventArray`
  | eventArray | Returns the IDs of the events in the domain

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `arraySizeBytes` or `eventArray` are NULL

CUptiResult cuptiEventDomainGetAttribute | ( | CUpti_EventDomainID | eventDomain,
|  | CUpti_EventDomainAttribute | attrib,
|  | size_t * | valueSize,
|  | void * | value |
| ) |  |  |

Returns an event domain attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventDomain | ID of the event domain
  | attrib | The event domain attribute to read
  | valueSize | The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  | value | Returns the attribute's value

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not an event domain attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiEventDomainGetNumEvents | ( | CUpti_EventDomainID | eventDomain,
|  | uint32_t * | numEvents |
| ) |  |  |

Returns the number of events in `numEvents` for a domain.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventDomain | ID of the event domain
  | numEvents | Returns the number of events in the domain

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_DOMAIN_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `numEvents` is NULL

CUptiResult cuptiEventGetAttribute | ( | CUpti_EventID | event,
|  | CUpti_EventAttribute | attrib,
|  | size_t * | valueSize,
|  | void * | value |
| ) |  |  |

Returns an event attribute in `*value`. The size of the `value` buffer is given by `*valueSize`. The value returned in `*valueSize` contains the number of bytes returned in `value`.

If the attribute value is a c-string that is longer than `*valueSize`, then only the first `*valueSize` characters will be returned and there will be no terminating null byte.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | event | ID of the event
  | attrib | The event attribute to read
  | valueSize | The size of the `value` buffer in bytes, and returns the number of bytes written to `value`
  | value | Returns the attribute's value

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not an event attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiEventGetIdFromName | ( | CUdevice | device,
|  | const char * | eventName,
|  | CUpti_EventID * | event |
| ) |  |  |

Find an event by name and return the event ID in `*event`.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | device | The CUDA device
  | eventName | The name of the event to find
  | event | Returns the ID of the found event or undefined if unable to find the event

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_DEVICE |
  | CUPTI_ERROR_INVALID_EVENT_NAME | if unable to find an event with name `eventName`. In this case `*event` is undefined
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventName` or `event` are NULL

CUptiResult cuptiEventGroupAddEvent | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_EventID | event |
| ) |  |  |

Add an event to an event group. The event add can fail for a number of reasons:

- The event group is enabled
- The event does not belong to the same event domain as the events that are already in the event group
- Device limitations on the events that can belong to the same group
- The event group is full

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group
  | event | The event to add to the group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_ID |
  | CUPTI_ERROR_OUT_OF_MEMORY |
  | CUPTI_ERROR_INVALID_OPERATION | if `eventGroup` is enabled
  | CUPTI_ERROR_NOT_COMPATIBLE | if `event` belongs to a different event domain than the events already in `eventGroup`, or if a device limitation prevents `event` from being collected at the same time as the events already in `eventGroup`
  | CUPTI_ERROR_MAX_LIMIT_REACHED | if `eventGroup` is full
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupCreate | ( | CUcontext | context,
|  | CUpti_EventGroup * | eventGroup,
|  | uint32_t | flags |
| ) |  |  |

Creates a new event group for `context` and returns the new group in `*eventGroup`.

Note:
  `flags` are reserved for future use and should be set to zero.

  Thread-safety: this function is thread safe.

Parameters:

  | context | The context for the event group
  | eventGroup | Returns the new event group
  | flags | Reserved - must be zero

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_CONTEXT |
  | CUPTI_ERROR_OUT_OF_MEMORY |
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupDestroy | ( | CUpti_EventGroup | eventGroup | ) |

Destroy an `eventGroup` and free its resources. An event group cannot be destroyed if it is enabled.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group to destroy

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_OPERATION | if the event group is enabled
  | CUPTI_ERROR_INVALID_PARAMETER | if eventGroup is NULL

CUptiResult cuptiEventGroupDisable | ( | CUpti_EventGroup | eventGroup | ) |

Disable an event group. Disabling an event group stops collection of events contained in the group.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupEnable | ( | CUpti_EventGroup | eventGroup | ) |

Enable an event group. Enabling an event group zeros the value of all the events in the group and then starts collection of those events.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_NOT_READY | if `eventGroup` does not contain any events
  | CUPTI_ERROR_NOT_COMPATIBLE | if `eventGroup` cannot be enabled due to other already enabled event groups
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL
  | CUPTI_ERROR_HARDWARE_BUSY | if another client is profiling and hardware is busy

CUptiResult cuptiEventGroupGetAttribute | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_EventGroupAttribute | attrib,
|  | size_t * | valueSize,
|  | void * | value |
| ) |  |  |

Read an event group attribute and return it in `*value`.

Note:
  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.).

Parameters:

  | eventGroup | The event group
  | attrib | The attribute to read
  | valueSize | Size of buffer pointed by the value, and returns the number of bytes written to `value`
  | value | Returns the value of the attribute

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not an eventgroup attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | For non-c-string attribute values, indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiEventGroupReadAllEvents | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_ReadEventFlags | flags,
|  | size_t * | eventValueBufferSizeBytes,
|  | uint64_t * | eventValueBuffer,
|  | size_t * | eventIdArraySizeBytes,
|  | CUpti_EventID * | eventIdArray,
|  | size_t * | numEventIdsRead |
| ) |  |  |

Read the values for all the events in an event group. The event values are returned in the `eventValueBuffer` buffer. `eventValueBufferSizeBytes` indicates the size of `eventValueBuffer`. The buffer must be at least (sizeof(uint64) * number of events in group) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is not set on the group containing the events. The buffer must be at least (sizeof(uint64) * number of domain instances * number of events in group) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is set on the group.

The data format returned in `eventValueBuffer` is:

- domain instance 0: event0 event1 ... eventN
- domain instance 1: event0 event1 ... eventN
- ...
- domain instance M: event0 event1 ... eventN

The event order in `eventValueBuffer` is returned in `eventIdArray`. The size of `eventIdArray` is specified in `eventIdArraySizeBytes`. The size should be at least (sizeof(CUpti_EventID) * number of events in group).

If any instance of any event counter overflows, the value returned for that event instance will be CUPTI_EVENT_OVERFLOW.

The only allowed value for `flags` is CUPTI_EVENT_READ_FLAG_NONE.

Reading events from a disabled event group is not allowed. After being read, an event's value is reset to zero.

Note:
  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.). If cuptiEventGroupResetAllEvents is called simultaneously with this function, then returned event values are undefined.

Parameters:

  | eventGroup | The event group
  | flags | Flags controlling the reading mode
  | eventValueBufferSizeBytes | The size of `eventValueBuffer` in bytes, and returns the number of bytes written to `eventValueBuffer`
  | eventValueBuffer | Returns the event values
  | eventIdArraySizeBytes | The size of `eventIdArray` in bytes, and returns the number of bytes written to `eventIdArray`
  | eventIdArray | Returns the IDs of the events in the same order as the values return in eventValueBuffer.
  | numEventIdsRead | Returns the number of event IDs returned in `eventIdArray`

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_INVALID_OPERATION | if `eventGroup` is disabled
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup`, `eventValueBufferSizeBytes`, `eventValueBuffer`, `eventIdArraySizeBytes`, `eventIdArray` or `numEventIdsRead` is NULL
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | if size of `eventValueBuffer` or `eventIdArray` is not sufficient

CUptiResult cuptiEventGroupReadEvent | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_ReadEventFlags | flags,
|  | CUpti_EventID | event,
|  | size_t * | eventValueBufferSizeBytes,
|  | uint64_t * | eventValueBuffer |
| ) |  |  |

Read the value for an event in an event group. The event value is returned in the `eventValueBuffer` buffer. `eventValueBufferSizeBytes` indicates the size of the `eventValueBuffer` buffer. The buffer must be at least sizeof(uint64) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is not set on the group containing the event. The buffer must be at least (sizeof(uint64) * number of domain instances) if CUPTI_EVENT_GROUP_ATTR_PROFILE_ALL_DOMAIN_INSTANCES is set on the group.

If any instance of an event counter overflows, the value returned for that event instance will be CUPTI_EVENT_OVERFLOW.

The only allowed value for `flags` is CUPTI_EVENT_READ_FLAG_NONE.

Reading an event from a disabled event group is not allowed. After being read, an event's value is reset to zero.

Note:
  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.). If cuptiEventGroupResetAllEvents is called simultaneously with this function, then returned event values are undefined.

Parameters:

  | eventGroup | The event group
  | flags | Flags controlling the reading mode
  | event | The event to read
  | eventValueBufferSizeBytes | The size of `eventValueBuffer` in bytes, and returns the number of bytes written to `eventValueBuffer`
  | eventValueBuffer | Returns the event value(s)

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_ID |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_INVALID_OPERATION | if `eventGroup` is disabled
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup`, `eventValueBufferSizeBytes` or `eventValueBuffer` is NULL
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | if size of `eventValueBuffer` is not sufficient

CUptiResult cuptiEventGroupRemoveAllEvents | ( | CUpti_EventGroup | eventGroup | ) |

Remove all events from an event group. Events cannot be removed if the event group is enabled.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_OPERATION | if `eventGroup` is enabled
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupRemoveEvent | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_EventID | event |
| ) |  |  |

Remove `event` from the an event group. The event cannot be removed if the event group is enabled.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group
  | event | The event to remove from the group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_EVENT_ID |
  | CUPTI_ERROR_INVALID_OPERATION | if `eventGroup` is enabled
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupResetAllEvents | ( | CUpti_EventGroup | eventGroup | ) |

Zero all the event counts in an event group.

Note:
  Thread-safety: this function is thread safe but client must guard against simultaneous destruction or modification of `eventGroup` (for example, client must guard against simultaneous calls to cuptiEventGroupDestroy, cuptiEventGroupAddEvent, etc.), and must guard against simultaneous destruction of the context in which `eventGroup` was created (for example, client must guard against simultaneous calls to cudaDeviceReset, cuCtxDestroy, etc.).

Parameters:

  | eventGroup | The event group

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroup` is NULL

CUptiResult cuptiEventGroupSetAttribute | ( | CUpti_EventGroup | eventGroup,
|  | CUpti_EventGroupAttribute | attrib,
|  | size_t | valueSize,
|  | void * | value |
| ) |  |  |

Write an event group attribute.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroup | The event group
  | attrib | The attribute to write
  | valueSize | The size, in bytes, of the value
  | value | The attribute value to write

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_PARAMETER | if `valueSize` or `value` is NULL, or if `attrib` is not an event group attribute, or if `attrib` is not a writable attribute
  | CUPTI_ERROR_PARAMETER_SIZE_NOT_SUFFICIENT | Indicates that the `value` buffer is too small to hold the attribute value.

CUptiResult cuptiEventGroupSetDisable | ( | CUpti_EventGroupSet * | eventGroupSet | ) |

Disable a set of event groups. Disabling a set of event groups stops collection of events contained in the groups.

Note:
  Thread-safety: this function is thread safe.

  If this call fails, some of the event groups in the set may be disabled and other event groups may remain enabled.

Parameters:

  | eventGroupSet | The pointer to the event group set

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroupSet` is NULL

CUptiResult cuptiEventGroupSetEnable | ( | CUpti_EventGroupSet * | eventGroupSet | ) |

Enable a set of event groups. Enabling a set of event groups zeros the value of all the events in all the groups and then starts collection of those events.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroupSet | The pointer to the event group set

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_HARDWARE |
  | CUPTI_ERROR_NOT_READY | if `eventGroup` does not contain any events
  | CUPTI_ERROR_NOT_COMPATIBLE | if `eventGroup` cannot be enabled due to other already enabled event groups
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroupSet` is NULL
  | CUPTI_ERROR_HARDWARE_BUSY | if other client is profiling and hardware is busy

CUptiResult cuptiEventGroupSetsCreate | ( | CUcontext | context,
|  | size_t | eventIdArraySizeBytes,
|  | CUpti_EventID * | eventIdArray,
|  | CUpti_EventGroupSets ** | eventGroupPasses |
| ) |  |  |

The number of events that can be collected simultaneously varies by device and by the type of the events. When events can be collected simultaneously, they may need to be grouped into multiple event groups because they are from different event domains. This function takes a set of events and determines how many passes are required to collect all those events, and which events can be collected simultaneously in each pass.

The CUpti_EventGroupSets returned in `eventGroupPasses` indicates how many passes are required to collect the events with the `numSets` field. Within each event group set, the `sets` array indicates the event groups that should be collected on each pass.

Note:
  Thread-safety: this function is thread safe, but client must guard against another thread simultaneously destroying `context`.

Parameters:

  | context | The context for event collection
  | eventIdArraySizeBytes | Size of `eventIdArray` in bytes
  | eventIdArray | Array of event IDs that need to be grouped
  | eventGroupPasses | Returns a CUpti_EventGroupSets object that indicates the number of passes required to collect the events and the events to collect on each pass

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_CONTEXT |
  | CUPTI_ERROR_INVALID_EVENT_ID |
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventIdArray` or `eventGroupPasses` is NULL

CUptiResult cuptiEventGroupSetsDestroy | ( | CUpti_EventGroupSets * | eventGroupSets | ) |

Destroy a CUpti_EventGroupSets object.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | eventGroupSets | The object to destroy

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_OPERATION | if any of the event groups contained in the sets is enabled
  | CUPTI_ERROR_INVALID_PARAMETER | if `eventGroupSets` is NULL

CUptiResult cuptiGetNumEventDomains | ( | uint32_t * | numDomains | ) |

Returns the total number of event domains available on any CUDA-capable device.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | numDomains | Returns the number of domains

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_INVALID_PARAMETER | if `numDomains` is NULL

CUptiResult cuptiKernelReplaySubscribeUpdate | ( | CUpti_KernelReplayUpdateFunc | updateFunc,
|  | void * | customData |
| ) |  |  |

When subscribed, the function pointer passed in will be called each time a kernel run is finished during kernel replay. Previously subscribed function pointer will be replaced. Pass in NULL as the function pointer unsubscribes the update.

Parameters:

  | updateFunc | The update function pointer
  | customData | Pointer to any custom data

Return values:

  | CUPTI_SUCCESS |

CUptiResult cuptiSetEventCollectionMode | ( | CUcontext | context,
|  | CUpti_EventCollectionMode | mode |
| ) |  |  |

Set the event collection mode for a `context`. The `mode` controls the event collection behavior of all events in event groups created in the `context`. This API is invalid in kernel replay mode.

Note:
  Thread-safety: this function is thread safe.

Parameters:

  | context | The context
  | mode | The event collection mode

Return values:

  | CUPTI_SUCCESS |
  | CUPTI_ERROR_NOT_INITIALIZED |
  | CUPTI_ERROR_INVALID_CONTEXT |
  | CUPTI_ERROR_INVALID_OPERATION | if called when replay mode is enabled
  | CUPTI_ERROR_NOT_SUPPORTED | if mode is not supported on the device