# 6.55. CUpti_ActivityMemory

struct CUpti_ActivityMemory

  The activity record for memory.

  This activity record represents a memory allocation and free operation (CUPTI_ACTIVITY_KIND_MEMORY). This activity record provides a single record for the memory allocation and memory release operations.

  Note: It is recommended to move to the new activity record CUpti_ActivityMemory3 enabled using the kind CUPTI_ACTIVITY_KIND_MEMORY2. CUpti_ActivityMemory3 provides separate records for memory allocation and memory release operations. This allows to correlate the corresponding driver and runtime API activity record with the memory operation.

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_MEMORY.

  CUpti_ActivityMemoryKind memoryKind

    The memory kind requested by the user.

  uint64_t address

    The virtual address of the allocation.

  uint64_t bytes

    The number of bytes of memory allocated.

  uint64_t start

    The start timestamp for the memory operation, i.e.

    the time when memory was allocated, in ns.

  uint64_t end

    The end timestamp for the memory operation, i.e.

    the time when memory was freed, in ns. This will be 0 if memory is not freed in the application

  uint64_t allocPC

    The program counter of the allocation of memory.

  uint64_t freePC

    The program counter of the freeing of memory.

    This will be 0 if memory is not freed in the application

  uint32_t processId

    The ID of the process to which this record belongs to.

  uint32_t deviceId

    The ID of the device where the memory allocation is taking place.

  uint32_t contextId

    The ID of the context.

    If context is NULL, `contextId` is set to CUPTI_INVALID_CONTEXT_ID.

  uint32_t pad

    Undefined.

    Reserved for internal use.

  const char *name

    Variable name.

    This name is shared across all activity records representing the same symbol, and so should not be modified.