# 6.95. CUpti_ActivityUnifiedMemoryCounterConfig

struct CUpti_ActivityUnifiedMemoryCounterConfig

  Unified Memory counters configuration structure.

  This structure controls the enable/disable of the various Unified Memory counters consisting of scope, kind and other parameters. See function cuptiActivityConfigureUnifiedMemoryCounter

  Public Members

  CUpti_ActivityUnifiedMemoryCounterScope scope

    Unified Memory counter Counter scope.

    (deprecated in CUDA 7.0)

  CUpti_ActivityUnifiedMemoryCounterKind kind

    Unified Memory counter Counter kind.

  uint32_t deviceId

    Device id of the target device.

    This is relevant only for single device scopes. (deprecated in CUDA 7.0)

  uint32_t enable

    Control to enable/disable the counter.

    To enable the counter set it to non-zero value while disable is indicated by zero.