# 6.37. CUpti_ActivityKernel3

struct CUpti_ActivityKernel3

  The activity record for a kernel (CUDA 6.5(with sm_52 support) onwards).

  (deprecated in CUDA 9.0)

  This activity record represents a kernel execution (CUPTI_ACTIVITY_KIND_KERNEL and CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL). Kernel activities are now reported using the CUpti_ActivityKernel9 activity record.

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_KERNEL or CUPTI_ACTIVITY_KIND_CONCURRENT_KERNEL.

  uint8_t requested

    The cache configuration requested by the kernel.

    The value is one of the CUfunc_cache enumeration values from cuda.h.

  uint8_t executed

    The cache configuration used for the kernel.

    The value is one of the CUfunc_cache enumeration values from cuda.h.

  uint8_t sharedMemoryConfig

    The shared memory configuration used for the kernel.

    The value is one of the CUsharedconfig enumeration values from cuda.h.

  uint16_t registersPerThread

    The number of registers required for each thread executing the kernel.

  CUpti_ActivityPartitionedGlobalCacheConfig partitionedGlobalCacheRequested

    The partitioned global caching requested for the kernel.

    Partitioned global caching is required to enable caching on certain chips, such as devices with compute capability 5.2.

  CUpti_ActivityPartitionedGlobalCacheConfig partitionedGlobalCacheExecuted

    The partitioned global caching executed for the kernel.

    Partitioned global caching is required to enable caching on certain chips, such as devices with compute capability 5.2. Partitioned global caching can be automatically disabled if the occupancy requirement of the launch cannot support caching.

  uint64_t start

    The start timestamp for the kernel execution, in ns.

    A value of 0 for both the start and end timestamps indicates that timestamp information could not be collected for the kernel.

  uint64_t end

    The end timestamp for the kernel execution, in ns.

    A value of 0 for both the start and end timestamps indicates that timestamp information could not be collected for the kernel.

  uint64_t completed

    The completed timestamp for the kernel execution, in ns.

    It represents the completion of all it’s child kernels and the kernel itself. A value of CUPTI_TIMESTAMP_UNKNOWN indicates that the completion time is unknown.

  uint32_t deviceId

    The ID of the device where the kernel is executing.

  uint32_t contextId

    The ID of the context where the kernel is executing.

  uint32_t streamId

    The ID of the stream where the kernel is executing.

  int32_t gridX

    The X-dimension grid size for the kernel.

  int32_t gridY

    The Y-dimension grid size for the kernel.

  int32_t gridZ

    The Z-dimension grid size for the kernel.

  int32_t blockX

    The X-dimension block size for the kernel.

  int32_t blockY

    The Y-dimension block size for the kernel.

  int32_t blockZ

    The Z-dimension grid size for the kernel.

  int32_t staticSharedMemory

    The static shared memory allocated for the kernel, in bytes.

  int32_t dynamicSharedMemory

    The dynamic shared memory reserved for the kernel, in bytes.

  uint32_t localMemoryPerThread

    The amount of local memory reserved for each thread, in bytes.

  uint32_t localMemoryTotal

    The total amount of local memory reserved for the kernel, in bytes.

  uint32_t correlationId

    The correlation ID of the kernel.

    Each kernel execution is assigned a unique correlation ID that is identical to the correlation ID in the driver or runtime API activity record that launched the kernel.

  int64_t gridId

    The grid ID of the kernel.

    Each kernel is assigned a unique grid ID at runtime.

  const char *name

    The name of the kernel.

    This name is shared across all activity records representing the same kernel, and so should not be modified.

  void *reserved0

    Undefined.

    Reserved for internal use.