# 6.143. CUpti_Profiler_DeviceSupported_Params

struct CUpti_Profiler_DeviceSupported_Params

  Params for cuptiProfilerDeviceSupported.

  Public Members

  size_t structSize

    [in] Must be CUpti_Profiler_DeviceSupported_Params_STRUCT_SIZE

  void *pPriv

    [in] assign to NULL

  CUdevice cuDevice

    [in] if NULL, the current CUcontext is used

  CUpti_Profiler_Support_Level isSupported

    [out] overall SUPPORTED / UNSUPPORTED flag representing whether Profiling and PC Sampling APIs work on the given device and configuration. SUPPORTED if all following flags are SUPPORTED, UNSUPPORTED otherwise.

  CUpti_Profiler_Support_Level architecture

    [out] SUPPORTED if the device architecture level supports the Profiling API (Compute Capability >= 7.0), UNSUPPORTED otherwise

  CUpti_Profiler_Support_Level sli

    [out] SUPPORTED if SLI is not enabled, UNSUPPORTED otherwise

  CUpti_Profiler_Support_Level vGpu

    [out] SUPPORTED if vGPU is supported and profiling is enabled, DISABLED if profiling is supported but not enabled, UNSUPPORTED otherwise

  CUpti_Profiler_Support_Level confidentialCompute

    [out] SUPPORTED if confidential compute is not enabled, UNSUPPORTED otherwise

  CUpti_Profiler_Support_Level cmp

    [out] SUPPORTED if not NVIDIA Crypto Mining Processors (CMP), UNSUPPORTED otherwise

  CUpti_Profiler_Support_Level wsl

    [out] SUPPORTED if WSL supported, UNSUPPORTED otherwise

  CUpti_Profiler_API api

    [in] the CUPTI API type for which device support will be checked