# 6.50. CUpti_ActivityMarkerData2

struct CUpti_ActivityMarkerData2

  The activity record providing detailed information for a marker.

  User must enable CUPTI_ACTIVITY_KIND_MARKER as well to get records for marker data. The marker data contains color, payload, and category. (CUPTI_ACTIVITY_KIND_MARKER_DATA).

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_MARKER_DATA.

  CUpti_ActivityFlag flags

    The flags associated with the marker.

    See also

    CUpti_ActivityFlag

  uint32_t id

    The marker ID.

  CUpti_MetricValueKind payloadKind

    Defines the payload format for the value associated with the marker.

  CUpti_MetricValue payload

    The payload value.

  uint32_t color

    The color for the marker.

  uint32_t category

    The category for the marker.

  uint32_t cuptiDomainId

    CUPTI maintained domain id required for NVTX extended payloads.

    To parse the payload correctly, the domain id must be used to identify the payload attributes as they are domain specific.

  uint32_t padding

    Reserved for internal use.