Skip to main content
`Ctrl`+`K`

# 7.92. CUpti_ActivityNvLink5

struct CUpti_ActivityNvLink5

  NVLink information.

  This structure gives capabilities of each logical NVLink connection between two devices, gpu<->gpu or gpu<->CPU which can be used to understand the topology.

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_NVLINK.

  uint32_t nvlinkVersion

    NvLink version.

  CUpti_DevType typeDev0

    Type of device 0 CUpti_DevType.

  CUpti_DevType typeDev1

    Type of device 1 CUpti_DevType.

  uint32_t index

    Index of the NPU.

    First index will always be zero.

  uint32_t domainId

    Domain ID of NPU.

    On Linux, this can be queried using lspci.

  union CUpti_ActivityNvLink5::[anonymous] idDev0

    If typeDev0 is CUPTI_DEV_TYPE_GPU, UUID for device 0.

    CUpti_ActivityDevice6. If typeDev0 is CUPTI_DEV_TYPE_NPU, struct npu for NPU.

  union CUpti_ActivityNvLink5::[anonymous] idDev1

    If typeDev1 is CUPTI_DEV_TYPE_GPU, UUID for device 1.

    CUpti_ActivityDevice6. If typeDev1 is CUPTI_DEV_TYPE_NPU, struct npu for NPU.

  uint32_t flag

    Flag gives capabilities of the link.

    See also

    CUpti_LinkFlag

  uint32_t physicalNvLinkCount

    Number of physical NVLinks present between two devices.

  uint32_t *portDev0

    Port numbers for NVLinks connected to device 0.

    If typeDev0 is CUPTI_DEV_TYPE_NPU, ignore this field. In case of invalid/unknown port number, this field will be set to value CUPTI_NVLINK_INVALID_PORT. This will be used to correlate the metric values to individual physical link and attribute traffic to the logical NVLink in the topology. CUPTI dynamically allocates memory using the malloc() function for physicalNvLinkCount ports. Client is responsible for freeing this memory using the free() function when done.

  uint32_t *portDev1

    Port numbers for NVLinks connected to device 1.

    If typeDev1 is CUPTI_DEV_TYPE_NPU, ignore this field. In case of invalid/unknown port number, this field will be set to value CUPTI_NVLINK_INVALID_PORT. This will be used to correlate the metric values to individual physical link and attribute traffic to the logical NVLink in the topology. CUPTI dynamically allocates memory using the malloc() function for physicalNvLinkCount ports. Client is responsible for freeing this memory using the free() function when done.

  uint64_t bandwidth

    Bandwidth of NVLink in kbytes/sec.

  uint8_t nvswitchConnected

    NVSwitch is connected as an intermediate node.

  uint8_t pad[7]

    Undefined.

    reserved for internal use