Skip to main content
`Ctrl`+`K`

# 7.3. CUpti_ActivityAutoBoostState

struct CUpti_ActivityAutoBoostState

  Device auto boost state structure.

  This structure defines auto boost state for a device. See function cuptiGetAutoBoostState

  Public Members

  uint32_t enabled

    Returned auto boost state.

    1 is returned in case auto boost is enabled, 0 otherwise

  uint32_t pid

    Id of process that has set the current boost state.

    The value will be CUPTI_AUTO_BOOST_INVALID_CLIENT_PID if the user does not have the permission to query process ids or there is an error in querying the process id.