Skip to main content
`Ctrl`+`K`

# 7.94. CUpti_ActivityOpenAcc

struct CUpti_ActivityOpenAcc

  The base activity record for OpenAcc records.

  The OpenACC activity API part uses a CUpti_ActivityOpenAcc as a generic representation for any OpenACC activity. The ‘kind’ field is used to determine the specific activity kind, and from that the CUpti_ActivityOpenAcc object can be cast to the specific OpenACC activity record type appropriate for that kind.

  Note that all OpenACC activity record types are padded and aligned to ensure that each member of the record is naturally aligned.

  See also

  CUpti_ActivityKind

  Public Members

  CUpti_ActivityKind kind

    The kind of this activity.

  CUpti_OpenAccEventKind eventKind

    CUPTI OpenACC event kind (.

    See also

    CUpti_OpenAccEventKind)

  CUpti_OpenAccConstructKind parentConstruct

    CUPTI OpenACC parent construct kind (.

    Note that for applications using PGI OpenACC runtime < 16.1, this will always be CUPTI_OPENACC_CONSTRUCT_KIND_UNKNOWN.

    See also

    CUpti_OpenAccConstructKind)

  uint32_t version

    Version number.

  uint32_t implicit

    1 for any implicit event, such as an implicit wait at a synchronous data construct 0 otherwise

  uint32_t deviceType

    Device type.

  uint32_t deviceNumber

    Device number.

  uint32_t threadId

    ThreadId.

  uint64_t async

    Value of async() clause of the corresponding directive.

  uint64_t asyncMap

    Internal asynchronous queue number used.

  uint32_t lineNo

    The line number of the directive or program construct or the starting line number of the OpenACC construct corresponding to the event.

    A zero value means the line number is not known.

  uint32_t endLineNo

    For an OpenACC construct, this contains the line number of the end of the construct.

    A zero value means the line number is not known.

  uint32_t funcLineNo

    The line number of the first line of the function named in funcName.

    A zero value means the line number is not known.

  uint32_t funcEndLineNo

    The last line number of the function named in funcName.

    A zero value means the line number is not known.

  uint64_t start

    CUPTI start timestamp.

  uint64_t end

    CUPTI end timestamp.

  uint32_t cuDeviceId

    CUDA device id Valid only if deviceType is acc_device_nvidia.

  uint32_t cuContextId

    CUDA context id Valid only if deviceType is acc_device_nvidia.

  uint32_t cuStreamId

    CUDA stream id Valid only if deviceType is acc_device_nvidia.

  uint32_t cuProcessId

    The ID of the process where the OpenACC activity is executing.

  uint32_t cuThreadId

    The ID of the thread where the OpenACC activity is executing.

  uint32_t externalId

    The OpenACC correlation ID.

    Valid only if deviceType is acc_device_nvidia. If not 0, it uniquely identifies this record. It is identical to the externalId in the preceding external correlation record of type CUPTI_EXTERNAL_CORRELATION_KIND_OPENACC.