# Sanitizer Patching API

## Typedefs
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackAsyncReduction )(void *userdata, uint64_t pc, uint32_t address, uint32_t mbarAddress, uint32_t accessSize)
| Function type for an asynchronous reduction operation on shared memory.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackAsyncStore )(void *userdata, uint64_t pc, uint32_t address, uint32_t mbarAddress, void *pNewValue, uint32_t accessSize)
| Function type for an asynchronous store operation on shared memory.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackBarrier )(void *userdata, uint64_t pc, uint32_t barIndex, uint32_t threadCount, uint32_t flags)
| Function type for a barrier callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackBlockEnter )(void *userdata, uint64_t pc)
| Function type for a CUDA block enter callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackBlockExit )(void *userdata, uint64_t pc)
| Function type for a CUDA block exit callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackCacheControl )(void *userdata, uint64_t pc, void *address, Sanitizer_CacheControlInstructionKind kind)
| Function type for a cache control instruction callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackCall )(void *userdata, uint64_t pc, uint64_t targetPc, uint32_t flags)
| Function type for a function call callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackClusterBarrierArrive )(void *userdata, uint64_t pc)
| Function type for a cluster barrier arrive.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackCudaBarrier )(void *userdata, uint64_t pc, void *barrier, uint32_t kind, uint32_t data)
| Function type for a CUDA Barrier action callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackDeviceSideFree )(void *userdata, uint64_t pc, void *ptr)
| Function type for a device-side free call.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackDeviceSideMalloc )(void *userdata, uint64_t pc, void *allocatedPtr, uint64_t allocatedSize)
| Function type for a device-side malloc call.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackMatrixMemoryAccess )(void *userdata, uint64_t pc, uint32_t address, uint32_t accessSize, uint32_t flags, uint32_t count, const void *pNewValue)
| Function type for a matrix shared memory access callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackMemcpyAsync )(void *userdata, uint64_t pc, void *src, uint32_t dst, uint32_t accessSize)
| Function type for a global to shared memory asynchronous copy.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackMemoryAccess )(void *userdata, uint64_t pc, void *ptr, uint32_t accessSize, uint32_t flags, const void *pData)
| Function type for a memory access callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackPipelineCommit )(void *userdata, uint64_t pc)
| Function type for a pipeline commit.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackPipelineWait )(void *userdata, uint64_t pc, uint32_t groups)
| Function type for a pipeline wait.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackRet )(void *userdata, uint64_t pc)
| Function type for a function return callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackSetSmemSize )(void *userdata, uint64_t pc, uint32_t size)
| Function type for setting the shared memory size allocated to a block.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackShfl )(void *userdata, uint64_t pc)
| Function type for a shfl callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackSyncwarp )(void *userdata, uint64_t pc, uint32_t mask)
| Function type for a syncwarp callback.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackWarpgroupFence )(void *userdata, uint64_t pc, uint32_t warpMask)
| Function type for a warpgroup MMA fence.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackWarpgroupMMAAsync )(void *userdata, uint64_t pc, uint32_t addressMatrixA, uint32_t sizeMatrixA, uint32_t addressMatrixB, uint32_t sizeMatrixB, uint32_t flags, uint32_t warpMask)
| Function type for a warpgroup aligned async MMA.
typedef SanitizerPatchResult(SANITIZERAPI * | SanitizerCallbackWarpgroupWaitGroup )(void *userdata, uint64_t pc, uint32_t numGroups, uint32_t warpMask)
| Function type for a warpgroup MMA wait group.
## Enumerations
enum | Sanitizer_BarrierFlags { SANITIZER_BARRIER_FLAG_NONE = 0, SANITIZER_BARRIER_FLAG_UNALIGNED_ALLOWED = 0x1 }
| Flags describing a barrier. More...
enum | Sanitizer_CacheControlInstructionKind { SANITIZER_CACHE_CONTROL_INVALID = 0, SANITIZER_CACHE_CONTROL_L1_PREFETCH = 1, SANITIZER_CACHE_CONTROL_L2_PREFETCH = 2 }
| Cache control action. More...
enum | Sanitizer_CallFlags { SANITIZER_CALL_FLAG_NONE = 0, SANITIZER_CALL_FLAG_UNALIGNED_ALLOWED = 0x1 }
| Flags describing a function call. More...
enum | Sanitizer_CudaBarrierInstructionKind { SANITIZER_CUDA_BARRIER_INVALID = 0, SANITIZER_CUDA_BARRIER_INIT = 1, SANITIZER_CUDA_BARRIER_ARRIVE = 2, SANITIZER_CUDA_BARRIER_ARRIVE_DROP = 3, SANITIZER_CUDA_BARRIER_ARRIVE_NOCOMPLETE = 4, SANITIZER_CUDA_BARRIER_ARRIVE_DROP_NOCOMPLETE = 5, SANITIZER_CUDA_BARRIER_WAIT = 6, SANITIZER_CUDA_BARRIER_INVALIDATE = 7 }
| CUDA Barrier action kind. More...
enum | Sanitizer_DeviceMemoryFlags { SANITIZER_MEMORY_DEVICE_FLAG_NONE = 0, SANITIZER_MEMORY_DEVICE_FLAG_READ = 0x1, SANITIZER_MEMORY_DEVICE_FLAG_WRITE = 0x2, SANITIZER_MEMORY_DEVICE_FLAG_ATOMSYS = 0x4, SANITIZER_MEMORY_DEVICE_FLAG_PREFETCH = 0x8 }
| Flags describing a memory access. More...
enum | Sanitizer_FunctionLoadedStatus { SANITIZER_FUNCTION_NOT_LOADED = 0x0, SANITIZER_FUNCTION_PARTIALLY_LOADED = 0x1, SANITIZER_FUNCTION_LOADED = 0x2 }
enum | Sanitizer_InstructionId { SANITIZER_INSTRUCTION_INVALID = 0, SANITIZER_INSTRUCTION_BLOCK_ENTER = 1, SANITIZER_INSTRUCTION_BLOCK_EXIT = 2, SANITIZER_INSTRUCTION_GLOBAL_MEMORY_ACCESS = 3, SANITIZER_INSTRUCTION_SHARED_MEMORY_ACCESS = 4, SANITIZER_INSTRUCTION_LOCAL_MEMORY_ACCESS = 5, SANITIZER_INSTRUCTION_BARRIER = 6, SANITIZER_INSTRUCTION_SYNCWARP = 7, SANITIZER_INSTRUCTION_SHFL = 8, SANITIZER_INSTRUCTION_CALL = 9, SANITIZER_INSTRUCTION_RET = 10, SANITIZER_INSTRUCTION_DEVICE_SIDE_MALLOC = 11, SANITIZER_INSTRUCTION_DEVICE_SIDE_FREE = 12, SANITIZER_INSTRUCTION_CUDA_BARRIER = 13, SANITIZER_INSTRUCTION_MEMCPY_ASYNC = 14, SANITIZER_INSTRUCTION_PIPELINE_COMMIT = 15, SANITIZER_INSTRUCTION_PIPELINE_WAIT = 16, SANITIZER_INSTRUCTION_REMOTE_SHARED_MEMORY_ACCESS = 17, SANITIZER_INSTRUCTION_DEVICE_ALIGNED_MALLOC = 18, SANITIZER_INSTRUCTION_MATRIX_MEMORY_ACCESS = 19, SANITIZER_INSTRUCTION_CACHE_CONTROL = 20, SANITIZER_INSTRUCTION_CLUSTER_BARRIER_ARRIVE = 21, SANITIZER_INSTRUCTION_CLUSTER_BARRIER_WAIT = 22, SANITIZER_INSTRUCTION_WARPGROUP_MMA_ASYNC = 23, SANITIZER_INSTRUCTION_WARPGROUP_WAIT_GROUP = 24, SANITIZER_INSTRUCTION_WARPGROUP_FENCE = 25, SANITIZER_INSTRUCTION_ASYNC_STORE = 26, SANITIZER_INSTRUCTION_ASYNC_REDUCTION = 27, SANITIZER_INSTRUCTION_SET_SHARED_MEMORY_SIZE = 28, SANITIZER_INSTRUCTION_BARRIER_RELEASE = 29 }
| Instrumentation. More...
enum | Sanitizer_WarpgroupMMAAsyncFlags { SANITIZER_WARPGROUP_MMA_ASYNC_FLAG_NONE = 0, SANITIZER_WARPGROUP_MMA_ASYNC_FLAG_COMMIT_GROUP = 0x1 }
| Flags describing a warpgroup aligned MMA async. More...
enum | SanitizerPatchResult { SANITIZER_PATCH_SUCCESS = 0, SANITIZER_PATCH_ERROR = 1 }
| Sanitizer patch result codes. More...
## Functions
SanitizerResult SANITIZERAPI | sanitizerAddPatches (const void *image, CUcontext ctx)
| Load a module containing patches that can be used by the patching API.
SanitizerResult SANITIZERAPI | sanitizerAddPatchesFromFile (const char *filename, CUcontext ctx)
| Load a module containing patches that can be used by the patching API.
SanitizerResult SANITIZERAPI | sanitizerGetCallbackPcAndSize (CUcontext ctx, const char *deviceCallbackName, uint64_t *pc, uint64_t *size)
| Get PC and size of a device callback.
SanitizerResult SANITIZERAPI | sanitizerGetFunctionLoadedStatus (CUfunction func, Sanitizer_FunctionLoadedStatus *loadingStatus)
| Get the loading status of a function. Requires a driver version >=515.
SanitizerResult SANITIZERAPI | sanitizerGetFunctionPcAndSize (CUmodule module, const char *functionName, uint64_t *pc, uint64_t *size)
| Get PC and size of a CUDA function.
SanitizerResult SANITIZERAPI | sanitizerPatchInstructions (const Sanitizer_InstructionId instructionId, CUmodule module, const char *deviceCallbackName)
| Set instrumentation points and patches to be applied in a module.
SanitizerResult SANITIZERAPI | sanitizerPatchModule (CUmodule module)
| Perform the actual instrumentation of a module.
SanitizerResult SANITIZERAPI | sanitizerSetCallbackData (CUfunction kernel, const void *userdata)
| Specifies the user data pointer for callbacks.
SanitizerResult SANITIZERAPI | sanitizerSetDeviceGraphData (CUgraphExec graphExec, Sanitizer_StreamHandle stream, const void *userdata)
| Specifies the user data pointer accessible from callbacks in the device-launched graphs launched by the specified host-launched graphExec.
SanitizerResult SANITIZERAPI | sanitizerSetLaunchCallbackData (Sanitizer_LaunchHandle launch, CUfunction kernel, Sanitizer_StreamHandle stream, const void *userdata)
| Specifies the user data pointer for callbacks.
SanitizerResult SANITIZERAPI | sanitizerUnpatchModule (CUmodule module)
| Remove existing instrumentation of a module.

## Detailed Description

Functions, types, and enums that implement the Sanitizer Patching API.

## Typedef Documentation

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackAsyncReduction)(void *userdata, uint64_t pc, uint32_t address, uint32_t mbarAddress, uint32_t accessSize)

This can be generated by a red.async PTX instruction

`userdata` is a pointer to user data. See sanitizerPatchModule. `pc` is the program counter of the patched instruction. `address` is the destination address in shared memory. `mbarAddress` is the address of the mbarrier object. `accessSize` is the size of the access in bytes. Valid values are 4 and 8.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackAsyncStore)(void *userdata, uint64_t pc, uint32_t address, uint32_t mbarAddress, void *pNewValue, uint32_t accessSize)

This can be generated by a st.async PTX instruction

`userdata` is a pointer to user data. See sanitizerPatchModule. `pc` is the program counter of the patched instruction. `address` is the destination address in shared memory. `mbarAddress` is the address of the mbarrier object. `pNewValue` is a pointer to the new value being written. `accessSize` is the size of the access in bytes. Valid values are 4 and 8.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackBarrier)(void *userdata, uint64_t pc, uint32_t barIndex, uint32_t threadCount, uint32_t flags)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `barIndex` is the barrier index. `threadCount` is the number of expected threads (must be a multiple of the warp size). `flags` contains information about the barrier. See Sanitizer_BarrierFlags to interpret this value. 0 means that all threads are participating in the barrier.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackBlockEnter)(void *userdata, uint64_t pc)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the entry point of the block

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackBlockExit)(void *userdata, uint64_t pc)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

typedef SanitizerPatchResult(SANITIZERAPI* SanitizerCallbackCacheControl)(void *userdata, uint64_t pc, void *address, Sanitizer_CacheControlInstructionKind kind)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `address` is the address of the memory being controlled `kind` is the type of cache control. See Sanitizer_CacheControlInstructionKind

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackCall)(void *userdata, uint64_t pc, uint64_t targetPc, uint32_t flags)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `targetPc` is the PC where the called function is located. `flags` contains information about the function call.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackClusterBarrierArrive)(void *userdata, uint64_t pc)

Function type for a cluster barrier wait.

This can be generated by a cg::this_cluster().sync() (C++ API), or a barrier.cluster.arrive (PTX API).

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

This can be generated by a cg::this_cluster().sync() (C++ API), or a barrier.cluster.wait (PTX API).

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackCudaBarrier)(void *userdata, uint64_t pc, void *barrier, uint32_t kind, uint32_t data)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `barrier` Barrier address which can be used as a unique identifier `kind` Barrier action type. See Sanitizer_CudaBarrierInstructionKind `data` Barrier data. This is specific to each action type, refer to Sanitizer_CudaBarrierInstructionKind

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackDeviceSideFree)(void *userdata, uint64_t pc, void *ptr)

Note:
  This is called prior to the actual call.

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `ptr` is the pointer passed to device-side free.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackDeviceSideMalloc)(void *userdata, uint64_t pc, void *allocatedPtr, uint64_t allocatedSize)

Note:
  This is called after the call has completed.

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `allocatedPtr` is the pointer returned by device-side malloc `allocatedSize` is the size requested by the user to device-side malloc.

typedef SanitizerPatchResult(SANITIZERAPI* SanitizerCallbackMatrixMemoryAccess)(void *userdata, uint64_t pc, uint32_t address, uint32_t accessSize, uint32_t flags, uint32_t count, const void *pNewValue)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `address` is the address of the shared memory being read or written. This is an offset within the shared memory window `accessSize` is the size of the access in bytes. Valid value is 16. `flags` contains information about the type of access. See Sanitizer_DeviceMemoryFlags to interpret this value. `count` is the number of matrices accessed. `pNewValue` is a pointer to the new value being written if the access is a write. If the access is a read or an atomic, the pointer will be NULL.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackMemcpyAsync)(void *userdata, uint64_t pc, void *src, uint32_t dst, uint32_t accessSize)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `src` is the address of the global memory being read. This can be NULL if src-size is 0. `dst` is the address of the shared memory being written. This is an offset within the shared memory window `accessSize` is the size of the access in bytes. Valid values are 4, 8 and 16.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackMemoryAccess)(void *userdata, uint64_t pc, void *ptr, uint32_t accessSize, uint32_t flags, const void *pData)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `ptr` is the address of the memory being accessed. For local or shared memory access, this is the offset within the local or shared memory window. `accessSize` is the size of the access in bytes. Valid values are 1, 2, 4, 8, and 16. `flags` contains information about the type of access. See Sanitizer_DeviceMemoryFlags to interpret this value. `pData` is a pointer which value depends on the type of access:

- If the access is a write, `pData` points to the new value being written.
- If the access is a read and `pData` is not `NULL`, then it points to a 32-bit mask of loaded bytes being used (padding bytes will not appear).
- If the access is an atomic, the pointer will be `NULL`.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackPipelineCommit)(void *userdata, uint64_t pc)

This can be generated by a pipeline::producer_commit (C++ API), a pipeline_commit (C API) or a cp.async.commit_group (PTX API).

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackPipelineWait)(void *userdata, uint64_t pc, uint32_t groups)

This can be generated by a pipeline::consumer_wait (C++ API), a pipeline_wait_prior (C API), cp.async.wait_group or cp.async.wait_all (PTX API).

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `groups` is the number of groups the pipeline will wait for. 0 is used to wait for all groups.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackRet)(void *userdata, uint64_t pc)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackSetSmemSize)(void *userdata, uint64_t pc, uint32_t size)

This can be generated by a setsmemsize.sync instruction

`userdata` is a pointer to user data. See sanitizerPatchModule. `pc` is the program counter of the patched instruction. `size` is the requested size in bytes.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackShfl)(void *userdata, uint64_t pc)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackSyncwarp)(void *userdata, uint64_t pc, uint32_t mask)

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `mask` is the thread mask passed to __syncwarp().

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackWarpgroupFence)(void *userdata, uint64_t pc, uint32_t warpMask)

This can be generated by a wgmma.fence in PTX.

`userdata` is a pointer to user data. See sanitizerPatchModule. `pc` is the program counter of the patched instruction. `warpMask` is a mask of threads that will perform the fence operation. Expected values are either 0x0 or 0xffffffff (full). The value is expected to be the same across the warpgroup. Other values can be reported but signal a programming error in the target application.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackWarpgroupMMAAsync)(void *userdata, uint64_t pc, uint32_t addressMatrixA, uint32_t sizeMatrixA, uint32_t addressMatrixB, uint32_t sizeMatrixB, uint32_t flags, uint32_t warpMask)

This can be generated by a wgmma.mma_async in PTX.

`userdata` is a pointer to user data. See sanitizerPatchModule `pc` is the program counter of the patched instruction `addressMatrixA` is the address in shared memory of the matrix A being read. This field is only valid if sizeMatrixA is non-zero and warpMask is full. `sizeMatrixA` is the size of the matrix A in shared memory. A value of 0 means that the matrix A is read from registers instead. `addressMatrixB` is the address in shared memory of the matrix B being read. This field is only valid if warpMask is full. `sizeMatrixB` is the size of the matrix B in shared memory. The value will always be non-zero. `flags` of type Sanitizer_WarpgroupMMAAsyncFlags provide information about the access. These flags are to be taken into account even if the warpMask is zero. `warpMask` is a mask of threads that will perform the operation and read the operands. Expected values are either 0x0 or 0xffffffff (full). The value is expected to be the same across the warpgroup. Other values can be reported but signal a programming error in the target application.

typedef SanitizerPatchResult(SANITIZERAPI * SanitizerCallbackWarpgroupWaitGroup)(void *userdata, uint64_t pc, uint32_t numGroups, uint32_t warpMask)

This can be generated by a wgmma.wait_group in PTX.

`userdata` is a pointer to user data. See sanitizerPatchModule. `pc` is the program counter of the patched instruction. `numGroups` is the maximum number of group that will be left pending after the operation. A value of zero means that all MMA async of the warpgroup are guaranteed to have completed after the operation. `warpMask` is a mask of threads for which the expected values are either 0x0 or 0xffffffff (full). The value is expected to be the same across the warpgroup. Other values can be reported but signal a programming error in the target application. If the value is valid, the value has no influence on the operation.

## Enumeration Type Documentation

enum Sanitizer_BarrierFlags

Flags describing a barrier. These values are to be or-combined in the value of flags for a SanitizerCallbackBarrier callback.

Enumerator:

  SANITIZER_BARRIER_FLAG_NONE | Empty flag.
  SANITIZER_BARRIER_FLAG_UNALIGNED_ALLOWED | Specifies that the barrier can be called unaligned. This flag is only valid on SM 7.0 and above.

enum Sanitizer_CacheControlInstructionKind

Enumerator:

  SANITIZER_CACHE_CONTROL_INVALID | Invalid action ID.
  SANITIZER_CACHE_CONTROL_L1_PREFETCH | Prefetch to L1.
  SANITIZER_CACHE_CONTROL_L2_PREFETCH | Prefetch to L2.

enum Sanitizer_CallFlags

Flags describing a function call. These values are to be or-combined in the value of flags for a SanitizerCallbackCall callback.

Enumerator:

  SANITIZER_CALL_FLAG_NONE | Empty flag.
  SANITIZER_CALL_FLAG_UNALIGNED_ALLOWED | Specifies that barriers within this function call can be called unaligned. This flag is only valid on SM 7.0 and above.

enum Sanitizer_CudaBarrierInstructionKind

Refer to the CUDA Barrier interface section of the CUDA toolkit documentation for a more extensive description of these actions.

Enumerator:

  SANITIZER_CUDA_BARRIER_INVALID | Invalid action ID.
  SANITIZER_CUDA_BARRIER_INIT | Barrier initialization.
  SANITIZER_CUDA_BARRIER_ARRIVE | Barrier arrive operation. On Hopper and newer architectures, barrier data is the count argument to the arrive-on operation.
  SANITIZER_CUDA_BARRIER_ARRIVE_DROP | Barrier arrive and drop operation. On Hopper and newer architectures, barrier data is the count argument to the arrive-on operation.
  SANITIZER_CUDA_BARRIER_ARRIVE_NOCOMPLETE | Barrier arrive operation without phase completion. Barrier data is the count argument to the arrive-on operation.
  SANITIZER_CUDA_BARRIER_ARRIVE_DROP_NOCOMPLETE | Barrier arrive and drop operation without phase completion. Barrier data is the count argument to the arrive-on operation.
  SANITIZER_CUDA_BARRIER_WAIT | Barrier wait operation.
  SANITIZER_CUDA_BARRIER_INVALIDATE | Barrier invalidation.

enum Sanitizer_DeviceMemoryFlags

Flags describing a memory access. These values are to be or-combined in the value of flags for a SanitizerCallbackMemoryAccess callback.

Enumerator:

  SANITIZER_MEMORY_DEVICE_FLAG_NONE | Empty flag.
  SANITIZER_MEMORY_DEVICE_FLAG_READ | Specifies that the access is a read.
  SANITIZER_MEMORY_DEVICE_FLAG_WRITE | Specifies that the access is a write.
  SANITIZER_MEMORY_DEVICE_FLAG_ATOMSYS | Specifies that the access is a system-scoped atomic.
  SANITIZER_MEMORY_DEVICE_FLAG_PREFETCH | Specifies that the access is a cache prefetch.

enum Sanitizer_FunctionLoadedStatus

Enumerator:

  SANITIZER_FUNCTION_NOT_LOADED | The function is not loaded.
  SANITIZER_FUNCTION_PARTIALLY_LOADED | The function is being loaded.
  SANITIZER_FUNCTION_LOADED | The function is fully loaded.

enum Sanitizer_InstructionId

Instrumentation. Every entry represent an instruction type or a function call where a callback patch can be inserted.

Enumerator:

  SANITIZER_INSTRUCTION_INVALID | Invalid instruction ID.
  SANITIZER_INSTRUCTION_BLOCK_ENTER | CUDA block enter. This is called prior to any user code. The type of the callback must be SanitizerCallbackBlockEnter.
  SANITIZER_INSTRUCTION_BLOCK_EXIT | CUDA block exit. This is called after all user code has executed. The type of the callback must be SanitizerCallbackBlockExit.
  SANITIZER_INSTRUCTION_GLOBAL_MEMORY_ACCESS | Global Memory Access. This can be a store, load or atomic operation. The type of the callback must be SanitizerCallbackMemoryAccess.
  SANITIZER_INSTRUCTION_SHARED_MEMORY_ACCESS | Shared Memory Access. This can be a store, load or atomic operation. The type of the callback must be SanitizerCallbackMemoryAccess.
  SANITIZER_INSTRUCTION_LOCAL_MEMORY_ACCESS | Local Memory Access. This can be a store or load operation. The type of the callback must be SanitizerCallbackMemoryAccess.
  SANITIZER_INSTRUCTION_BARRIER | Barrier. The type of the callback must be SanitizerCallbackBarrier.
  SANITIZER_INSTRUCTION_SYNCWARP | Syncwarp. The type of the callback must be SanitizerCallbackSyncwarp.
  SANITIZER_INSTRUCTION_SHFL | Shfl. The type of the callback must be SanitizerCallbackShfl.
  SANITIZER_INSTRUCTION_CALL | Function call. The type of the callback must be SanitizerCallbackCall.
  SANITIZER_INSTRUCTION_RET | Function return. The type of the callback must be SanitizerCallbackRet.
  SANITIZER_INSTRUCTION_DEVICE_SIDE_MALLOC | Device-side malloc. The type of the callback must be SanitizerCallbackDeviceSideMalloc.
  SANITIZER_INSTRUCTION_DEVICE_SIDE_FREE | Device-side free. The type of the callback must be SanitizerCallbackDeviceSideFree.
  SANITIZER_INSTRUCTION_CUDA_BARRIER | CUDA Barrier operation. The type of the callback must be SanitizerCallbackCudaBarrier.
  SANITIZER_INSTRUCTION_MEMCPY_ASYNC | Global to shared memory asynchronous copy. The type of the callback must be SanitizerCallbackMemcpyAsync.
  SANITIZER_INSTRUCTION_PIPELINE_COMMIT | Pipeline commit. The type of the callback must be SanitizerCallbackPipelineCommit.
  SANITIZER_INSTRUCTION_PIPELINE_WAIT | Pipeline wait. The type of the callback must be SanitizerCallbackPipelineWait.
  SANITIZER_INSTRUCTION_REMOTE_SHARED_MEMORY_ACCESS | Remote Shared Memory Access. This can be a store or load operation. The type of the callback must be SanitizerCallbackMemoryAccess.
  SANITIZER_INSTRUCTION_DEVICE_ALIGNED_MALLOC | Device-side aligned malloc. The type of the callback must be SanitizerCallbackDeviceSideMalloc.
  SANITIZER_INSTRUCTION_MATRIX_MEMORY_ACCESS | Matrix shared memory access. The type of the callback must be SanitizerCallbackMatrixMemoryAccess.
  SANITIZER_INSTRUCTION_CACHE_CONTROL | Cache control instruction. The type of the callback must be SanitizerCallbackCacheControl.
  SANITIZER_INSTRUCTION_CLUSTER_BARRIER_ARRIVE | Cluster barrier arrive instruction. The type of the callback must be SanitizerCallbackClusterBarrierArrive.
  SANITIZER_INSTRUCTION_CLUSTER_BARRIER_WAIT | Cluster barrier wait instruction. The type of the callback must be SanitizerCallbackClusterBarrierWait.
  SANITIZER_INSTRUCTION_WARPGROUP_MMA_ASYNC | Warpgroup aligned async MMA instruction. The type of the callback must be SanitizerCallbackWarpgroupMMAAsync.
  SANITIZER_INSTRUCTION_WARPGROUP_WAIT_GROUP | Warpgroup wait MMA group instruction. The type of the callback must be SanitizerCallbackWarpgroupWaitGroup.
  SANITIZER_INSTRUCTION_WARPGROUP_FENCE | Warpgroup fence instruction. The type of the callback must be SanitizerCallbackWarpgroupFence.
  SANITIZER_INSTRUCTION_ASYNC_STORE | Asynchronous store instruction. The type of the callback must be SanitizerCallbackAsyncStore.
  SANITIZER_INSTRUCTION_ASYNC_REDUCTION | Asynchronous reduction instruction. The type of the callback must be SanitizerCallbackAsyncReduction.
  SANITIZER_INSTRUCTION_SET_SHARED_MEMORY_SIZE | Set the shared memory size allocated to a block instruction. The type of the callback must SanitizerCallbackSetSmemSize
  SANITIZER_INSTRUCTION_BARRIER_RELEASE | Barrier after it is released. The type of the callback must be SanitizerCallbackBarrier.

enum Sanitizer_WarpgroupMMAAsyncFlags

Flags describing a warpgroup aligned MMA async. These values are to be or-combined in the value of flags for a SanitizerCallbackWarpgroupMMAAsync callback.

Enumerator:

  SANITIZER_WARPGROUP_MMA_ASYNC_FLAG_NONE | Empty flag.
  SANITIZER_WARPGROUP_MMA_ASYNC_FLAG_COMMIT_GROUP | Specifies that the MMA async delimits a MMA async group of which it is the last instruction. Please refer to the PTX documentation for wgmma_async.commit_group for more details. This property is valid even if the warpMask is zero.

enum SanitizerPatchResult

Error and result codes returned by Sanitizer patches. If a patch returns SANITIZER_PATCH_ERROR, the thread will be exited. On Volta and newer architectures, the full warp which the thread belongs to will be exited.

Enumerator:

  SANITIZER_PATCH_SUCCESS | No error.
  SANITIZER_PATCH_ERROR | An error was detected in the patch.

## Function Documentation

SanitizerResult SANITIZERAPI sanitizerAddPatches | ( | const void * | image,
|  | CUcontext | ctx |
| ) |  |  |

Note:
  Thread-safety: an API user must serialize access to sanitizerAddPatchesFromFile, sanitizerAddPatches, sanitizerPatchInstructions, and sanitizerPatchModule. For example if sanitizerAddPatches(image) and sanitizerPatchInstruction(*, *, cbName) are called concurrently and cbName is intended to be found in the loaded image, the results are undefined.

  The patches loaded are only valid for the specified CUDA context.

Parameters:

  | image | Pointer to module data to load. This API supports the same module formats as the cuModuleLoadData and cuModuleLoadFatBinary functions from the CUDA driver API.
  | ctx | CUDA context in which to load the patches. If ctx is NULL, the current context will be used.

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_NOT_INITIALIZED | if unable to initialize the sanitizer
  | SANITIZER_ERROR_INVALID_PARAMETER | if `image` does not point to a valid CUDA module.

SanitizerResult SANITIZERAPI sanitizerAddPatchesFromFile | ( | const char * | filename,
|  | CUcontext | ctx |
| ) |  |  |

Note:
  Thread-safety: an API user must serialize access to sanitizerAddPatchesFromFile, sanitizerAddPatches, sanitizerPatchInstructions, and sanitizerPatchModule. For example if sanitizerAddPatchesFromFile(filename) and sanitizerPatchInstruction(*, *, cbName) are called concurrently and cbName is intended to be found in the loaded module, the results are undefined.

  The patches loaded are only valid for the specified CUDA context.

Parameters:

  | filename | Path to the module file. This API supports the same module formats as the cuModuleLoad function from the CUDA driver API.
  | ctx | CUDA context in which to load the patches. If ctx is NULL, the current context will be used.

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_NOT_INITIALIZED | if unable to initialize the sanitizer
  | SANITIZER_ERROR_INVALID_PARAMETER | if `filename` is not a path to a valid CUDA module.

SanitizerResult SANITIZERAPI sanitizerGetCallbackPcAndSize | ( | CUcontext | ctx,
|  | const char * | deviceCallbackName,
|  | uint64_t * | pc,
|  | uint64_t * | size |
| ) |  |  |

Parameters:

  `[in]` | ctx | CUDA context in which the patches were loaded. If ctx is NULL, the current context will be used.
  `[in]` | deviceCallbackName | device function callback name
  `[out]` | pc | Callback PC returned
  `[out]` | size | Callback size returned

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_INVALID_PARAMETER | if `deviceCallbackName` function cannot be located, if pc is NULL or if size is NULL.

SanitizerResult SANITIZERAPI sanitizerGetFunctionLoadedStatus | ( | CUfunction | func,
|  | Sanitizer_FunctionLoadedStatus * | loadingStatus |
| ) |  |  |

Parameters:

  `[in]` | func | CUDA function for which the loading status is queried.
  `[out]` | loadingStatus | Loading status returned

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_INVALID_PARAMETER | if `func` is NULL or if loadingStatus is NULL.
  | SANITIZER_ERROR_NOT_SUPPORTED | if the loading status cannot be queried with this driver version.

SanitizerResult SANITIZERAPI sanitizerGetFunctionPcAndSize | ( | CUmodule | module,
|  | const char * | functionName,
|  | uint64_t * | pc,
|  | uint64_t * | size |
| ) |  |  |

Parameters:

  `[in]` | module | CUDA module containing the function
  `[in]` | deviceCallbackName | CUDA function name
  `[out]` | pc | Function start program counter (PC) returned
  `[out]` | size | Function size in bytes returned

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_INVALID_PARAMETER | if `functionName` function cannot be located, if pc is NULL or if size is NULL.

SanitizerResult SANITIZERAPI sanitizerPatchInstructions | ( | const Sanitizer_InstructionId | instructionId,
|  | CUmodule | module,
|  | const char * | deviceCallbackName |
| ) |  |  |

Mark that all instrumentation points matching instructionId are to be patched in order to call the device function identified by deviceCallbackName. It is up to the API client to ensure that this device callback exists and match the correct callback format for this instrumentation point.

Note:
  Thread-safety: an API user must serialize access to sanitizerAddPatchesFromFile, sanitizerAddPatches, sanitizerPatchInstructions, and sanitizerPatchModule. For example if sanitizerAddPatches(fileName) and sanitizerPatchInstruction(*, *, cbName) are called concurrently and cbName is intended to be found in the loaded module, the results are undefined.

Parameters:

  | instructionId | Instrumentation point for which to insert patches
  | module | CUDA module to instrument
  | deviceCallbackName | Name of the device function callback that the inserted patch will call at the instrumented points. This function is expected to be found in code previously loaded by sanitizerAddPatchesFromFile or sanitizerAddPatches.

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_NOT_INITIALIZED | if unable to initialize the sanitizer
  | SANITIZER_ERROR_INVALID_PARAMETER | if `module` is not a CUDA module or if `deviceCallbackName` function cannot be located.

SanitizerResult SANITIZERAPI sanitizerPatchModule | ( | CUmodule | module | ) |

Perform the instrumentation of a CUDA module based on previous calls to sanitizerPatchInstructions. This function also specifies the device memory buffer to be passed in as userdata to all callback functions.

Note:
  Thread-safety: an API user must serialize access to sanitizerAddPatchesFromFile, sanitizerAddPatches, sanitizerPatchInstructions, and sanitizerPatchModule. For example if sanitizerPatchModule(mod, *) and sanitizerPatchInstruction(*, mod, *) are called concurrently, the results are undefined.

Parameters:

  | module | CUDA module to instrument

Return values:

  | SANITIZER_SUCCESS | on success
  | SANITIZER_ERROR_INVALID_PARAMETER | if `module` is not a CUDA module

SanitizerResult SANITIZERAPI sanitizerSetCallbackData | ( | CUfunction | kernel,
|  | const void * | userdata |
| ) |  |  |

Mark all subsequent launches of `kernel` to use `userdata` pointer as the device memory buffer to pass in to callback functions.

Parameters:

  | kernel | CUDA function to link to user data. Callbacks in subsequent launches on this kernel will use `userdata` as callback data.
  | userdata | Device memory buffer. This data will be passed to callback functions via the `userdata` parameter.

Return values:

  | SANITIZER_SUCCESS | on success

SanitizerResult SANITIZERAPI sanitizerSetDeviceGraphData | ( | CUgraphExec | graphExec,
|  | Sanitizer_StreamHandle | stream,
|  | const void * | userdata |
| ) |  |  |

Mark all subsequent launch of `graphExec` to make available `userdata` in device callbacks from device-launched graphs. `userdata` will not be set in the callback userdata parameter but must be accessed through another mean instead. Please refer to the Sanitizer API reference manual. This function is only available if the driver version is 535 or newer.

Parameters:

  | graphExec | CUDA graphExec that will launch CUDA graphs from the device.
  | stream | CUDA stream associated with the stream launch.
  | userdata | Device memory buffer.

Return values:

  | SANITIZER_SUCCESS | on success

SanitizerResult SANITIZERAPI sanitizerSetLaunchCallbackData | ( | Sanitizer_LaunchHandle | launch,
|  | CUfunction | kernel,
|  | Sanitizer_StreamHandle | stream,
|  | const void * | userdata |
| ) |  |  |

Mark `launch` to use `userdata` pointer as the device memory buffer to pass in to callback functions. This function is only available if the driver version is 455 or newer.

Parameters:

  | launch | Kernel launch to link to user data. Callbacks in this kernel launch will use `userdata` as callback data.
  | kernel | CUDA function associated with the kernel launch.
  | stream | CUDA stream associated with the stream launch.
  | userdata | Device memory buffer. This data will be passed to callback functions via the `userdata` parameter.

Return values:

  | SANITIZER_SUCCESS | on success

SanitizerResult SANITIZERAPI sanitizerUnpatchModule | ( | CUmodule | module | ) |

Remove any instrumentation of a CUDA module performed by previous calls to sanitizerPatchModule.

Note:
  Thread-safety: an API user must serialize access to sanitizerPatchModule and sanitizerUnpatchModule on the same module. For example, if sanitizerPatchModule(mod) and sanitizerUnpatchModule(mod) are called concurrently, the results are undefined.

Parameters:

  | module | CUDA module on which to remove instrumentation

Return values:

  | SANITIZER_SUCCESS | on success