Skip to main content
`Ctrl`+`K`

# 7.63. CUpti_ActivityMemDecompress

struct CUpti_ActivityMemDecompress

  The activity record for trace of decompression operations.

  This activity record represents execution for a batch of decompression operatios. The activity kind is CUPTI_ACTIVITY_KIND_MEM_DECOMPRESS

  Public Members

  CUpti_ActivityKind kind

    The activity record kind, must be CUPTI_ACTIVITY_KIND_MEM_DECOMPRESS.

  uint32_t deviceId

    The ID of the device.

  uint32_t contextId

    The ID of the context.

  uint32_t streamId

    The ID of the stream.

  uint32_t channelID

    The ID of the HW channel on which the memory copy is occurring.

  CUpti_ChannelType channelType

    The type of the channel.

  uint32_t correlationId

    The correlation ID of the decompression operations.

    Each operation is assigned a unique correlation ID that is identical to the correlation ID in the driver API activity record that launched the operation.

  uint32_t numberOfOperations

    The number of operations in the batch.

  uint64_t sourceBytes

    The number of bytes to be read and decompressed in the batch operation.

  void *reserved0

    This field is reserved for internal use.

  uint64_t start

    The start timestamp.

    A value of CUPTI_TIMESTAMP_UNKNOWN indicates that the start time is unknown.

  uint64_t end

    The end timestamp.

    A value of CUPTI_TIMESTAMP_UNKNOWN indicates that the start time is unknown.