Skip to main content
`Ctrl`+`K`

# 8.1.1.6. CUptiUtil_PutPcSampDataParams

Fully qualified name: `CUPTI::PcSamplingUtil::CUptiUtil_PutPcSampDataParams`

struct CUptiUtil_PutPcSampDataParams

  Params for CuptiUtilPutPcSampData.

  Public Members

  size_t size

    Size of the data structure i.e.

    CUpti_PCSamplingDisableParamsSize CUPTI client should set the size of the structure. It will be used in CUPTI to check what fields are available in the structure. Used to preserve backward compatibility.

  PcSamplingBufferType bufferType

    Type of buffer to store in file.

  void *pSamplingData

    PC sampling buffer.

  size_t numAttributes

    Number of configured attributes.

  CUpti_PCSamplingConfigurationInfo *pPCSamplingConfigurationInfo

    Refer CUpti_PCSamplingConfigurationInfo It is expected to provide configuration details of at least CUPTI_PC_SAMPLING_CONFIGURATION_ATTR_TYPE_STALL_REASON attribute.

  PcSamplingStallReasons *pPcSamplingStallReasons

    Refer PcSamplingStallReasons.

  const char *fileName

    File name to store buffer into it.